From 4d6bfb6fbb00af38402db4d1ce464e22def9fd9e Mon Sep 17 00:00:00 2001
From: Russell King <rmk+kernel@armlinux.org.uk>
Date: Thu, 28 Nov 2019 14:24:40 +0000
Subject: [PATCH 1/4] net: sfp: use a definition for the fault recovery
 attempts

Signed-off-by: Russell King <rmk+kernel@armlinux.org.uk>
---
 drivers/net/phy/sfp.c | 14 +++++++++++---
 1 file changed, 11 insertions(+), 3 deletions(-)

--- a/drivers/net/phy/sfp.c
+++ b/drivers/net/phy/sfp.c
@@ -172,6 +172,14 @@ static const enum gpiod_flags gpio_flags
 #define T_RESET_US		10
 #define T_FAULT_RECOVER		msecs_to_jiffies(1000)
 
+/* N_FAULT_INIT is the number of recovery attempts at module initialisation
+ * time. If the TX_FAULT signal is not deasserted after this number of
+ * attempts at clearing it, we decide that the module is faulty.
+ * N_FAULT is the same but after the module has initialised.
+ */
+#define N_FAULT_INIT		5
+#define N_FAULT			5
+
 /* SFP module presence detection is poor: the three MOD DEF signals are
  * the same length on the PCB, which means it's possible for MOD DEF 0 to
  * connect before the I2C bus on MOD DEF 1/2.
@@ -1980,7 +1988,7 @@ static void sfp_sm_main(struct sfp *sfp,
 		sfp_module_tx_enable(sfp);
 
 		/* Initialise the fault clearance retries */
-		sfp->sm_retries = 5;
+		sfp->sm_retries = N_FAULT_INIT;
 
 		/* We need to check the TX_FAULT state, which is not defined
 		 * while TX_DISABLE is asserted. The earliest we want to do
@@ -2020,7 +2028,7 @@ static void sfp_sm_main(struct sfp *sfp,
 			 * or t_start_up, so assume there is a fault.
 			 */
 			sfp_sm_fault(sfp, SFP_S_INIT_TX_FAULT,
-				     sfp->sm_retries == 5);
+				     sfp->sm_retries == N_FAULT_INIT);
 		} else if (event == SFP_E_TIMEOUT || event == SFP_E_TX_CLEAR) {
 	init_done:	/* TX_FAULT deasserted or we timed out with TX_FAULT
 			 * clear.  Probe for the PHY and check the LOS state.
@@ -2033,7 +2041,7 @@ static void sfp_sm_main(struct sfp *sfp,
 			sfp_sm_link_check_los(sfp);
 
 			/* Reset the fault retry count */
-			sfp->sm_retries = 5;
+			sfp->sm_retries = N_FAULT;
 		}
 		break;
 
