From b058c3c898472ad8799bba29365c3295fdd24970 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Wed, 29 Jan 2020 14:32:51 +0000
Subject: [PATCH] overlays: Correct the eth_led* colour assignments

See: https://github.com/raspberrypi/firmware/issues/1311

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 arch/arm/boot/dts/overlays/README | 17 +++++++++--------
 1 file changed, 9 insertions(+), 8 deletions(-)

--- a/arch/arm/boot/dts/overlays/README
+++ b/arch/arm/boot/dts/overlays/README
@@ -109,27 +109,28 @@ Params:
                                 Legal values are 2, 3, 4, 5 and 0, where
                                 0 means never downshift (default 2). Pi3B+ only.
 
-        eth_led0                Set mode of LED0 (usually orange). The legal
-                                values are:
+        eth_led0                Set mode of LED0 - amber on Pi3B+ (default "1"),
+                                green on Pi4 (default "0").
+                                The legal values are:
 
                                 Pi3B+
 
-                                0=link/activity    1=link1000/activity (default)
+                                0=link/activity          1=link1000/activity
                                 2=link100/activity       3=link10/activity
                                 4=link100/1000/activity  5=link10/1000/activity
                                 6=link10/100/activity    14=off    15=on
 
                                 Pi4
 
-                                0=Speed/Activity (default)       1=Speed
-                                2=Speed/Flash activity   3=FDX
+                                0=Speed/Activity         1=Speed
+                                2=Flash activity         3=FDX
                                 4=Off                    5=On
                                 6=Alt                    7=Speed/Flash
                                 8=Link                   9=Activity
 
-        eth_led1                Set mode of LED1 (usually green) (Pi3B+ default
-                                "6", Pi4 default "8"). See eth_led0 for legal
-                                values.
+        eth_led1                Set mode of LED1 - green on Pi3B (default "6"),
+                                amber on Pi4 (default "8"). See eth_led0 for
+                                legal values.
 
         eth_max_speed           Set the maximum speed a link is allowed
                                 to negotiate. Legal values are 10, 100 and
