#include "rt5350.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "wiznet,wizfi630a", "ralink,rt5350-soc";
	model = "WIZnet WizFi630A";

	aliases {
		led-boot = &led_run;
		led-failsafe = &led_run;
		led-running = &led_run;
		led-upgrade = &led_run;
	};

	chosen {
		bootargs = "console=ttyS1,115200";
	};

	leds {
		compatible = "gpio-leds";

		led_run: run {
			label = ":run";
			gpios = <&gpio0 1 GPIO_ACTIVE_LOW>;
		};

		wps {
			label = ":wps";
			gpios = <&gpio0 20 GPIO_ACTIVE_LOW>;
		};

		uart1 {
			label = ":uart1";
			gpios = <&gpio0 18 GPIO_ACTIVE_LOW>;
		};

		uart2 {
			label = ":uart2";
			gpios = <&gpio0 21 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;

		reset {
			label = "reset";
			gpios = <&gpio0 17 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio0 0 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		scm1 {
			label = "SCM1";
			gpios = <&gpio0 19 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_0>;
		};

		scm2 {
			label = "SCM2";
			gpios = <&gpio0 2 GPIO_ACTIVE_LOW>;
			linux,code = <BTN_1>;
		};
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				#size-cells = <1>;
				label = "uboot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				#size-cells = <1>;
				label = "uboot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				#size-cells = <1>;
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				#size-cells = <1>;
				label = "firmware";
				reg = <0x50000 0xfb0000>;
			};
		};
	};
};

&uart {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&uartf_pins>;
};

&state_default {
	gpio {
		groups = "i2c", "jtag" ;
		function = "gpio";
	};
};

&ethernet {
	mtd-mac-address = <&factory 0x4>;
};

&esw {
	mediatek,portmap = <0x17>;
};

&wmac {
	ralink,mtd-eeprom = <&factory 0x0>;
};
