From 0c7e3f6f557c2a68527980e940e6a605da1f9e12 Mon Sep 17 00:00:00 2001
From: Ran Wang <ran.wang_1@nxp.com>
Date: Wed, 16 Jan 2019 15:40:33 +0800
Subject: [PATCH] arm64: dts: Fix DWC3 IP VBUS glitch issue on Layerscape
 platforms

Cover LS1012A, LS1043A, LS1046A, LS1088A, LS208xA, LX2160A

Signed-off-by: Ran Wang <ran.wang_1@nxp.com>
---
 arch/arm64/boot/dts/freescale/fsl-ls1012a.dtsi | 1 +
 arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi | 3 +++
 arch/arm64/boot/dts/freescale/fsl-ls1046a.dtsi | 3 +++
 arch/arm64/boot/dts/freescale/fsl-ls1088a.dtsi | 2 ++
 arch/arm64/boot/dts/freescale/fsl-ls208xa.dtsi | 2 ++
 arch/arm64/boot/dts/freescale/fsl-lx2160a.dtsi | 2 ++
 6 files changed, 13 insertions(+)

--- a/arch/arm64/boot/dts/freescale/fsl-ls1012a.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1012a.dtsi
@@ -443,6 +443,7 @@
 			snps,quirk-frame-length-adjustment = <0x20>;
 			snps,dis_rxdet_inp3_quirk;
 			snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
+			snps,host-vbus-glitches;
 		};
 
 		sata: sata@3200000 {
--- a/arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1043a.dtsi
@@ -713,6 +713,7 @@
 				usb3-lpm-capable;
 				snps,dis-u1u2-when-u3-quirk;
 				snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
+				snps,host-vbus-glitches;
 				configure-gfladj;
 			};
 
@@ -726,6 +727,7 @@
 				usb3-lpm-capable;
 				snps,dis-u1u2-when-u3-quirk;
 				snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
+				snps,host-vbus-glitches;
 				configure-gfladj;
 			};
 
@@ -739,6 +741,7 @@
 				usb3-lpm-capable;
 				snps,dis-u1u2-when-u3-quirk;
 				snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
+				snps,host-vbus-glitches;
 				configure-gfladj;
 			};
 
--- a/arch/arm64/boot/dts/freescale/fsl-ls1046a.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1046a.dtsi
@@ -611,6 +611,7 @@
 				snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
 				usb3-lpm-capable;
 				snps,dis-u1u2-when-u3-quirk;
+				snps,host-vbus-glitches;
 			};
 
 			usb1: usb@3000000 {
@@ -623,6 +624,7 @@
 				snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
 				usb3-lpm-capable;
 				snps,dis-u1u2-when-u3-quirk;
+				snps,host-vbus-glitches;
 			};
 
 			usb2: usb@3100000 {
@@ -635,6 +637,7 @@
 				snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
 				usb3-lpm-capable;
 				snps,dis-u1u2-when-u3-quirk;
+				snps,host-vbus-glitches;
 			};
 
 			sata: sata@3200000 {
--- a/arch/arm64/boot/dts/freescale/fsl-ls1088a.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-ls1088a.dtsi
@@ -452,6 +452,7 @@
 			snps,quirk-frame-length-adjustment = <0x20>;
 			snps,dis_rxdet_inp3_quirk;
 			snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
+			snps,host-vbus-glitches;
 			status = "disabled";
 		};
 
@@ -463,6 +464,7 @@
 			snps,quirk-frame-length-adjustment = <0x20>;
 			snps,dis_rxdet_inp3_quirk;
 			snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
+			snps,host-vbus-glitches;
 			status = "disabled";
 		};
 
--- a/arch/arm64/boot/dts/freescale/fsl-ls208xa.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-ls208xa.dtsi
@@ -819,6 +819,7 @@
 			snps,quirk-frame-length-adjustment = <0x20>;
 			snps,dis_rxdet_inp3_quirk;
 			snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
+			snps,host-vbus-glitches;
 		};
 
 		usb1: usb3@3110000 {
@@ -830,6 +831,7 @@
 			snps,quirk-frame-length-adjustment = <0x20>;
 			snps,dis_rxdet_inp3_quirk;
 			snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
+			snps,host-vbus-glitches;
 		};
 
 		serdes1: serdes@1ea0000 {
--- a/arch/arm64/boot/dts/freescale/fsl-lx2160a.dtsi
+++ b/arch/arm64/boot/dts/freescale/fsl-lx2160a.dtsi
@@ -845,6 +845,7 @@
 			snps,quirk-frame-length-adjustment = <0x20>;
 			snps,dis_rxdet_inp3_quirk;
 			snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
+			snps,host-vbus-glitches;
 			status = "disabled";
 		};
 
@@ -856,6 +857,7 @@
 			snps,quirk-frame-length-adjustment = <0x20>;
 			snps,dis_rxdet_inp3_quirk;
 			snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
+			snps,host-vbus-glitches;
 			status = "disabled";
 		};
 
