From 316be7f5f5f05e846b639b1eeee4267e18db9e69 Mon Sep 17 00:00:00 2001
From: Kuldeep Singh <kuldeep.singh@nxp.com>
Date: Fri, 3 Jan 2020 14:45:05 +0530
Subject: [PATCH] LF-20-2 mtd: spi-nor: Use 1 bit mode of spansion(s25fs512s)
 flash

Signed-off-by: Kuldeep Singh <kuldeep.singh@nxp.com>
---
 drivers/mtd/spi-nor/spi-nor.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/mtd/spi-nor/spi-nor.c
+++ b/drivers/mtd/spi-nor/spi-nor.c
@@ -2422,7 +2422,7 @@ static const struct flash_info spi_nor_i
 	{ "s25fl512s",  INFO6(0x010220, 0x4d0080, 256 * 1024, 256,
 			SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ |
 			SPI_NOR_HAS_LOCK | USE_CLSR) },
-	{ "s25fs512s",  INFO6(0x010220, 0x4d0081, 256 * 1024, 256, SPI_NOR_DUAL_READ | SPI_NOR_QUAD_READ | USE_CLSR) },
+	{ "s25fs512s",  INFO6(0x010220, 0x4d0081, 256 * 1024, 256, SPI_NOR_4B_OPCODES | USE_CLSR) },
 	{ "s70fl01gs",  INFO(0x010221, 0x4d00, 256 * 1024, 256, 0) },
 	{ "s25sl12800", INFO(0x012018, 0x0300, 256 * 1024,  64, 0) },
 	{ "s25sl12801", INFO(0x012018, 0x0301,  64 * 1024, 256, 0) },
