From 511c9a4b7c3d2e40eee68dad4d4c02ca42678204 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Thu, 25 Jun 2020 17:53:32 +0100
Subject: [PATCH] media: bcm2835-unicam: Add support for 12bit mono
 packed format

Now that V4L2_PIX_FMT_Y12P is defined, allow passing raw 12bit
mono packed data through the peripheral.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/media/platform/bcm2835/bcm2835-unicam.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/media/platform/bcm2835/bcm2835-unicam.c
+++ b/drivers/media/platform/bcm2835/bcm2835-unicam.c
@@ -336,7 +336,7 @@ static const struct unicam_fmt formats[]
 		.depth		= 10,
 		.csi_dt		= 0x2b,
 	}, {
-		/* NB There is no packed V4L2 fourcc for this format. */
+		.fourcc		= V4L2_PIX_FMT_Y12P,
 		.repacked_fourcc = V4L2_PIX_FMT_Y12,
 		.code		= MEDIA_BUS_FMT_Y12_1X12,
 		.depth		= 12,
