From 19d95534071c0bc330cce57d26391d804b24257c Mon Sep 17 00:00:00 2001
From: Xiaowei Bao <xiaowei.bao@nxp.com>
Date: Mon, 18 Feb 2019 16:12:42 +0800
Subject: [PATCH] misc: pci_endpoint_test: Add the layerscape PCIe GEN4 EP
 device support

Add the layerscape PCIE GEN4 EP device support in pci_endpoint_test driver.

Signed-off-by: Xiaowei Bao <xiaowei.bao@nxp.com>
Signed-off-by: Hou Zhiqiang <Zhiqiang.Hou@nxp.com>
---
 drivers/misc/pci_endpoint_test.c | 2 ++
 1 file changed, 2 insertions(+)

--- a/drivers/misc/pci_endpoint_test.c
+++ b/drivers/misc/pci_endpoint_test.c
@@ -65,6 +65,7 @@
 #define PCI_ENDPOINT_TEST_IRQ_NUMBER		0x28
 
 #define PCI_DEVICE_ID_TI_AM654			0xb00c
+#define PCI_DEVICE_ID_LX2160A			0x8d80
 
 #define is_am654_pci_dev(pdev)		\
 		((pdev)->device == PCI_DEVICE_ID_TI_AM654)
@@ -803,6 +804,7 @@ static const struct pci_device_id pci_en
 	{ PCI_DEVICE(PCI_VENDOR_ID_TI, PCI_DEVICE_ID_TI_DRA74x) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_TI, PCI_DEVICE_ID_TI_DRA72x) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_FREESCALE, 0x81c0) },
+	{ PCI_DEVICE(PCI_VENDOR_ID_FREESCALE, PCI_DEVICE_ID_LX2160A) },
 	{ PCI_DEVICE_DATA(SYNOPSYS, EDDA, NULL) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_TI, PCI_DEVICE_ID_TI_AM654),
 	  .driver_data = (kernel_ulong_t)&am654_data
