From d0e68d354f345873e15876a7b35be1baaf5e3ec9 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Fri, 5 Nov 2021 11:14:13 +0100
Subject: [PATCH] arm64: dts: broadcom: bcm4908: add DT for Netgear RAXE500
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

It's a home router based on BCM4908 SoC. It has: 1 GiB of RAM, 512 MiB
NAND flash, 6 Ethernet ports and 3 x BCM43684 (WiFi). One of Ethernet
ports is "2.5 G Multi-Gig port" that isn't described yet (it isn't known
how it's wired up).

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm64/boot/dts/broadcom/bcm4908/Makefile |  1 +
 .../bcm4908/bcm4908-netgear-raxe500.dts       | 50 +++++++++++++++++++
 2 files changed, 51 insertions(+)
 create mode 100644 arch/arm64/boot/dts/broadcom/bcm4908/bcm4908-netgear-raxe500.dts

--- a/arch/arm64/boot/dts/broadcom/bcm4908/Makefile
+++ b/arch/arm64/boot/dts/broadcom/bcm4908/Makefile
@@ -2,3 +2,4 @@
 dtb-$(CONFIG_ARCH_BCM4908) += bcm4906-netgear-r8000p.dtb
 dtb-$(CONFIG_ARCH_BCM4908) += bcm4906-tplink-archer-c2300-v1.dtb
 dtb-$(CONFIG_ARCH_BCM4908) += bcm4908-asus-gt-ac5300.dtb
+dtb-$(CONFIG_ARCH_BCM4908) += bcm4908-netgear-raxe500.dtb
--- /dev/null
+++ b/arch/arm64/boot/dts/broadcom/bcm4908/bcm4908-netgear-raxe500.dts
@@ -0,0 +1,50 @@
+// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
+
+#include "bcm4908.dtsi"
+
+/ {
+	compatible = "netgear,raxe500", "brcm,bcm4908";
+	model = "Netgear RAXE500";
+
+	memory@0 {
+		device_type = "memory";
+		reg = <0x00 0x00 0x00 0x40000000>;
+	};
+};
+
+&ehci {
+	status = "okay";
+};
+
+&ohci {
+	status = "okay";
+};
+
+&xhci {
+	status = "okay";
+};
+
+&ports {
+	port@0 {
+		label = "lan4";
+	};
+
+	port@1 {
+		label = "lan3";
+	};
+
+	port@2 {
+		label = "lan2";
+	};
+
+	port@3 {
+		label = "lan1";
+	};
+
+	port@7 {
+		reg = <7>;
+		phy-mode = "internal";
+		phy-handle = <&phy12>;
+		label = "wan";
+	};
+};
