From e7731194fdf085f46d58b1adccfddbd0dfee4873 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Fri, 7 Jul 2023 08:53:25 +0200
Subject: [PATCH] net: bgmac: postpone turning IRQs off to avoid SoC hangs
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Turning IRQs off is done by accessing Ethernet controller registers.
That can't be done until device's clock is enabled. It results in a SoC
hang otherwise.

This bug remained unnoticed for years as most bootloaders keep all
Ethernet interfaces turned on. It seems to only affect a niche SoC
family BCM47189. It has two Ethernet controllers but CFE bootloader uses
only the first one.

Fixes: 34322615cbaa ("net: bgmac: Mask interrupts during probe")
Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Reviewed-by: Michal Kubiak <michal.kubiak@intel.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/ethernet/broadcom/bgmac.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/drivers/net/ethernet/broadcom/bgmac.c
+++ b/drivers/net/ethernet/broadcom/bgmac.c
@@ -1491,8 +1491,6 @@ int bgmac_enet_probe(struct bgmac *bgmac
 
 	bgmac->in_init = true;
 
-	bgmac_chip_intrs_off(bgmac);
-
 	net_dev->irq = bgmac->irq;
 	SET_NETDEV_DEV(net_dev, bgmac->dev);
 	dev_set_drvdata(bgmac->dev, bgmac);
@@ -1510,6 +1508,8 @@ int bgmac_enet_probe(struct bgmac *bgmac
 	 */
 	bgmac_clk_enable(bgmac, 0);
 
+	bgmac_chip_intrs_off(bgmac);
+
 	/* This seems to be fixing IRQ by assigning OOB #6 to the core */
 	if (!(bgmac->feature_flags & BGMAC_FEAT_IDM_MASK)) {
 		if (bgmac->feature_flags & BGMAC_FEAT_IRQ_ID_OOB_6)
