From 9ad42557109a9db9ca16964352c3c045a775b018 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Thu, 19 Dec 2019 09:28:21 -0800
Subject: [PATCH] arm64: dts: allwinner: h5: Add thermal sensor and thermal
 zones

There are two sensors, one for CPU, one for GPU.

Signed-off-by: Ondrej Jirman <megous@megous.com>
Signed-off-by: Vasily Khoruzhick <anarsoul@gmail.com>
Signed-off-by: Maxime Ripard <maxime@cerno.tech>
---
 arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi | 26 ++++++++++++++++++++
 1 file changed, 26 insertions(+)

--- a/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi
@@ -174,6 +174,32 @@
 			assigned-clocks = <&ccu CLK_GPU>;
 			assigned-clock-rates = <384000000>;
 		};
+
+		ths: thermal-sensor@1c25000 {
+			compatible = "allwinner,sun50i-h5-ths";
+			reg = <0x01c25000 0x400>;
+			interrupts = <GIC_SPI 31 IRQ_TYPE_LEVEL_HIGH>;
+			resets = <&ccu RST_BUS_THS>;
+			clocks = <&ccu CLK_BUS_THS>, <&ccu CLK_THS>;
+			clock-names = "bus", "mod";
+			nvmem-cells = <&ths_calibration>;
+			nvmem-cell-names = "calibration";
+			#thermal-sensor-cells = <1>;
+		};
+	};
+
+	thermal-zones {
+		cpu_thermal: cpu-thermal {
+			polling-delay-passive = <0>;
+			polling-delay = <0>;
+			thermal-sensors = <&ths 0>;
+		};
+
+		gpu_thermal {
+			polling-delay-passive = <0>;
+			polling-delay = <0>;
+			thermal-sensors = <&ths 1>;
+		};
 	};
 };
 
