From 253358f373492608348136e569366d73cb969f6a Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Tue, 24 Oct 2023 09:26:05 +0200
Subject: [PATCH] ARM: dts: BCM5301X: Set switch ports for Linksys EA9200
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This patch was developed as OpenWrt downstream change and was recently
confirmed to work as expected.

Tested-by: Rani Hod <rani.hod@gmail.com>
Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Link: https://lore.kernel.org/r/20231024072605.32517-1-zajec5@gmail.com
Signed-off-by: Florian Fainelli <florian.fainelli@broadcom.com>
---
 .../dts/broadcom/bcm4709-linksys-ea9200.dts   | 38 +++++++++++++++++++
 1 file changed, 38 insertions(+)

--- a/arch/arm/boot/dts/bcm4709-linksys-ea9200.dts
+++ b/arch/arm/boot/dts/bcm4709-linksys-ea9200.dts
@@ -47,3 +47,41 @@
 &usb3_phy {
 	status = "okay";
 };
+
+&srab {
+	status = "okay";
+
+	ports {
+		port@0 {
+			label = "lan1";
+		};
+
+		port@1 {
+			label = "lan2";
+		};
+
+		port@2 {
+			label = "lan3";
+		};
+
+		port@3 {
+			label = "lan4";
+		};
+
+		port@4 {
+			label = "wan";
+		};
+
+		port@5 {
+			status = "disabled";
+		};
+
+		port@7 {
+			status = "disabled";
+		};
+
+		port@8 {
+			label = "cpu";
+		};
+	};
+};
