From 4d2bd7f66bac81b042afc2a6e742bd776a5a3938 Mon Sep 17 00:00:00 2001
From: Nicolas Saenz Julienne <nsaenzjulienne@suse.de>
Date: Wed, 11 Sep 2019 20:25:44 +0200
Subject: [PATCH] arm64: rename variables used to calculate
 ZONE_DMA32's size

commit a573cdd7973dedd87e62196c400332896bb236c8 upstream.

Let the name indicate that they are used to calculate ZONE_DMA32's size
as opposed to ZONE_DMA.

Signed-off-by: Nicolas Saenz Julienne <nsaenzjulienne@suse.de>
Reviewed-by: Catalin Marinas <catalin.marinas@arm.com>
Signed-off-by: Catalin Marinas <catalin.marinas@arm.com>
---
 arch/arm64/mm/init.c | 30 +++++++++++++++---------------
 1 file changed, 15 insertions(+), 15 deletions(-)

--- a/arch/arm64/mm/init.c
+++ b/arch/arm64/mm/init.c
@@ -50,7 +50,7 @@
 s64 memstart_addr __ro_after_init = -1;
 EXPORT_SYMBOL(memstart_addr);
 
-phys_addr_t arm64_dma_phys_limit __ro_after_init;
+phys_addr_t arm64_dma32_phys_limit __ro_after_init;
 
 #ifdef CONFIG_KEXEC_CORE
 /*
@@ -168,7 +168,7 @@ static void __init reserve_elfcorehdr(vo
  * currently assumes that for memory starting above 4G, 32-bit devices will
  * use a DMA offset.
  */
-static phys_addr_t __init max_zone_dma_phys(void)
+static phys_addr_t __init max_zone_dma32_phys(void)
 {
 	phys_addr_t offset = memblock_start_of_DRAM() & GENMASK_ULL(63, 32);
 	return min(offset + (1ULL << 32), memblock_end_of_DRAM());
@@ -181,7 +181,7 @@ static void __init zone_sizes_init(unsig
 	unsigned long max_zone_pfns[MAX_NR_ZONES]  = {0};
 
 #ifdef CONFIG_ZONE_DMA32
-	max_zone_pfns[ZONE_DMA32] = PFN_DOWN(arm64_dma_phys_limit);
+	max_zone_pfns[ZONE_DMA32] = PFN_DOWN(arm64_dma32_phys_limit);
 #endif
 	max_zone_pfns[ZONE_NORMAL] = max;
 
@@ -194,16 +194,16 @@ static void __init zone_sizes_init(unsig
 {
 	struct memblock_region *reg;
 	unsigned long zone_size[MAX_NR_ZONES], zhole_size[MAX_NR_ZONES];
-	unsigned long max_dma = min;
+	unsigned long max_dma32 = min;
 
 	memset(zone_size, 0, sizeof(zone_size));
 
 	/* 4GB maximum for 32-bit only capable devices */
 #ifdef CONFIG_ZONE_DMA32
-	max_dma = PFN_DOWN(arm64_dma_phys_limit);
-	zone_size[ZONE_DMA32] = max_dma - min;
+	max_dma32 = PFN_DOWN(arm64_dma32_phys_limit);
+	zone_size[ZONE_DMA32] = max_dma32 - min;
 #endif
-	zone_size[ZONE_NORMAL] = max - max_dma;
+	zone_size[ZONE_NORMAL] = max - max_dma32;
 
 	memcpy(zhole_size, zone_size, sizeof(zhole_size));
 
@@ -215,14 +215,14 @@ static void __init zone_sizes_init(unsig
 			continue;
 
 #ifdef CONFIG_ZONE_DMA32
-		if (start < max_dma) {
-			unsigned long dma_end = min(end, max_dma);
+		if (start < max_dma32) {
+			unsigned long dma_end = min(end, max_dma32);
 			zhole_size[ZONE_DMA32] -= dma_end - start;
 		}
 #endif
-		if (end > max_dma) {
+		if (end > max_dma32) {
 			unsigned long normal_end = min(end, max);
-			unsigned long normal_start = max(start, max_dma);
+			unsigned long normal_start = max(start, max_dma32);
 			zhole_size[ZONE_NORMAL] -= normal_end - normal_start;
 		}
 	}
@@ -422,9 +422,9 @@ void __init arm64_memblock_init(void)
 
 	/* 4GB maximum for 32-bit only capable devices */
 	if (IS_ENABLED(CONFIG_ZONE_DMA32))
-		arm64_dma_phys_limit = max_zone_dma_phys();
+		arm64_dma32_phys_limit = max_zone_dma32_phys();
 	else
-		arm64_dma_phys_limit = PHYS_MASK + 1;
+		arm64_dma32_phys_limit = PHYS_MASK + 1;
 
 	reserve_crashkernel();
 
@@ -432,7 +432,7 @@ void __init arm64_memblock_init(void)
 
 	high_memory = __va(memblock_end_of_DRAM() - 1) + 1;
 
-	dma_contiguous_reserve(arm64_dma_phys_limit);
+	dma_contiguous_reserve(arm64_dma32_phys_limit);
 }
 
 void __init bootmem_init(void)
@@ -536,7 +536,7 @@ static void __init free_unused_memmap(vo
 void __init mem_init(void)
 {
 	if (swiotlb_force == SWIOTLB_FORCE ||
-	    max_pfn > (arm64_dma_phys_limit >> PAGE_SHIFT))
+	    max_pfn > (arm64_dma32_phys_limit >> PAGE_SHIFT))
 		swiotlb_init(1);
 	else
 		swiotlb_force = SWIOTLB_NO_FORCE;
