From 92f17eecf263f3705a6e1a4f27ecb273ed3a33e5 Mon Sep 17 00:00:00 2001
From: Phil Elwell <phil@raspberrypi.org>
Date: Thu, 14 Nov 2019 12:00:43 +0000
Subject: [PATCH] drm/v3d: The third IRQ is optional

As of 5.4, the kernel logs errors for absent IRQs unless requested
with platform_get_irq_optional.

Signed-off-by: Phil Elwell <phil@raspberrypi.org>
---
 drivers/net/ethernet/broadcom/genet/bcmgenet.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/ethernet/broadcom/genet/bcmgenet.c
+++ b/drivers/net/ethernet/broadcom/genet/bcmgenet.c
@@ -3491,7 +3491,7 @@ static int bcmgenet_probe(struct platfor
 	priv = netdev_priv(dev);
 	priv->irq0 = platform_get_irq(pdev, 0);
 	priv->irq1 = platform_get_irq(pdev, 1);
-	priv->wol_irq = platform_get_irq(pdev, 2);
+	priv->wol_irq = platform_get_irq_optional(pdev, 2);
 	if (!priv->irq0 || !priv->irq1) {
 		dev_err(&pdev->dev, "can't find IRQs\n");
 		err = -EINVAL;
