// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "jdcloud,re-sp-01b", "mediatek,mt7621-soc";
	model = "JDCloud RE-SP-01B";

	aliases {
		led-boot = &led_red;
		led-failsafe = &led_red;
		led-running = &led_green;
		led-upgrade = &led_blue;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_red: red {
			label = "red:sys";
			gpios = <&gpio 6 GPIO_ACTIVE_LOW>;
			panic-indicator;
		};

		led_green: green {
			label = "green:sys";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
		};

		led_blue: blue {
			label = "blue:sys";
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
		};
	};
};

&sdhci {
	status = "okay";
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "config";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0x1ab0000>;
			};

			partition@1b00000 {
				label = "mini";
				reg = <0x1b00000 0x400000>;
				read-only;
			};

			partition@1f00000 {
				label = "oem";
				reg = <0x1f00000 0x100000>;
				read-only;
			};
		};
	};
};

&switch0 {
	ports {
		port@0 {
			status = "okay";
			label = "wan";
		};

		port@1 {
			status = "okay";
			label = "lan1";
		};

		port@2 {
			status = "okay";
			label = "lan2";
		};
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x0>;
	};
};

&pcie1 {
	wifi@0,0 {
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x8000>;
		ieee80211-freq-limit = <5000000 6000000>;
	};
};

&state_default {
	gpio {
		groups = "uart2", "uart3", "wdt";
		function = "gpio";
	};
};
