// SPDX-License-Identifier: GPL-2.0-only

#include "mt7620a.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	compatible = "lb-link,bl-w1200", "ralink,mt7620a-soc";
	model = "LB-Link BL-W1200";

	aliases {
		led-boot = &led_wps;
		led-failsafe = &led_wps;
		led-upgrade = &led_wps;
	};

	keys {
		compatible = "gpio-keys";

		reset_wps {
			label = "reset_wps";
			gpios = <&gpio0 13 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_wps: wps {
			label = "green:wps";
			gpios = <&gpio1 15 GPIO_ACTIVE_LOW>;
		};
	};
};

&gpio1 {
	status = "okay";
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <50000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "config";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0x7b0000>;
			};
		};
	};
};

&state_default {
	gpio {
		groups = "uartf", "spi refclk";
		function = "gpio";
	};
};

&ethernet {
	pinctrl-names = "default";
	pinctrl-0 = <&rgmii2_pins &mdio_pins>;

	mtd-mac-address = <&factory 0x28>;

	mediatek,portmap = "wllll";

	port@5 {
		status = "okay";
		mediatek,fixed-link = <1000 1 1 1>;
		phy-mode = "rgmii";
	};

	mdio-bus {
		status = "okay";

		ethernet-phy@0 {
			reg = <0>;
			phy-mode = "rgmii";
		};

		ethernet-phy@1 {
			reg = <1>;
			phy-mode = "rgmii";
		};

		ethernet-phy@2 {
			reg = <2>;
			phy-mode = "rgmii";
		};

		ethernet-phy@3 {
			reg = <3>;
			phy-mode = "rgmii";
		};

		ethernet-phy@4 {
			reg = <4>;
			phy-mode = "rgmii";
		};

		ethernet-phy@1f {
			reg = <0x1f>;
			phy-mode = "rgmii";
		};
	};
};

&gsw {
	mediatek,ephy-base = /bits/ 8 <12>;
};

&wmac {
	ralink,mtd-eeprom = <&factory 0x0>;
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		ieee80211-freq-limit = <5000000 6000000>;
		mediatek,mtd-eeprom = <&factory 0x8000>;

		led {
			led-sources = <2>;
			led-active-low;
		};
	};
};

&ehci {
	status = "okay";
};

&ohci {
	status = "okay";
};
