From 16422635ebace7f01b42412e5c0d889f5ad7512e Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.com>
Date: Wed, 6 Nov 2019 13:57:58 +0000
Subject: [PATCH] staging: vchiq_arm: Register bcm2835-codec as a
 platform driver

Following the same pattern as bcm2835-camera and bcm2835-audio,
register the V4L2 codec driver as a platform driver

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.com>
---
 drivers/staging/vc04_services/interface/vchiq_arm/vchiq_arm.c | 3 +++
 1 file changed, 3 insertions(+)

--- a/drivers/staging/vc04_services/interface/vchiq_arm/vchiq_arm.c
+++ b/drivers/staging/vc04_services/interface/vchiq_arm/vchiq_arm.c
@@ -140,6 +140,7 @@ static struct class  *vchiq_class;
 static DEFINE_SPINLOCK(msg_queue_spinlock);
 static struct platform_device *bcm2835_camera;
 static struct platform_device *bcm2835_audio;
+static struct platform_device *bcm2835_codec;
 static struct platform_device *vcsm_cma;
 
 static struct vchiq_drvdata bcm2835_drvdata = {
@@ -3252,6 +3253,7 @@ static int vchiq_probe(struct platform_d
 		MAJOR(vchiq_devid), MINOR(vchiq_devid));
 
 	vcsm_cma = vchiq_register_child(pdev, "vcsm-cma");
+	bcm2835_codec = vchiq_register_child(pdev, "bcm2835-codec");
 	bcm2835_camera = vchiq_register_child(pdev, "bcm2835-camera");
 	bcm2835_audio = vchiq_register_child(pdev, "bcm2835_audio");
 
@@ -3268,6 +3270,7 @@ static int vchiq_remove(struct platform_
 {
 	platform_device_unregister(bcm2835_audio);
 	platform_device_unregister(bcm2835_camera);
+	platform_device_unregister(bcm2835_codec);
 	platform_device_unregister(vcsm_cma);
 	vchiq_debugfs_deinit();
 	device_destroy(vchiq_class, vchiq_devid);
