#include "mt7620a.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	aliases {
		led-boot = &led_power;
		led-failsafe = &led_power;
		led-running = &led_power;
		led-upgrade = &led_power;
		label-mac-device = &ethernet;
	};

	leds {
		compatible = "gpio-leds";

		wlan {
			label = "blue:wlan";
			gpios = <&gpio3 0 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		usb {
			label = "blue:usb";
			gpios = <&gpio1 11 GPIO_ACTIVE_LOW>;
			trigger-sources = <&ohci_port1>, <&ehci_port1>;
			linux,default-trigger = "usbport";
		};

		led_power: power {
			label = "blue:power";
			gpios = <&gpio1 5 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&gpio0 1 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};
};

&gpio1 {
	status = "okay";
};

&gpio3 {
	status = "okay";
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <80000000>;
		m25p,fast-read;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x10000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;
			};

			firmware: partition@50000 {
				compatible = "openwrt,uimage", "denx,uimage";
				label = "firmware";
				openwrt,ih-magic = <0x12291000>;
				/* reg property is set based on flash size in DTS files */
			};
		};
	};
};

&state_default {
	default {
		groups = "i2c", "rgmii1", "wled";
		function = "gpio";
	};
};

&ethernet {
	pinctrl-names = "default";

	mtd-mac-address = <&factory 0x28>;

	mediatek,portmap = "llllw";
};

&wmac {
	ralink,mtd-eeprom = <&factory 0x0>;

	pinctrl-names = "default", "pa_gpio";
	pinctrl-0 = <&pa_pins>;
	pinctrl-1 = <&pa_gpio_pins>;
};

&sdhci {
	status = "okay";
};

&ehci {
	status = "okay";
};

&ohci {
	status = "okay";
};
