From ee6adaada426e3f04925f93b4372fa3534889775 Mon Sep 17 00:00:00 2001
From: Shengjiu Wang <shengjiu.wang@freescale.com>
Date: Thu, 12 May 2016 17:54:08 +0800
Subject: [PATCH] MLK-12786-2: ASoC: fsl_sai: correct the clock source for
 mclk0

mclk0 is assigned through the device tree.

Signed-off-by: Shengjiu Wang <shengjiu.wang@freescale.com>
---
 sound/soc/fsl/fsl_sai.c | 3 +--
 1 file changed, 1 insertion(+), 2 deletions(-)

--- a/sound/soc/fsl/fsl_sai.c
+++ b/sound/soc/fsl/fsl_sai.c
@@ -869,8 +869,7 @@ static int fsl_sai_probe(struct platform
 		sai->bus_clk = NULL;
 	}
 
-	sai->mclk_clk[0] = sai->bus_clk;
-	for (i = 1; i < FSL_SAI_MCLK_MAX; i++) {
+	for (i = 0; i < FSL_SAI_MCLK_MAX; i++) {
 		sprintf(tmp, "mclk%d", i);
 		sai->mclk_clk[i] = devm_clk_get(&pdev->dev, tmp);
 		if (IS_ERR(sai->mclk_clk[i])) {
