From 1b5a2dd9e266d78d5fddd7e6b116e47ba9577b5e Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Pali=20Roh=C3=A1r?= <pali@kernel.org>
Date: Thu, 30 Apr 2020 10:06:25 +0200
Subject: [PATCH] arm64: dts: marvell: armada-37xx: Move PCIe max-link-speed
 property
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Move the max-link-speed property of the PCIe node from board specific
device tree files to the generic armada-37xx.dtsi.

Armada 37xx supports only PCIe gen2 speed so max-link-speed property
should be in the generic armada-37xx.dtsi file.

Signed-off-by: Pali Rohár <pali@kernel.org>
Tested-by: Tomasz Maciej Nowak <tmn505@gmail.com>
Acked-by: Thomas Petazzoni <thomas.petazzoni@bootlin.com>
Signed-off-by: Gregory CLEMENT <gregory.clement@bootlin.com>
---
 arch/arm64/boot/dts/marvell/armada-3720-turris-mox.dts | 1 -
 arch/arm64/boot/dts/marvell/armada-37xx.dtsi           | 1 +
 2 files changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm64/boot/dts/marvell/armada-3720-turris-mox.dts
+++ b/arch/arm64/boot/dts/marvell/armada-3720-turris-mox.dts
@@ -135,7 +135,6 @@
 	pinctrl-names = "default";
 	pinctrl-0 = <&pcie_reset_pins &pcie_clkreq_pins>;
 	status = "okay";
-	max-link-speed = <2>;
 	reset-gpios = <&gpiosb 3 GPIO_ACTIVE_LOW>;
 	/*
 	 * U-Boot port for Turris Mox has a bug which always expects that "ranges" DT property
--- a/arch/arm64/boot/dts/marvell/armada-37xx.dtsi
+++ b/arch/arm64/boot/dts/marvell/armada-37xx.dtsi
@@ -501,6 +501,7 @@
 					<0 0 0 2 &pcie_intc 1>,
 					<0 0 0 3 &pcie_intc 2>,
 					<0 0 0 4 &pcie_intc 3>;
+			max-link-speed = <2>;
 			phys = <&comphy1 0>;
 			pcie_intc: interrupt-controller {
 				interrupt-controller;
