From: Lorenzo Bianconi <lorenzo@kernel.org>
Date: Thu, 24 Nov 2022 16:22:51 +0100
Subject: [PATCH] net: ethernet: mtk_wed: return status value in
 mtk_wdma_rx_reset

Move MTK_WDMA_RESET_IDX configuration in mtk_wdma_rx_reset routine.
Increase poll timeout to 10ms in order to be aligned with vendor sdk.
This is a preliminary patch to add Wireless Ethernet Dispatcher reset
support.

Co-developed-by: Sujuan Chen <sujuan.chen@mediatek.com>
Signed-off-by: Sujuan Chen <sujuan.chen@mediatek.com>
Signed-off-by: Lorenzo Bianconi <lorenzo@kernel.org>
Signed-off-by: Paolo Abeni <pabeni@redhat.com>
---

--- a/drivers/net/ethernet/mediatek/mtk_wed.c
+++ b/drivers/net/ethernet/mediatek/mtk_wed.c
@@ -101,17 +101,21 @@ mtk_wdma_read_reset(struct mtk_wed_devic
 	return wdma_r32(dev, MTK_WDMA_GLO_CFG);
 }
 
-static void
+static int
 mtk_wdma_rx_reset(struct mtk_wed_device *dev)
 {
 	u32 status, mask = MTK_WDMA_GLO_CFG_RX_DMA_BUSY;
-	int i;
+	int i, ret;
 
 	wdma_clr(dev, MTK_WDMA_GLO_CFG, MTK_WDMA_GLO_CFG_RX_DMA_EN);
-	if (readx_poll_timeout(mtk_wdma_read_reset, dev, status,
-			       !(status & mask), 0, 1000))
+	ret = readx_poll_timeout(mtk_wdma_read_reset, dev, status,
+				 !(status & mask), 0, 10000);
+	if (ret)
 		dev_err(dev->hw->dev, "rx reset failed\n");
 
+	wdma_w32(dev, MTK_WDMA_RESET_IDX, MTK_WDMA_RESET_IDX_RX);
+	wdma_w32(dev, MTK_WDMA_RESET_IDX, 0);
+
 	for (i = 0; i < ARRAY_SIZE(dev->rx_wdma); i++) {
 		if (dev->rx_wdma[i].desc)
 			continue;
@@ -119,6 +123,8 @@ mtk_wdma_rx_reset(struct mtk_wed_device
 		wdma_w32(dev,
 			 MTK_WDMA_RING_RX(i) + MTK_WED_RING_OFS_CPU_IDX, 0);
 	}
+
+	return ret;
 }
 
 static void
@@ -565,9 +571,7 @@ mtk_wed_detach(struct mtk_wed_device *de
 
 	mtk_wed_stop(dev);
 
-	wdma_w32(dev, MTK_WDMA_RESET_IDX, MTK_WDMA_RESET_IDX_RX);
-	wdma_w32(dev, MTK_WDMA_RESET_IDX, 0);
-
+	mtk_wdma_rx_reset(dev);
 	mtk_wed_reset(dev, MTK_WED_RESET_WED);
 	if (mtk_wed_get_rx_capa(dev)) {
 		wdma_clr(dev, MTK_WDMA_GLO_CFG, MTK_WDMA_GLO_CFG_TX_DMA_EN);
@@ -582,7 +586,6 @@ mtk_wed_detach(struct mtk_wed_device *de
 		mtk_wed_wo_reset(dev);
 		mtk_wed_free_rx_rings(dev);
 		mtk_wed_wo_deinit(hw);
-		mtk_wdma_rx_reset(dev);
 	}
 
 	if (dev->wlan.bus_type == MTK_WED_BUS_PCIE) {
@@ -1006,11 +1009,7 @@ mtk_wed_reset_dma(struct mtk_wed_device
 		wed_w32(dev, MTK_WED_RESET_IDX, 0);
 	}
 
-	wdma_w32(dev, MTK_WDMA_RESET_IDX, MTK_WDMA_RESET_IDX_RX);
-	wdma_w32(dev, MTK_WDMA_RESET_IDX, 0);
-
-	if (mtk_wed_get_rx_capa(dev))
-		mtk_wdma_rx_reset(dev);
+	mtk_wdma_rx_reset(dev);
 
 	if (busy) {
 		mtk_wed_reset(dev, MTK_WED_RESET_WDMA_INT_AGENT);
