From ee995101fde67f85a3cd4c74f4f92fc4592e726b Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Pali=20Roh=C3=A1r?= <pali@kernel.org>
Date: Thu, 3 Feb 2022 22:44:42 +0100
Subject: [PATCH 1/3] Revert "ata: ahci: mvebu: Make SATA PHY optional for
 Armada 3720"
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This reverts commit 45aefe3d2251e4e229d7662052739f96ad1d08d9.

Armada 3720 PHY driver (phy-mvebu-a3700-comphy.c) does not return
-EOPNOTSUPP from phy_power_on() callback anymore.

So remove AHCI_HFLAG_IGN_NOTSUPP_POWER_ON flag from Armada 3720 plat data.

AHCI_HFLAG_IGN_NOTSUPP_POWER_ON is not used by any other ahci driver, so
remove this flag completely.

Signed-off-by: Pali Rohár <pali@kernel.org>
Signed-off-by: Marek Behún <kabel@kernel.org>
Acked-by: Miquel Raynal <miquel.raynal@bootlin.com>
Acked-by: Damien Le Moal <damien.lemoal@opensource.wdc.com>
Link: https://lore.kernel.org/r/20220203214444.1508-4-kabel@kernel.org
Signed-off-by: Vinod Koul <vkoul@kernel.org>
---
 drivers/ata/ahci.h             | 2 --
 drivers/ata/ahci_mvebu.c       | 2 +-
 drivers/ata/libahci_platform.c | 2 +-
 3 files changed, 2 insertions(+), 4 deletions(-)

--- a/drivers/ata/ahci.h
+++ b/drivers/ata/ahci.h
@@ -241,8 +241,6 @@ enum {
 						      as default lpm_policy */
 	AHCI_HFLAG_SUSPEND_PHYS		= BIT(26), /* handle PHYs during
 						      suspend/resume */
-	AHCI_HFLAG_IGN_NOTSUPP_POWER_ON	= BIT(27), /* ignore -EOPNOTSUPP
-						      from phy_power_on() */
 	AHCI_HFLAG_NO_SXS		= BIT(28), /* SXS not supported */
 
 	/* ap->flags bits */
--- a/drivers/ata/ahci_mvebu.c
+++ b/drivers/ata/ahci_mvebu.c
@@ -227,7 +227,7 @@ static const struct ahci_mvebu_plat_data
 
 static const struct ahci_mvebu_plat_data ahci_mvebu_armada_3700_plat_data = {
 	.plat_config = ahci_mvebu_armada_3700_config,
-	.flags = AHCI_HFLAG_SUSPEND_PHYS | AHCI_HFLAG_IGN_NOTSUPP_POWER_ON,
+	.flags = AHCI_HFLAG_SUSPEND_PHYS,
 };
 
 static const struct of_device_id ahci_mvebu_of_match[] = {
--- a/drivers/ata/libahci_platform.c
+++ b/drivers/ata/libahci_platform.c
@@ -59,7 +59,7 @@ int ahci_platform_enable_phys(struct ahc
 		}
 
 		rc = phy_power_on(hpriv->phys[i]);
-		if (rc && !(rc == -EOPNOTSUPP && (hpriv->flags & AHCI_HFLAG_IGN_NOTSUPP_POWER_ON))) {
+		if (rc) {
 			phy_exit(hpriv->phys[i]);
 			goto disable_phys;
 		}
