From e6915e1acca57bc4fdb61dccd5cc2e49f72ef743 Mon Sep 17 00:00:00 2001
From: Peter Geis <pgwipeout@gmail.com>
Date: Wed, 15 Dec 2021 16:02:48 -0500
Subject: [PATCH] phy: phy-rockchip-inno-usb2: support standalone phy nodes

New Rockchip devices have the usb2 phy devices as standalone nodes
instead of children of the grf node.
Allow the driver to find the grf node from a phandle.

Signed-off-by: Peter Geis <pgwipeout@gmail.com>
Tested-by: Michael Riesch <michael.riesch@wolfvision.net>
Link: https://lore.kernel.org/r/20211215210252.120923-5-pgwipeout@gmail.com
Signed-off-by: Vinod Koul <vkoul@kernel.org>
---
 drivers/phy/rockchip/phy-rockchip-inno-usb2.c | 17 ++++++++++++-----
 1 file changed, 12 insertions(+), 5 deletions(-)

--- a/drivers/phy/rockchip/phy-rockchip-inno-usb2.c
+++ b/drivers/phy/rockchip/phy-rockchip-inno-usb2.c
@@ -1138,12 +1138,19 @@ static int rockchip_usb2phy_probe(struct
 		return -EINVAL;
 	}
 
-	if (!dev->parent || !dev->parent->of_node)
-		return -EINVAL;
+	if (!dev->parent || !dev->parent->of_node) {
+		rphy->grf = syscon_regmap_lookup_by_phandle(np, "rockchip,usbgrf");
+		if (IS_ERR(rphy->grf)) {
+			dev_err(dev, "failed to locate usbgrf\n");
+			return PTR_ERR(rphy->grf);
+		}
+	}
 
-	rphy->grf = syscon_node_to_regmap(dev->parent->of_node);
-	if (IS_ERR(rphy->grf))
-		return PTR_ERR(rphy->grf);
+	else {
+		rphy->grf = syscon_node_to_regmap(dev->parent->of_node);
+			if (IS_ERR(rphy->grf))
+				return PTR_ERR(rphy->grf);
+	}
 
 	if (of_device_is_compatible(np, "rockchip,rv1108-usb2phy")) {
 		rphy->usbgrf =
