From 94343612f165fc8b4f95fcbe6fd044d6f63d4a28 Mon Sep 17 00:00:00 2001
From: Shawn Guo <shawn.guo@linaro.org>
Date: Tue, 31 Aug 2021 13:23:25 +0800
Subject: [PATCH] arm64: dts: qcom: Update BAM DMA node name per DT schema

Follow dma-controller.yaml schema to use `dma-controller` as node name
of BAM DMA devices.

Signed-off-by: Shawn Guo <shawn.guo@linaro.org>
Signed-off-by: Bjorn Andersson <bjorn.andersson@linaro.org>
Link: https://lore.kernel.org/r/20210831052325.21229-1-shawn.guo@linaro.org
---
 arch/arm64/boot/dts/qcom/ipq8074.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm64/boot/dts/qcom/ipq8074.dtsi
+++ b/arch/arm64/boot/dts/qcom/ipq8074.dtsi
@@ -239,7 +239,7 @@
 			status = "disabled";
 		};
 
-		cryptobam: dma@704000 {
+		cryptobam: dma-controller@704000 {
 			compatible = "qcom,bam-v1.7.0";
 			reg = <0x00704000 0x20000>;
 			interrupts = <GIC_SPI 207 IRQ_TYPE_LEVEL_HIGH>;
