// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "tozed,zlt-s12-pro", "mediatek,mt7621-soc";
	model = "TOZED ZLT S12 PRO";

	aliases {
		led-boot = &led_power_blue;
		led-failsafe = &led_power_yellow;
		led-running = &led_power_blue;
		led-upgrade = &led_power_blue;
		label-mac-device = &wifi1;
	};

	chosen {
		bootargs = "console=ttyS0,115200";
	};

	leds {
		compatible = "gpio-leds";

		led-modem-blue {
			label = "blue:modem";
			gpios = <&gpio 33 GPIO_ACTIVE_LOW>;
		};

		led-modem-red {
			label = "red:modem";
			gpios = <&gpio 27 GPIO_ACTIVE_LOW>;
		};

		led_power_blue: led-power-blue {
			label = "blue:power";
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};

		led_power_yellow: led-power-yellow {
			label = "yellow:power";
			gpios = <&gpio 29 GPIO_ACTIVE_LOW>;
		};

		led-wifi {
			label = "blue:wifi";
			gpios = <&gpio 28 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};

		led-signal1 {
			label = "blue:signal1";
			gpios = <&gpio 25 GPIO_ACTIVE_LOW>;
		};

		led-signal2 {
			label = "blue:signal2";
			gpios = <&gpio 24 GPIO_ACTIVE_LOW>;
		};

		led-signal3 {
			label = "blue:signal3";
			gpios = <&gpio 23 GPIO_ACTIVE_LOW>;
		};

		led-signal4 {
			label = "blue:signal4";
			gpios = <&gpio 22 GPIO_ACTIVE_LOW>;
		};

		led-signal5 {
			label = "blue:signal5";
			gpios = <&gpio 26 GPIO_ACTIVE_LOW>;
		};

		led-phone {
			label = "blue:phone";
			gpios = <&gpio 31 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		button-reset {
			label = "reset";
			gpios = <&gpio 13 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		button-rfkill {
			label = "rfkill";
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RFKILL>;
		};

		button-wps {
			label = "wps";
			gpios = <&gpio 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};

	gpio_export {
		compatible = "gpio-export";

		lt72_ant0 {
			gpio-export,name = "lt72_ant0";
			gpio-export,input = <0>;
			gpios = <&gpio 6 GPIO_ACTIVE_HIGH>;
		};

		lt72_ant1 {
			gpio-export,name = "lt72_ant1";
			gpio-export,input = <0>;
			gpios = <&gpio 7 GPIO_ACTIVE_HIGH>;
		};

		lt72_power {
			gpio-export,name = "lt72_power";
			gpio-export,output = <1>;
			gpios = <&gpio 14 GPIO_ACTIVE_HIGH>;
		};
	};
};

&spi0 {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x0 0x30000>;
				read-only;
			};

			partition@30000 {
				label = "u-boot-env";
				reg = <0x30000 0x8000>;
				read-only;
			};

			// Stock config partition
			partition@38000 {
				label = "tozed-conf";
				reg = <0x38000 0x8000>;
				read-only;
			};

			factory: partition@40000 {
				label = "factory";
				reg = <0x40000 0x10000>;
				read-only;

				compatible = "nvmem-cells";
				#address-cells = <1>;
				#size-cells = <1>;

				macaddr_factory_e000: macaddr@e000 {
					reg = <0xe000 0x6>;
				};
			};

			partition@50000 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x50000 0xfb0000>;
			};
		};
	};
};

&pcie {
	status = "okay";
};

&pcie0 {
	wifi0: mt76@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x8000>;
		ieee80211-freq-limit = <5000000 6000000>;
	};
};

&pcie1 {
	wifi1: mt76@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		mediatek,mtd-eeprom = <&factory 0x0000>;
		ieee80211-freq-limit = <2400000 2500000>;
	};
};

&ethernet {
	pinctrl-0 = <&mdio_pins>, <&rgmii1_pins>;
};

&gmac0 {
	nvmem-cells = <&macaddr_factory_e000>;
	nvmem-cell-names = "mac-address";
};

&switch0 {
	ports {
		port@0 {
			status = "okay";
			label = "wan";
		};

		port@1 {
			status = "okay";
			label = "lan3";
		};

		port@2 {
			status = "okay";
			label = "lan2";
		};

		port@4 {
			status = "okay";
			label = "lan1";
		};
	};
};

&state_default {
	gpio {
		groups = "wdt", "rgmii2", "jtag", "uart3";
		function = "gpio";
	};
};
