# SPDX-License-Identifier: GPL-2.0-or-later

. /lib/functions/leds.sh
. /lib/functions/uci-defaults.sh

board_config_update

case "$(board_name)" in
arcadyan,ar7516)
	ucidef_set_led_netdev "wan" "WAN" "green:wan" "wan"
	ucidef_set_led_netdev "wlan0" "WiFi" "green:wifi" "phy0-ap0"
	;;
nucom,r5010unv2 |\
sercomm,ad1018)
	ucidef_set_led_usbport "usb" "USB" "green:usb" "usb1-port1" "usb2-port1"
	;;
esac

board_config_flush

exit 0
