
. /lib/functions/leds.sh
. /lib/functions/uci-defaults.sh

board=$(board_name)

board_config_update

case $board in
airlink101,ar670w|\
airlink101,ar725w)
	ucidef_set_led_netdev "wifi_led" "wifi" "rt2800soc-phy0::radio" "wlan0"
	;;
belkin,f5d8235-v1)
	ucidef_set_led_netdev "wifi_led" "wifi" "blue:wireless" "wlan0"
	;;
ralink,v11st-fe)
	ucidef_set_led_netdev "wifi_led" "wifi" "rt2800pci-phy0::radio" "wlan0"
	;;
esac

board_config_flush

exit 0
