From 2382c1b044231fd49eaf9aa82bc7113fc55487b8 Mon Sep 17 00:00:00 2001
From: Peng Fan <peng.fan@nxp.com>
Date: Fri, 13 Oct 2023 13:49:04 +0100
Subject: [PATCH] nvmem: imx: correct nregs for i.MX6ULL

The nregs for i.MX6ULL should be 80 per fuse map, correct it.

Fixes: ffbc34bf0e9c ("nvmem: imx-ocotp: Implement i.MX6ULL/ULZ support")
Cc: Stable@vger.kernel.org
Signed-off-by: Peng Fan <peng.fan@nxp.com>
Signed-off-by: Srinivas Kandagatla <srinivas.kandagatla@linaro.org>
Link: https://lore.kernel.org/r/20231013124904.175782-4-srinivas.kandagatla@linaro.org
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/nvmem/imx-ocotp.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/nvmem/imx-ocotp.c
+++ b/drivers/nvmem/imx-ocotp.c
@@ -520,7 +520,7 @@ static const struct ocotp_params imx6ul_
 };
 
 static const struct ocotp_params imx6ull_params = {
-	.nregs = 64,
+	.nregs = 80,
 	.bank_address_words = 0,
 	.set_timing = imx_ocotp_set_imx6_timing,
 	.ctrl = IMX_OCOTP_BM_CTRL_DEFAULT,
