From 0b000cbfe0aa0323bffa855ef8449c0687a4c071 Mon Sep 17 00:00:00 2001
From: INAGAKI Hiroshi <musashino.open@gmail.com>
Date: Thu, 6 May 2021 19:30:58 +0900
Subject: realtek: backport spi-realtek-rtl driver from 5.12 to 5.10

This patch backports "spi-realtek-rtl" driver to Kernel 5.10 from 5.12.
"MACH_REALTEK_RTL" is used as a platform name in upstream, but "RTL838X"
is used in OpenWrt, so update the dependency by the additional patch.

Submitted-by: INAGAKI Hiroshi <musashino.open@gmail.com>
---
 drivers/spi/Makefile                          |  2 +-
 1 files changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/spi/Makefile
+++ b/drivers/spi/Makefile
@@ -97,7 +97,7 @@ obj-$(CONFIG_SPI_QUP)			+= spi-qup.o
 obj-$(CONFIG_SPI_ROCKCHIP)		+= spi-rockchip.o
 obj-$(CONFIG_SPI_ROCKCHIP_SFC)		+= spi-rockchip-sfc.o
 obj-$(CONFIG_SPI_RB4XX)			+= spi-rb4xx.o
-obj-$(CONFIG_MACH_REALTEK_RTL)		+= spi-realtek-rtl.o
+obj-$(CONFIG_RTL83XX)			+= spi-realtek-rtl.o
 obj-$(CONFIG_SPI_RPCIF)			+= spi-rpc-if.o
 obj-$(CONFIG_SPI_RSPI)			+= spi-rspi.o
 obj-$(CONFIG_SPI_S3C24XX)		+= spi-s3c24xx-hw.o
