From patchwork Wed Nov  2 00:58:01 2022
Content-Type: text/plain; charset="utf-8"
MIME-Version: 1.0
Content-Transfer-Encoding: 7bit
X-Patchwork-Submitter: Daniel Golle <daniel@makrotopia.org>
X-Patchwork-Id: 13027653
X-Patchwork-Delegate: kuba@kernel.org
Return-Path: <netdev-owner@kernel.org>
Date: Wed, 2 Nov 2022 00:58:01 +0000
From: Daniel Golle <daniel@makrotopia.org>
To: Felix Fietkau <nbd@nbd.name>, John Crispin <john@phrozen.org>,
        Sean Wang <sean.wang@mediatek.com>,
        Mark Lee <Mark-MC.Lee@mediatek.com>,
        "David S. Miller" <davem@davemloft.net>,
        Eric Dumazet <edumazet@google.com>,
        Jakub Kicinski <kuba@kernel.org>,
        Paolo Abeni <pabeni@redhat.com>,
        Matthias Brugger <matthias.bgg@gmail.com>,
        netdev@vger.kernel.org, linux-arm-kernel@lists.infradead.org,
        linux-mediatek@lists.infradead.org, linux-kernel@vger.kernel.org
Subject: [PATCH v4] net: ethernet: mediatek: ppe: add support for flow
 accounting
Message-ID: <Y2HAmYYPd77dz+K5@makrotopia.org>
MIME-Version: 1.0
Content-Disposition: inline
Precedence: bulk
List-ID: <netdev.vger.kernel.org>
X-Mailing-List: netdev@vger.kernel.org
X-Patchwork-Delegate: kuba@kernel.org

The PPE units found in MT7622 and newer support packet and byte
accounting of hw-offloaded flows. Add support for reading those
counters as found in MediaTek's SDK[1].

[1]: https://git01.mediatek.com/plugins/gitiles/openwrt/feeds/mtk-openwrt-feeds/+/bc6a6a375c800dc2b80e1a325a2c732d1737df92
Signed-off-by: Daniel Golle <daniel@makrotopia.org>
---
v4: declare function mtk_mib_entry_read as static
v3: don't bother to set 'false' values in any zero-initialized struct
    use mtk_foe_entry_ib2
    both changes were requested by Felix Fietkau

v2: fix wrong variable name in return value check spotted by Denis Kirjanov

 drivers/net/ethernet/mediatek/mtk_eth_soc.c   |   7 +-
 drivers/net/ethernet/mediatek/mtk_eth_soc.h   |   1 +
 drivers/net/ethernet/mediatek/mtk_ppe.c       | 110 +++++++++++++++++-
 drivers/net/ethernet/mediatek/mtk_ppe.h       |  23 +++-
 .../net/ethernet/mediatek/mtk_ppe_debugfs.c   |   9 +-
 .../net/ethernet/mediatek/mtk_ppe_offload.c   |   7 ++
 drivers/net/ethernet/mediatek/mtk_ppe_regs.h  |  14 +++
 7 files changed, 166 insertions(+), 5 deletions(-)

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -4638,8 +4638,8 @@ static int mtk_probe(struct platform_dev
 		for (i = 0; i < num_ppe; i++) {
 			u32 ppe_addr = eth->soc->reg_map->ppe_base + i * 0x400;
 
-			eth->ppe[i] = mtk_ppe_init(eth, eth->base + ppe_addr,
-						   eth->soc->offload_version, i);
+			eth->ppe[i] = mtk_ppe_init(eth, eth->base + ppe_addr, i);
+
 			if (!eth->ppe[i]) {
 				err = -ENOMEM;
 				goto err_deinit_ppe;
@@ -4765,6 +4765,7 @@ static const struct mtk_soc_data mt7622_
 	.required_pctl = false,
 	.offload_version = 2,
 	.hash_offset = 2,
+	.has_accounting = true,
 	.foe_entry_size = sizeof(struct mtk_foe_entry) - 16,
 	.txrx = {
 		.txd_size = sizeof(struct mtk_tx_dma),
@@ -4802,6 +4803,7 @@ static const struct mtk_soc_data mt7629_
 	.hw_features = MTK_HW_FEATURES,
 	.required_clks = MT7629_CLKS_BITMAP,
 	.required_pctl = false,
+	.has_accounting = true,
 	.txrx = {
 		.txd_size = sizeof(struct mtk_tx_dma),
 		.rxd_size = sizeof(struct mtk_rx_dma),
@@ -4822,6 +4824,7 @@ static const struct mtk_soc_data mt7981_
 	.offload_version = 2,
 	.hash_offset = 4,
 	.foe_entry_size = sizeof(struct mtk_foe_entry),
+	.has_accounting = true,
 	.txrx = {
 		.txd_size = sizeof(struct mtk_tx_dma_v2),
 		.rxd_size = sizeof(struct mtk_rx_dma_v2),
@@ -4842,6 +4845,7 @@ static const struct mtk_soc_data mt7986_
 	.offload_version = 2,
 	.hash_offset = 4,
 	.foe_entry_size = sizeof(struct mtk_foe_entry),
+	.has_accounting = true,
 	.txrx = {
 		.txd_size = sizeof(struct mtk_tx_dma_v2),
 		.rxd_size = sizeof(struct mtk_rx_dma_v2),
--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.h
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.h
@@ -1008,6 +1008,8 @@ struct mtk_reg_map {
  *				the extra setup for those pins used by GMAC.
  * @hash_offset			Flow table hash offset.
  * @foe_entry_size		Foe table entry size.
+ * @has_accounting		Bool indicating support for accounting of
+ *				offloaded flows.
  * @txd_size			Tx DMA descriptor size.
  * @rxd_size			Rx DMA descriptor size.
  * @rx_irq_done_mask		Rx irq done register mask.
@@ -1025,6 +1027,7 @@ struct mtk_soc_data {
 	u8		hash_offset;
 	u16		foe_entry_size;
 	netdev_features_t hw_features;
+	bool		has_accounting;
 	struct {
 		u32	txd_size;
 		u32	rxd_size;
--- a/drivers/net/ethernet/mediatek/mtk_ppe.c
+++ b/drivers/net/ethernet/mediatek/mtk_ppe.c
@@ -74,6 +74,48 @@ static int mtk_ppe_wait_busy(struct mtk_
 	return ret;
 }
 
+static int mtk_ppe_mib_wait_busy(struct mtk_ppe *ppe)
+{
+	int ret;
+	u32 val;
+
+	ret = readl_poll_timeout(ppe->base + MTK_PPE_MIB_SER_CR, val,
+				 !(val & MTK_PPE_MIB_SER_CR_ST),
+				 20, MTK_PPE_WAIT_TIMEOUT_US);
+
+	if (ret)
+		dev_err(ppe->dev, "MIB table busy");
+
+	return ret;
+}
+
+static int mtk_mib_entry_read(struct mtk_ppe *ppe, u16 index, u64 *bytes, u64 *packets)
+{
+	u32 byte_cnt_low, byte_cnt_high, pkt_cnt_low, pkt_cnt_high;
+	u32 val, cnt_r0, cnt_r1, cnt_r2;
+	int ret;
+
+	val = FIELD_PREP(MTK_PPE_MIB_SER_CR_ADDR, index) | MTK_PPE_MIB_SER_CR_ST;
+	ppe_w32(ppe, MTK_PPE_MIB_SER_CR, val);
+
+	ret = mtk_ppe_mib_wait_busy(ppe);
+	if (ret)
+		return ret;
+
+	cnt_r0 = readl(ppe->base + MTK_PPE_MIB_SER_R0);
+	cnt_r1 = readl(ppe->base + MTK_PPE_MIB_SER_R1);
+	cnt_r2 = readl(ppe->base + MTK_PPE_MIB_SER_R2);
+
+	byte_cnt_low = FIELD_GET(MTK_PPE_MIB_SER_R0_BYTE_CNT_LOW, cnt_r0);
+	byte_cnt_high = FIELD_GET(MTK_PPE_MIB_SER_R1_BYTE_CNT_HIGH, cnt_r1);
+	pkt_cnt_low = FIELD_GET(MTK_PPE_MIB_SER_R1_PKT_CNT_LOW, cnt_r1);
+	pkt_cnt_high = FIELD_GET(MTK_PPE_MIB_SER_R2_PKT_CNT_HIGH, cnt_r2);
+	*bytes = ((u64)byte_cnt_high << 32) | byte_cnt_low;
+	*packets = (pkt_cnt_high << 16) | pkt_cnt_low;
+
+	return 0;
+}
+
 static void mtk_ppe_cache_clear(struct mtk_ppe *ppe)
 {
 	ppe_set(ppe, MTK_PPE_CACHE_CTL, MTK_PPE_CACHE_CTL_CLEAR);
@@ -465,6 +507,13 @@ __mtk_foe_entry_clear(struct mtk_ppe *pp
 		hwe->ib1 |= FIELD_PREP(MTK_FOE_IB1_STATE, MTK_FOE_STATE_INVALID);
 		dma_wmb();
 		mtk_ppe_cache_clear(ppe);
+		if (ppe->accounting) {
+			struct mtk_foe_accounting *acct;
+
+			acct = ppe->acct_table + entry->hash * sizeof(*acct);
+			acct->packets = 0;
+			acct->bytes = 0;
+		}
 	}
 	entry->hash = 0xffff;
 
@@ -572,6 +621,9 @@ __mtk_foe_entry_commit(struct mtk_ppe *p
 	wmb();
 	hwe->ib1 = entry->ib1;
 
+	if (ppe->accounting)
+		*mtk_foe_entry_ib2(eth, hwe) |= MTK_FOE_IB2_MIB_CNT;
+
 	dma_wmb();
 
 	mtk_ppe_cache_clear(ppe);
@@ -763,11 +815,39 @@ int mtk_ppe_prepare_reset(struct mtk_ppe
 	return mtk_ppe_wait_busy(ppe);
 }
 
-struct mtk_ppe *mtk_ppe_init(struct mtk_eth *eth, void __iomem *base,
-			     int version, int index)
+struct mtk_foe_accounting *mtk_foe_entry_get_mib(struct mtk_ppe *ppe, u32 index,
+						 struct mtk_foe_accounting *diff)
+{
+	struct mtk_foe_accounting *acct;
+	int size = sizeof(struct mtk_foe_accounting);
+	u64 bytes, packets;
+
+	if (!ppe->accounting)
+		return NULL;
+
+	if (mtk_mib_entry_read(ppe, index, &bytes, &packets))
+		return NULL;
+
+	acct = ppe->acct_table + index * size;
+
+	acct->bytes += bytes;
+	acct->packets += packets;
+
+	if (diff) {
+		diff->bytes = bytes;
+		diff->packets = packets;
+	}
+
+	return acct;
+}
+
+struct mtk_ppe *mtk_ppe_init(struct mtk_eth *eth, void __iomem *base, int index)
 {
+	bool accounting = eth->soc->has_accounting;
 	const struct mtk_soc_data *soc = eth->soc;
+	struct mtk_foe_accounting *acct;
 	struct device *dev = eth->dev;
+	struct mtk_mib_entry *mib;
 	struct mtk_ppe *ppe;
 	u32 foe_flow_size;
 	void *foe;
@@ -784,7 +864,8 @@ struct mtk_ppe *mtk_ppe_init(struct mtk_
 	ppe->base = base;
 	ppe->eth = eth;
 	ppe->dev = dev;
-	ppe->version = version;
+	ppe->version = eth->soc->offload_version;
+	ppe->accounting = accounting;
 
 	foe = dmam_alloc_coherent(ppe->dev,
 				  MTK_PPE_ENTRIES * soc->foe_entry_size,
@@ -800,6 +881,23 @@ struct mtk_ppe *mtk_ppe_init(struct mtk_
 	if (!ppe->foe_flow)
 		goto err_free_l2_flows;
 
+	if (accounting) {
+		mib = dmam_alloc_coherent(ppe->dev, MTK_PPE_ENTRIES * sizeof(*mib),
+					  &ppe->mib_phys, GFP_KERNEL);
+		if (!mib)
+			return NULL;
+
+		ppe->mib_table = mib;
+
+		acct = devm_kzalloc(dev, MTK_PPE_ENTRIES * sizeof(*acct),
+				    GFP_KERNEL);
+
+		if (!acct)
+			return NULL;
+
+		ppe->acct_table = acct;
+	}
+
 	mtk_ppe_debugfs_init(ppe, index);
 
 	return ppe;
@@ -929,6 +1027,16 @@ void mtk_ppe_start(struct mtk_ppe *ppe)
 		ppe_w32(ppe, MTK_PPE_DEFAULT_CPU_PORT1, 0xcb777);
 		ppe_w32(ppe, MTK_PPE_SBW_CTRL, 0x7f);
 	}
+
+	if (ppe->accounting && ppe->mib_phys) {
+		ppe_w32(ppe, MTK_PPE_MIB_TB_BASE, ppe->mib_phys);
+		ppe_m32(ppe, MTK_PPE_MIB_CFG, MTK_PPE_MIB_CFG_EN,
+			MTK_PPE_MIB_CFG_EN);
+		ppe_m32(ppe, MTK_PPE_MIB_CFG, MTK_PPE_MIB_CFG_RD_CLR,
+			MTK_PPE_MIB_CFG_RD_CLR);
+		ppe_m32(ppe, MTK_PPE_MIB_CACHE_CTL, MTK_PPE_MIB_CACHE_CTL_EN,
+			MTK_PPE_MIB_CFG_RD_CLR);
+	}
 }
 
 int mtk_ppe_stop(struct mtk_ppe *ppe)
--- a/drivers/net/ethernet/mediatek/mtk_ppe.h
+++ b/drivers/net/ethernet/mediatek/mtk_ppe.h
@@ -57,6 +57,7 @@ enum {
 #define MTK_FOE_IB2_MULTICAST		BIT(8)
 
 #define MTK_FOE_IB2_WDMA_QID2		GENMASK(13, 12)
+#define MTK_FOE_IB2_MIB_CNT		BIT(15)
 #define MTK_FOE_IB2_WDMA_DEVIDX		BIT(16)
 #define MTK_FOE_IB2_WDMA_WINFO		BIT(17)
 
@@ -285,16 +286,34 @@ struct mtk_flow_entry {
 	unsigned long cookie;
 };
 
+struct mtk_mib_entry {
+	u32	byt_cnt_l;
+	u16	byt_cnt_h;
+	u32	pkt_cnt_l;
+	u8	pkt_cnt_h;
+	u8	_rsv0;
+	u32	_rsv1;
+} __packed;
+
+struct mtk_foe_accounting {
+	u64	bytes;
+	u64	packets;
+};
+
 struct mtk_ppe {
 	struct mtk_eth *eth;
 	struct device *dev;
 	void __iomem *base;
 	int version;
 	char dirname[5];
+	bool accounting;
 
 	void *foe_table;
 	dma_addr_t foe_phys;
 
+	struct mtk_mib_entry *mib_table;
+	dma_addr_t mib_phys;
+
 	u16 foe_check_time[MTK_PPE_ENTRIES];
 	struct hlist_head *foe_flow;
 
@@ -303,8 +322,7 @@ struct mtk_ppe {
 	void *acct_table;
 };
 
-struct mtk_ppe *mtk_ppe_init(struct mtk_eth *eth, void __iomem *base,
-			     int version, int index);
+struct mtk_ppe *mtk_ppe_init(struct mtk_eth *eth, void __iomem *base, int index);
 void mtk_ppe_deinit(struct mtk_eth *eth);
 void mtk_ppe_start(struct mtk_ppe *ppe);
 int mtk_ppe_stop(struct mtk_ppe *ppe);
@@ -359,5 +377,7 @@ int mtk_foe_entry_commit(struct mtk_ppe
 void mtk_foe_entry_clear(struct mtk_ppe *ppe, struct mtk_flow_entry *entry);
 int mtk_foe_entry_idle_time(struct mtk_ppe *ppe, struct mtk_flow_entry *entry);
 int mtk_ppe_debugfs_init(struct mtk_ppe *ppe, int index);
+struct mtk_foe_accounting *mtk_foe_entry_get_mib(struct mtk_ppe *ppe, u32 index,
+						 struct mtk_foe_accounting *diff);
 
 #endif
--- a/drivers/net/ethernet/mediatek/mtk_ppe_debugfs.c
+++ b/drivers/net/ethernet/mediatek/mtk_ppe_debugfs.c
@@ -82,6 +82,7 @@ mtk_ppe_debugfs_foe_show(struct seq_file
 		struct mtk_foe_entry *entry = mtk_foe_get_entry(ppe, i);
 		struct mtk_foe_mac_info *l2;
 		struct mtk_flow_addr_info ai = {};
+		struct mtk_foe_accounting *acct;
 		unsigned char h_source[ETH_ALEN];
 		unsigned char h_dest[ETH_ALEN];
 		int type, state;
@@ -95,6 +96,8 @@ mtk_ppe_debugfs_foe_show(struct seq_file
 		if (bind && state != MTK_FOE_STATE_BIND)
 			continue;
 
+		acct = mtk_foe_entry_get_mib(ppe, i, NULL);
+
 		type = FIELD_GET(MTK_FOE_IB1_PACKET_TYPE, entry->ib1);
 		seq_printf(m, "%05x %s %7s", i,
 			   mtk_foe_entry_state_str(state),
@@ -153,9 +156,11 @@ mtk_ppe_debugfs_foe_show(struct seq_file
 		*((__be16 *)&h_dest[4]) = htons(l2->dest_mac_lo);
 
 		seq_printf(m, " eth=%pM->%pM etype=%04x"
-			      " vlan=%d,%d ib1=%08x ib2=%08x\n",
+			      " vlan=%d,%d ib1=%08x ib2=%08x"
+			      " packets=%llu bytes=%llu\n",
 			   h_source, h_dest, ntohs(l2->etype),
-			   l2->vlan1, l2->vlan2, entry->ib1, ib2);
+			   l2->vlan1, l2->vlan2, entry->ib1, ib2,
+			   acct ? acct->packets : 0, acct ? acct->bytes : 0);
 	}
 
 	return 0;
--- a/drivers/net/ethernet/mediatek/mtk_ppe_offload.c
+++ b/drivers/net/ethernet/mediatek/mtk_ppe_offload.c
@@ -497,6 +497,7 @@ static int
 mtk_flow_offload_stats(struct mtk_eth *eth, struct flow_cls_offload *f)
 {
 	struct mtk_flow_entry *entry;
+	struct mtk_foe_accounting diff;
 	u32 idle;
 
 	entry = rhashtable_lookup(&eth->flow_table, &f->cookie,
@@ -507,6 +508,13 @@ mtk_flow_offload_stats(struct mtk_eth *e
 	idle = mtk_foe_entry_idle_time(eth->ppe[entry->ppe_index], entry);
 	f->stats.lastused = jiffies - idle * HZ;
 
+	if (entry->hash != 0xFFFF &&
+	    mtk_foe_entry_get_mib(eth->ppe[entry->ppe_index], entry->hash,
+				  &diff)) {
+		f->stats.pkts += diff.packets;
+		f->stats.bytes += diff.bytes;
+	}
+
 	return 0;
 }
 
--- a/drivers/net/ethernet/mediatek/mtk_ppe_regs.h
+++ b/drivers/net/ethernet/mediatek/mtk_ppe_regs.h
@@ -149,6 +149,20 @@ enum {
 
 #define MTK_PPE_MIB_TB_BASE			0x338
 
+#define MTK_PPE_MIB_SER_CR			0x33C
+#define MTK_PPE_MIB_SER_CR_ST			BIT(16)
+#define MTK_PPE_MIB_SER_CR_ADDR			GENMASK(13, 0)
+
+#define MTK_PPE_MIB_SER_R0			0x340
+#define MTK_PPE_MIB_SER_R0_BYTE_CNT_LOW		GENMASK(31, 0)
+
+#define MTK_PPE_MIB_SER_R1			0x344
+#define MTK_PPE_MIB_SER_R1_PKT_CNT_LOW		GENMASK(31, 16)
+#define MTK_PPE_MIB_SER_R1_BYTE_CNT_HIGH	GENMASK(15, 0)
+
+#define MTK_PPE_MIB_SER_R2			0x348
+#define MTK_PPE_MIB_SER_R2_PKT_CNT_HIGH		GENMASK(23, 0)
+
 #define MTK_PPE_MIB_CACHE_CTL			0x350
 #define MTK_PPE_MIB_CACHE_CTL_EN		BIT(0)
 #define MTK_PPE_MIB_CACHE_CTL_FLUSH		BIT(2)
