From ba39b344e9240a4a5fd4ab8178200b85cd1809da Mon Sep 17 00:00:00 2001
From: Christian Marangi <ansuelsmth@gmail.com>
Date: Sat, 23 Jul 2022 16:29:32 +0200
Subject: [PATCH 4/5] net: ethernet: stmicro: stmmac: generate stmmac dma conf
 before open

Rework the driver to generate the stmmac dma_conf before stmmac_open.
This permits a function to first check if it's possible to allocate a
new dma_config and then pass it directly to __stmmac_open and "open" the
interface with the new configuration.

Signed-off-by: Christian Marangi <ansuelsmth@gmail.com>
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 .../net/ethernet/stmicro/stmmac/stmmac_main.c | 462 +++++++++++-------
 1 file changed, 289 insertions(+), 173 deletions(-)

--- a/drivers/net/ethernet/stmicro/stmmac/stmmac_main.c
+++ b/drivers/net/ethernet/stmicro/stmmac/stmmac_main.c
@@ -1301,7 +1301,8 @@ static int stmmac_phy_setup(struct stmma
 	return 0;
 }
 
-static void stmmac_display_rx_rings(struct stmmac_priv *priv)
+static void stmmac_display_rx_rings(struct stmmac_priv *priv,
+				    struct stmmac_dma_conf *dma_conf)
 {
 	u32 rx_cnt = priv->plat->rx_queues_to_use;
 	unsigned int desc_size;
@@ -1310,7 +1311,7 @@ static void stmmac_display_rx_rings(stru
 
 	/* Display RX rings */
 	for (queue = 0; queue < rx_cnt; queue++) {
-		struct stmmac_rx_queue *rx_q = &priv->dma_conf.rx_queue[queue];
+		struct stmmac_rx_queue *rx_q = &dma_conf->rx_queue[queue];
 
 		pr_info("\tRX Queue %u rings\n", queue);
 
@@ -1323,12 +1324,13 @@ static void stmmac_display_rx_rings(stru
 		}
 
 		/* Display RX ring */
-		stmmac_display_ring(priv, head_rx, priv->dma_conf.dma_rx_size, true,
+		stmmac_display_ring(priv, head_rx, dma_conf->dma_rx_size, true,
 				    rx_q->dma_rx_phy, desc_size);
 	}
 }
 
-static void stmmac_display_tx_rings(struct stmmac_priv *priv)
+static void stmmac_display_tx_rings(struct stmmac_priv *priv,
+				    struct stmmac_dma_conf *dma_conf)
 {
 	u32 tx_cnt = priv->plat->tx_queues_to_use;
 	unsigned int desc_size;
@@ -1337,7 +1339,7 @@ static void stmmac_display_tx_rings(stru
 
 	/* Display TX rings */
 	for (queue = 0; queue < tx_cnt; queue++) {
-		struct stmmac_tx_queue *tx_q = &priv->dma_conf.tx_queue[queue];
+		struct stmmac_tx_queue *tx_q = &dma_conf->tx_queue[queue];
 
 		pr_info("\tTX Queue %d rings\n", queue);
 
@@ -1352,18 +1354,19 @@ static void stmmac_display_tx_rings(stru
 			desc_size = sizeof(struct dma_desc);
 		}
 
-		stmmac_display_ring(priv, head_tx, priv->dma_conf.dma_tx_size, false,
+		stmmac_display_ring(priv, head_tx, dma_conf->dma_tx_size, false,
 				    tx_q->dma_tx_phy, desc_size);
 	}
 }
 
-static void stmmac_display_rings(struct stmmac_priv *priv)
+static void stmmac_display_rings(struct stmmac_priv *priv,
+				 struct stmmac_dma_conf *dma_conf)
 {
 	/* Display RX ring */
-	stmmac_display_rx_rings(priv);
+	stmmac_display_rx_rings(priv, dma_conf);
 
 	/* Display TX ring */
-	stmmac_display_tx_rings(priv);
+	stmmac_display_tx_rings(priv, dma_conf);
 }
 
 static int stmmac_set_bfsize(int mtu, int bufsize)
@@ -1387,44 +1390,50 @@ static int stmmac_set_bfsize(int mtu, in
 /**
  * stmmac_clear_rx_descriptors - clear RX descriptors
  * @priv: driver private structure
+ * @dma_conf: structure to take the dma data
  * @queue: RX queue index
  * Description: this function is called to clear the RX descriptors
  * in case of both basic and extended descriptors are used.
  */
-static void stmmac_clear_rx_descriptors(struct stmmac_priv *priv, u32 queue)
+static void stmmac_clear_rx_descriptors(struct stmmac_priv *priv,
+					struct stmmac_dma_conf *dma_conf,
+					u32 queue)
 {
-	struct stmmac_rx_queue *rx_q = &priv->dma_conf.rx_queue[queue];
+	struct stmmac_rx_queue *rx_q = &dma_conf->rx_queue[queue];
 	int i;
 
 	/* Clear the RX descriptors */
-	for (i = 0; i < priv->dma_conf.dma_rx_size; i++)
+	for (i = 0; i < dma_conf->dma_rx_size; i++)
 		if (priv->extend_desc)
 			stmmac_init_rx_desc(priv, &rx_q->dma_erx[i].basic,
 					priv->use_riwt, priv->mode,
-					(i == priv->dma_conf.dma_rx_size - 1),
-					priv->dma_conf.dma_buf_sz);
+					(i == dma_conf->dma_rx_size - 1),
+					dma_conf->dma_buf_sz);
 		else
 			stmmac_init_rx_desc(priv, &rx_q->dma_rx[i],
 					priv->use_riwt, priv->mode,
-					(i == priv->dma_conf.dma_rx_size - 1),
-					priv->dma_conf.dma_buf_sz);
+					(i == dma_conf->dma_rx_size - 1),
+					dma_conf->dma_buf_sz);
 }
 
 /**
  * stmmac_clear_tx_descriptors - clear tx descriptors
  * @priv: driver private structure
+ * @dma_conf: structure to take the dma data
  * @queue: TX queue index.
  * Description: this function is called to clear the TX descriptors
  * in case of both basic and extended descriptors are used.
  */
-static void stmmac_clear_tx_descriptors(struct stmmac_priv *priv, u32 queue)
+static void stmmac_clear_tx_descriptors(struct stmmac_priv *priv,
+					struct stmmac_dma_conf *dma_conf,
+					u32 queue)
 {
-	struct stmmac_tx_queue *tx_q = &priv->dma_conf.tx_queue[queue];
+	struct stmmac_tx_queue *tx_q = &dma_conf->tx_queue[queue];
 	int i;
 
 	/* Clear the TX descriptors */
-	for (i = 0; i < priv->dma_conf.dma_tx_size; i++) {
-		int last = (i == (priv->dma_conf.dma_tx_size - 1));
+	for (i = 0; i < dma_conf->dma_tx_size; i++) {
+		int last = (i == (dma_conf->dma_tx_size - 1));
 		struct dma_desc *p;
 
 		if (priv->extend_desc)
@@ -1441,10 +1450,12 @@ static void stmmac_clear_tx_descriptors(
 /**
  * stmmac_clear_descriptors - clear descriptors
  * @priv: driver private structure
+ * @dma_conf: structure to take the dma data
  * Description: this function is called to clear the TX and RX descriptors
  * in case of both basic and extended descriptors are used.
  */
-static void stmmac_clear_descriptors(struct stmmac_priv *priv)
+static void stmmac_clear_descriptors(struct stmmac_priv *priv,
+				     struct stmmac_dma_conf *dma_conf)
 {
 	u32 rx_queue_cnt = priv->plat->rx_queues_to_use;
 	u32 tx_queue_cnt = priv->plat->tx_queues_to_use;
@@ -1452,16 +1463,17 @@ static void stmmac_clear_descriptors(str
 
 	/* Clear the RX descriptors */
 	for (queue = 0; queue < rx_queue_cnt; queue++)
-		stmmac_clear_rx_descriptors(priv, queue);
+		stmmac_clear_rx_descriptors(priv, dma_conf, queue);
 
 	/* Clear the TX descriptors */
 	for (queue = 0; queue < tx_queue_cnt; queue++)
-		stmmac_clear_tx_descriptors(priv, queue);
+		stmmac_clear_tx_descriptors(priv, dma_conf, queue);
 }
 
 /**
  * stmmac_init_rx_buffers - init the RX descriptor buffer.
  * @priv: driver private structure
+ * @dma_conf: structure to take the dma data
  * @p: descriptor pointer
  * @i: descriptor index
  * @flags: gfp flag
@@ -1469,10 +1481,12 @@ static void stmmac_clear_descriptors(str
  * Description: this function is called to allocate a receive buffer, perform
  * the DMA mapping and init the descriptor.
  */
-static int stmmac_init_rx_buffers(struct stmmac_priv *priv, struct dma_desc *p,
+static int stmmac_init_rx_buffers(struct stmmac_priv *priv,
+				  struct stmmac_dma_conf *dma_conf,
+				  struct dma_desc *p,
 				  int i, gfp_t flags, u32 queue)
 {
-	struct stmmac_rx_queue *rx_q = &priv->dma_conf.rx_queue[queue];
+	struct stmmac_rx_queue *rx_q = &dma_conf->rx_queue[queue];
 	struct stmmac_rx_buffer *buf = &rx_q->buf_pool[i];
 
 	if (!buf->page) {
@@ -1497,7 +1511,7 @@ static int stmmac_init_rx_buffers(struct
 	buf->addr = page_pool_get_dma_addr(buf->page) + buf->page_offset;
 
 	stmmac_set_desc_addr(priv, p, buf->addr);
-	if (priv->dma_conf.dma_buf_sz == BUF_SIZE_16KiB)
+	if (dma_conf->dma_buf_sz == BUF_SIZE_16KiB)
 		stmmac_init_desc3(priv, p);
 
 	return 0;
@@ -1506,12 +1520,13 @@ static int stmmac_init_rx_buffers(struct
 /**
  * stmmac_free_rx_buffer - free RX dma buffers
  * @priv: private structure
- * @queue: RX queue index
+ * @rx_q: RX queue
  * @i: buffer index.
  */
-static void stmmac_free_rx_buffer(struct stmmac_priv *priv, u32 queue, int i)
+static void stmmac_free_rx_buffer(struct stmmac_priv *priv,
+				  struct stmmac_rx_queue *rx_q,
+				  int i)
 {
-	struct stmmac_rx_queue *rx_q = &priv->dma_conf.rx_queue[queue];
 	struct stmmac_rx_buffer *buf = &rx_q->buf_pool[i];
 
 	if (buf->page)
@@ -1526,12 +1541,15 @@ static void stmmac_free_rx_buffer(struct
 /**
  * stmmac_free_tx_buffer - free RX dma buffers
  * @priv: private structure
+ * @dma_conf: structure to take the dma data
  * @queue: RX queue index
  * @i: buffer index.
  */
-static void stmmac_free_tx_buffer(struct stmmac_priv *priv, u32 queue, int i)
+static void stmmac_free_tx_buffer(struct stmmac_priv *priv,
+				  struct stmmac_dma_conf *dma_conf,
+				  u32 queue, int i)
 {
-	struct stmmac_tx_queue *tx_q = &priv->dma_conf.tx_queue[queue];
+	struct stmmac_tx_queue *tx_q = &dma_conf->tx_queue[queue];
 
 	if (tx_q->tx_skbuff_dma[i].buf &&
 	    tx_q->tx_skbuff_dma[i].buf_type != STMMAC_TXBUF_T_XDP_TX) {
@@ -1570,23 +1588,28 @@ static void stmmac_free_tx_buffer(struct
 /**
  * dma_free_rx_skbufs - free RX dma buffers
  * @priv: private structure
+ * @dma_conf: structure to take the dma data
  * @queue: RX queue index
  */
-static void dma_free_rx_skbufs(struct stmmac_priv *priv, u32 queue)
+static void dma_free_rx_skbufs(struct stmmac_priv *priv,
+			       struct stmmac_dma_conf *dma_conf,
+			       u32 queue)
 {
+	struct stmmac_rx_queue *rx_q = &dma_conf->rx_queue[queue];
 	int i;
 
-	for (i = 0; i < priv->dma_conf.dma_rx_size; i++)
-		stmmac_free_rx_buffer(priv, queue, i);
+	for (i = 0; i < dma_conf->dma_rx_size; i++)
+		stmmac_free_rx_buffer(priv, rx_q, i);
 }
 
-static int stmmac_alloc_rx_buffers(struct stmmac_priv *priv, u32 queue,
-				   gfp_t flags)
+static int stmmac_alloc_rx_buffers(struct stmmac_priv *priv,
+				   struct stmmac_dma_conf *dma_conf,
+				   u32 queue, gfp_t flags)
 {
-	struct stmmac_rx_queue *rx_q = &priv->dma_conf.rx_queue[queue];
+	struct stmmac_rx_queue *rx_q = &dma_conf->rx_queue[queue];
 	int i;
 
-	for (i = 0; i < priv->dma_conf.dma_rx_size; i++) {
+	for (i = 0; i < dma_conf->dma_rx_size; i++) {
 		struct dma_desc *p;
 		int ret;
 
@@ -1595,7 +1618,7 @@ static int stmmac_alloc_rx_buffers(struc
 		else
 			p = rx_q->dma_rx + i;
 
-		ret = stmmac_init_rx_buffers(priv, p, i, flags,
+		ret = stmmac_init_rx_buffers(priv, dma_conf, p, i, flags,
 					     queue);
 		if (ret)
 			return ret;
@@ -1609,14 +1632,17 @@ static int stmmac_alloc_rx_buffers(struc
 /**
  * dma_free_rx_xskbufs - free RX dma buffers from XSK pool
  * @priv: private structure
+ * @dma_conf: structure to take the dma data
  * @queue: RX queue index
  */
-static void dma_free_rx_xskbufs(struct stmmac_priv *priv, u32 queue)
+static void dma_free_rx_xskbufs(struct stmmac_priv *priv,
+				struct stmmac_dma_conf *dma_conf,
+				u32 queue)
 {
-	struct stmmac_rx_queue *rx_q = &priv->dma_conf.rx_queue[queue];
+	struct stmmac_rx_queue *rx_q = &dma_conf->rx_queue[queue];
 	int i;
 
-	for (i = 0; i < priv->dma_conf.dma_rx_size; i++) {
+	for (i = 0; i < dma_conf->dma_rx_size; i++) {
 		struct stmmac_rx_buffer *buf = &rx_q->buf_pool[i];
 
 		if (!buf->xdp)
@@ -1627,12 +1653,14 @@ static void dma_free_rx_xskbufs(struct s
 	}
 }
 
-static int stmmac_alloc_rx_buffers_zc(struct stmmac_priv *priv, u32 queue)
+static int stmmac_alloc_rx_buffers_zc(struct stmmac_priv *priv,
+				      struct stmmac_dma_conf *dma_conf,
+				      u32 queue)
 {
-	struct stmmac_rx_queue *rx_q = &priv->dma_conf.rx_queue[queue];
+	struct stmmac_rx_queue *rx_q = &dma_conf->rx_queue[queue];
 	int i;
 
-	for (i = 0; i < priv->dma_conf.dma_rx_size; i++) {
+	for (i = 0; i < dma_conf->dma_rx_size; i++) {
 		struct stmmac_rx_buffer *buf;
 		dma_addr_t dma_addr;
 		struct dma_desc *p;
@@ -1667,22 +1695,25 @@ static struct xsk_buff_pool *stmmac_get_
 /**
  * __init_dma_rx_desc_rings - init the RX descriptor ring (per queue)
  * @priv: driver private structure
+ * @dma_conf: structure to take the dma data
  * @queue: RX queue index
  * @flags: gfp flag.
  * Description: this function initializes the DMA RX descriptors
  * and allocates the socket buffers. It supports the chained and ring
  * modes.
  */
-static int __init_dma_rx_desc_rings(struct stmmac_priv *priv, u32 queue, gfp_t flags)
+static int __init_dma_rx_desc_rings(struct stmmac_priv *priv,
+				    struct stmmac_dma_conf *dma_conf,
+				    u32 queue, gfp_t flags)
 {
-	struct stmmac_rx_queue *rx_q = &priv->dma_conf.rx_queue[queue];
+	struct stmmac_rx_queue *rx_q = &dma_conf->rx_queue[queue];
 	int ret;
 
 	netif_dbg(priv, probe, priv->dev,
 		  "(%s) dma_rx_phy=0x%08x\n", __func__,
 		  (u32)rx_q->dma_rx_phy);
 
-	stmmac_clear_rx_descriptors(priv, queue);
+	stmmac_clear_rx_descriptors(priv, dma_conf, queue);
 
 	xdp_rxq_info_unreg_mem_model(&rx_q->xdp_rxq);
 
@@ -1709,9 +1740,9 @@ static int __init_dma_rx_desc_rings(stru
 		/* RX XDP ZC buffer pool may not be populated, e.g.
 		 * xdpsock TX-only.
 		 */
-		stmmac_alloc_rx_buffers_zc(priv, queue);
+		stmmac_alloc_rx_buffers_zc(priv, dma_conf, queue);
 	} else {
-		ret = stmmac_alloc_rx_buffers(priv, queue, flags);
+		ret = stmmac_alloc_rx_buffers(priv, dma_conf, queue, flags);
 		if (ret < 0)
 			return -ENOMEM;
 	}
@@ -1721,17 +1752,19 @@ static int __init_dma_rx_desc_rings(stru
 		if (priv->extend_desc)
 			stmmac_mode_init(priv, rx_q->dma_erx,
 					 rx_q->dma_rx_phy,
-					 priv->dma_conf.dma_rx_size, 1);
+					 dma_conf->dma_rx_size, 1);
 		else
 			stmmac_mode_init(priv, rx_q->dma_rx,
 					 rx_q->dma_rx_phy,
-					 priv->dma_conf.dma_rx_size, 0);
+					 dma_conf->dma_rx_size, 0);
 	}
 
 	return 0;
 }
 
-static int init_dma_rx_desc_rings(struct net_device *dev, gfp_t flags)
+static int init_dma_rx_desc_rings(struct net_device *dev,
+				  struct stmmac_dma_conf *dma_conf,
+				  gfp_t flags)
 {
 	struct stmmac_priv *priv = netdev_priv(dev);
 	u32 rx_count = priv->plat->rx_queues_to_use;
@@ -1743,7 +1776,7 @@ static int init_dma_rx_desc_rings(struct
 		  "SKB addresses:\nskb\t\tskb data\tdma data\n");
 
 	for (queue = 0; queue < rx_count; queue++) {
-		ret = __init_dma_rx_desc_rings(priv, queue, flags);
+		ret = __init_dma_rx_desc_rings(priv, dma_conf, queue, flags);
 		if (ret)
 			goto err_init_rx_buffers;
 	}
@@ -1752,12 +1785,12 @@ static int init_dma_rx_desc_rings(struct
 
 err_init_rx_buffers:
 	while (queue >= 0) {
-		struct stmmac_rx_queue *rx_q = &priv->dma_conf.rx_queue[queue];
+		struct stmmac_rx_queue *rx_q = &dma_conf->rx_queue[queue];
 
 		if (rx_q->xsk_pool)
-			dma_free_rx_xskbufs(priv, queue);
+			dma_free_rx_xskbufs(priv, dma_conf, queue);
 		else
-			dma_free_rx_skbufs(priv, queue);
+			dma_free_rx_skbufs(priv, dma_conf, queue);
 
 		rx_q->buf_alloc_num = 0;
 		rx_q->xsk_pool = NULL;
@@ -1774,14 +1807,17 @@ err_init_rx_buffers:
 /**
  * __init_dma_tx_desc_rings - init the TX descriptor ring (per queue)
  * @priv: driver private structure
- * @queue : TX queue index
+ * @dma_conf: structure to take the dma data
+ * @queue: TX queue index
  * Description: this function initializes the DMA TX descriptors
  * and allocates the socket buffers. It supports the chained and ring
  * modes.
  */
-static int __init_dma_tx_desc_rings(struct stmmac_priv *priv, u32 queue)
+static int __init_dma_tx_desc_rings(struct stmmac_priv *priv,
+				    struct stmmac_dma_conf *dma_conf,
+				    u32 queue)
 {
-	struct stmmac_tx_queue *tx_q = &priv->dma_conf.tx_queue[queue];
+	struct stmmac_tx_queue *tx_q = &dma_conf->tx_queue[queue];
 	int i;
 
 	netif_dbg(priv, probe, priv->dev,
@@ -1793,16 +1829,16 @@ static int __init_dma_tx_desc_rings(stru
 		if (priv->extend_desc)
 			stmmac_mode_init(priv, tx_q->dma_etx,
 					 tx_q->dma_tx_phy,
-					 priv->dma_conf.dma_tx_size, 1);
+					 dma_conf->dma_tx_size, 1);
 		else if (!(tx_q->tbs & STMMAC_TBS_AVAIL))
 			stmmac_mode_init(priv, tx_q->dma_tx,
 					 tx_q->dma_tx_phy,
-					 priv->dma_conf.dma_tx_size, 0);
+					 dma_conf->dma_tx_size, 0);
 	}
 
 	tx_q->xsk_pool = stmmac_get_xsk_pool(priv, queue);
 
-	for (i = 0; i < priv->dma_conf.dma_tx_size; i++) {
+	for (i = 0; i < dma_conf->dma_tx_size; i++) {
 		struct dma_desc *p;
 
 		if (priv->extend_desc)
@@ -1824,7 +1860,8 @@ static int __init_dma_tx_desc_rings(stru
 	return 0;
 }
 
-static int init_dma_tx_desc_rings(struct net_device *dev)
+static int init_dma_tx_desc_rings(struct net_device *dev,
+				  struct stmmac_dma_conf *dma_conf)
 {
 	struct stmmac_priv *priv = netdev_priv(dev);
 	u32 tx_queue_cnt;
@@ -1833,7 +1870,7 @@ static int init_dma_tx_desc_rings(struct
 	tx_queue_cnt = priv->plat->tx_queues_to_use;
 
 	for (queue = 0; queue < tx_queue_cnt; queue++)
-		__init_dma_tx_desc_rings(priv, queue);
+		__init_dma_tx_desc_rings(priv, dma_conf, queue);
 
 	return 0;
 }
@@ -1841,26 +1878,29 @@ static int init_dma_tx_desc_rings(struct
 /**
  * init_dma_desc_rings - init the RX/TX descriptor rings
  * @dev: net device structure
+ * @dma_conf: structure to take the dma data
  * @flags: gfp flag.
  * Description: this function initializes the DMA RX/TX descriptors
  * and allocates the socket buffers. It supports the chained and ring
  * modes.
  */
-static int init_dma_desc_rings(struct net_device *dev, gfp_t flags)
+static int init_dma_desc_rings(struct net_device *dev,
+			       struct stmmac_dma_conf *dma_conf,
+			       gfp_t flags)
 {
 	struct stmmac_priv *priv = netdev_priv(dev);
 	int ret;
 
-	ret = init_dma_rx_desc_rings(dev, flags);
+	ret = init_dma_rx_desc_rings(dev, dma_conf, flags);
 	if (ret)
 		return ret;
 
-	ret = init_dma_tx_desc_rings(dev);
+	ret = init_dma_tx_desc_rings(dev, dma_conf);
 
-	stmmac_clear_descriptors(priv);
+	stmmac_clear_descriptors(priv, dma_conf);
 
 	if (netif_msg_hw(priv))
-		stmmac_display_rings(priv);
+		stmmac_display_rings(priv, dma_conf);
 
 	return ret;
 }
@@ -1868,17 +1908,20 @@ static int init_dma_desc_rings(struct ne
 /**
  * dma_free_tx_skbufs - free TX dma buffers
  * @priv: private structure
+ * @dma_conf: structure to take the dma data
  * @queue: TX queue index
  */
-static void dma_free_tx_skbufs(struct stmmac_priv *priv, u32 queue)
+static void dma_free_tx_skbufs(struct stmmac_priv *priv,
+			       struct stmmac_dma_conf *dma_conf,
+			       u32 queue)
 {
-	struct stmmac_tx_queue *tx_q = &priv->dma_conf.tx_queue[queue];
+	struct stmmac_tx_queue *tx_q = &dma_conf->tx_queue[queue];
 	int i;
 
 	tx_q->xsk_frames_done = 0;
 
-	for (i = 0; i < priv->dma_conf.dma_tx_size; i++)
-		stmmac_free_tx_buffer(priv, queue, i);
+	for (i = 0; i < dma_conf->dma_tx_size; i++)
+		stmmac_free_tx_buffer(priv, dma_conf, queue, i);
 
 	if (tx_q->xsk_pool && tx_q->xsk_frames_done) {
 		xsk_tx_completed(tx_q->xsk_pool, tx_q->xsk_frames_done);
@@ -1897,34 +1940,37 @@ static void stmmac_free_tx_skbufs(struct
 	u32 queue;
 
 	for (queue = 0; queue < tx_queue_cnt; queue++)
-		dma_free_tx_skbufs(priv, queue);
+		dma_free_tx_skbufs(priv, &priv->dma_conf, queue);
 }
 
 /**
  * __free_dma_rx_desc_resources - free RX dma desc resources (per queue)
  * @priv: private structure
+ * @dma_conf: structure to take the dma data
  * @queue: RX queue index
  */
-static void __free_dma_rx_desc_resources(struct stmmac_priv *priv, u32 queue)
+static void __free_dma_rx_desc_resources(struct stmmac_priv *priv,
+					 struct stmmac_dma_conf *dma_conf,
+					 u32 queue)
 {
-	struct stmmac_rx_queue *rx_q = &priv->dma_conf.rx_queue[queue];
+	struct stmmac_rx_queue *rx_q = &dma_conf->rx_queue[queue];
 
 	/* Release the DMA RX socket buffers */
 	if (rx_q->xsk_pool)
-		dma_free_rx_xskbufs(priv, queue);
+		dma_free_rx_xskbufs(priv, dma_conf, queue);
 	else
-		dma_free_rx_skbufs(priv, queue);
+		dma_free_rx_skbufs(priv, dma_conf, queue);
 
 	rx_q->buf_alloc_num = 0;
 	rx_q->xsk_pool = NULL;
 
 	/* Free DMA regions of consistent memory previously allocated */
 	if (!priv->extend_desc)
-		dma_free_coherent(priv->device, priv->dma_conf.dma_rx_size *
+		dma_free_coherent(priv->device, dma_conf->dma_rx_size *
 				  sizeof(struct dma_desc),
 				  rx_q->dma_rx, rx_q->dma_rx_phy);
 	else
-		dma_free_coherent(priv->device, priv->dma_conf.dma_rx_size *
+		dma_free_coherent(priv->device, dma_conf->dma_rx_size *
 				  sizeof(struct dma_extended_desc),
 				  rx_q->dma_erx, rx_q->dma_rx_phy);
 
@@ -1936,29 +1982,33 @@ static void __free_dma_rx_desc_resources
 		page_pool_destroy(rx_q->page_pool);
 }
 
-static void free_dma_rx_desc_resources(struct stmmac_priv *priv)
+static void free_dma_rx_desc_resources(struct stmmac_priv *priv,
+				       struct stmmac_dma_conf *dma_conf)
 {
 	u32 rx_count = priv->plat->rx_queues_to_use;
 	u32 queue;
 
 	/* Free RX queue resources */
 	for (queue = 0; queue < rx_count; queue++)
-		__free_dma_rx_desc_resources(priv, queue);
+		__free_dma_rx_desc_resources(priv, dma_conf, queue);
 }
 
 /**
  * __free_dma_tx_desc_resources - free TX dma desc resources (per queue)
  * @priv: private structure
+ * @dma_conf: structure to take the dma data
  * @queue: TX queue index
  */
-static void __free_dma_tx_desc_resources(struct stmmac_priv *priv, u32 queue)
+static void __free_dma_tx_desc_resources(struct stmmac_priv *priv,
+					 struct stmmac_dma_conf *dma_conf,
+					 u32 queue)
 {
-	struct stmmac_tx_queue *tx_q = &priv->dma_conf.tx_queue[queue];
+	struct stmmac_tx_queue *tx_q = &dma_conf->tx_queue[queue];
 	size_t size;
 	void *addr;
 
 	/* Release the DMA TX socket buffers */
-	dma_free_tx_skbufs(priv, queue);
+	dma_free_tx_skbufs(priv, dma_conf, queue);
 
 	if (priv->extend_desc) {
 		size = sizeof(struct dma_extended_desc);
@@ -1971,7 +2021,7 @@ static void __free_dma_tx_desc_resources
 		addr = tx_q->dma_tx;
 	}
 
-	size *= priv->dma_conf.dma_tx_size;
+	size *= dma_conf->dma_tx_size;
 
 	dma_free_coherent(priv->device, size, addr, tx_q->dma_tx_phy);
 
@@ -1979,28 +2029,32 @@ static void __free_dma_tx_desc_resources
 	kfree(tx_q->tx_skbuff);
 }
 
-static void free_dma_tx_desc_resources(struct stmmac_priv *priv)
+static void free_dma_tx_desc_resources(struct stmmac_priv *priv,
+				       struct stmmac_dma_conf *dma_conf)
 {
 	u32 tx_count = priv->plat->tx_queues_to_use;
 	u32 queue;
 
 	/* Free TX queue resources */
 	for (queue = 0; queue < tx_count; queue++)
-		__free_dma_tx_desc_resources(priv, queue);
+		__free_dma_tx_desc_resources(priv, dma_conf, queue);
 }
 
 /**
  * __alloc_dma_rx_desc_resources - alloc RX resources (per queue).
  * @priv: private structure
+ * @dma_conf: structure to take the dma data
  * @queue: RX queue index
  * Description: according to which descriptor can be used (extend or basic)
  * this function allocates the resources for TX and RX paths. In case of
  * reception, for example, it pre-allocated the RX socket buffer in order to
  * allow zero-copy mechanism.
  */
-static int __alloc_dma_rx_desc_resources(struct stmmac_priv *priv, u32 queue)
+static int __alloc_dma_rx_desc_resources(struct stmmac_priv *priv,
+					 struct stmmac_dma_conf *dma_conf,
+					 u32 queue)
 {
-	struct stmmac_rx_queue *rx_q = &priv->dma_conf.rx_queue[queue];
+	struct stmmac_rx_queue *rx_q = &dma_conf->rx_queue[queue];
 	struct stmmac_channel *ch = &priv->channel[queue];
 	bool xdp_prog = stmmac_xdp_is_enabled(priv);
 	struct page_pool_params pp_params = { 0 };
@@ -2012,8 +2066,8 @@ static int __alloc_dma_rx_desc_resources
 	rx_q->priv_data = priv;
 
 	pp_params.flags = PP_FLAG_DMA_MAP | PP_FLAG_DMA_SYNC_DEV;
-	pp_params.pool_size = priv->dma_conf.dma_rx_size;
-	num_pages = DIV_ROUND_UP(priv->dma_conf.dma_buf_sz, PAGE_SIZE);
+	pp_params.pool_size = dma_conf->dma_rx_size;
+	num_pages = DIV_ROUND_UP(dma_conf->dma_buf_sz, PAGE_SIZE);
 	pp_params.order = ilog2(num_pages);
 	pp_params.nid = dev_to_node(priv->device);
 	pp_params.dev = priv->device;
@@ -2028,7 +2082,7 @@ static int __alloc_dma_rx_desc_resources
 		return ret;
 	}
 
-	rx_q->buf_pool = kcalloc(priv->dma_conf.dma_rx_size,
+	rx_q->buf_pool = kcalloc(dma_conf->dma_rx_size,
 				 sizeof(*rx_q->buf_pool),
 				 GFP_KERNEL);
 	if (!rx_q->buf_pool)
@@ -2036,7 +2090,7 @@ static int __alloc_dma_rx_desc_resources
 
 	if (priv->extend_desc) {
 		rx_q->dma_erx = dma_alloc_coherent(priv->device,
-						   priv->dma_conf.dma_rx_size *
+						   dma_conf->dma_rx_size *
 						   sizeof(struct dma_extended_desc),
 						   &rx_q->dma_rx_phy,
 						   GFP_KERNEL);
@@ -2045,7 +2099,7 @@ static int __alloc_dma_rx_desc_resources
 
 	} else {
 		rx_q->dma_rx = dma_alloc_coherent(priv->device,
-						  priv->dma_conf.dma_rx_size *
+						  dma_conf->dma_rx_size *
 						  sizeof(struct dma_desc),
 						  &rx_q->dma_rx_phy,
 						  GFP_KERNEL);
@@ -2070,7 +2124,8 @@ static int __alloc_dma_rx_desc_resources
 	return 0;
 }
 
-static int alloc_dma_rx_desc_resources(struct stmmac_priv *priv)
+static int alloc_dma_rx_desc_resources(struct stmmac_priv *priv,
+				       struct stmmac_dma_conf *dma_conf)
 {
 	u32 rx_count = priv->plat->rx_queues_to_use;
 	u32 queue;
@@ -2078,7 +2133,7 @@ static int alloc_dma_rx_desc_resources(s
 
 	/* RX queues buffers and DMA */
 	for (queue = 0; queue < rx_count; queue++) {
-		ret = __alloc_dma_rx_desc_resources(priv, queue);
+		ret = __alloc_dma_rx_desc_resources(priv, dma_conf, queue);
 		if (ret)
 			goto err_dma;
 	}
@@ -2086,7 +2141,7 @@ static int alloc_dma_rx_desc_resources(s
 	return 0;
 
 err_dma:
-	free_dma_rx_desc_resources(priv);
+	free_dma_rx_desc_resources(priv, dma_conf);
 
 	return ret;
 }
@@ -2094,28 +2149,31 @@ err_dma:
 /**
  * __alloc_dma_tx_desc_resources - alloc TX resources (per queue).
  * @priv: private structure
+ * @dma_conf: structure to take the dma data
  * @queue: TX queue index
  * Description: according to which descriptor can be used (extend or basic)
  * this function allocates the resources for TX and RX paths. In case of
  * reception, for example, it pre-allocated the RX socket buffer in order to
  * allow zero-copy mechanism.
  */
-static int __alloc_dma_tx_desc_resources(struct stmmac_priv *priv, u32 queue)
+static int __alloc_dma_tx_desc_resources(struct stmmac_priv *priv,
+					 struct stmmac_dma_conf *dma_conf,
+					 u32 queue)
 {
-	struct stmmac_tx_queue *tx_q = &priv->dma_conf.tx_queue[queue];
+	struct stmmac_tx_queue *tx_q = &dma_conf->tx_queue[queue];
 	size_t size;
 	void *addr;
 
 	tx_q->queue_index = queue;
 	tx_q->priv_data = priv;
 
-	tx_q->tx_skbuff_dma = kcalloc(priv->dma_conf.dma_tx_size,
+	tx_q->tx_skbuff_dma = kcalloc(dma_conf->dma_tx_size,
 				      sizeof(*tx_q->tx_skbuff_dma),
 				      GFP_KERNEL);
 	if (!tx_q->tx_skbuff_dma)
 		return -ENOMEM;
 
-	tx_q->tx_skbuff = kcalloc(priv->dma_conf.dma_tx_size,
+	tx_q->tx_skbuff = kcalloc(dma_conf->dma_tx_size,
 				  sizeof(struct sk_buff *),
 				  GFP_KERNEL);
 	if (!tx_q->tx_skbuff)
@@ -2128,7 +2186,7 @@ static int __alloc_dma_tx_desc_resources
 	else
 		size = sizeof(struct dma_desc);
 
-	size *= priv->dma_conf.dma_tx_size;
+	size *= dma_conf->dma_tx_size;
 
 	addr = dma_alloc_coherent(priv->device, size,
 				  &tx_q->dma_tx_phy, GFP_KERNEL);
@@ -2145,7 +2203,8 @@ static int __alloc_dma_tx_desc_resources
 	return 0;
 }
 
-static int alloc_dma_tx_desc_resources(struct stmmac_priv *priv)
+static int alloc_dma_tx_desc_resources(struct stmmac_priv *priv,
+				       struct stmmac_dma_conf *dma_conf)
 {
 	u32 tx_count = priv->plat->tx_queues_to_use;
 	u32 queue;
@@ -2153,7 +2212,7 @@ static int alloc_dma_tx_desc_resources(s
 
 	/* TX queues buffers and DMA */
 	for (queue = 0; queue < tx_count; queue++) {
-		ret = __alloc_dma_tx_desc_resources(priv, queue);
+		ret = __alloc_dma_tx_desc_resources(priv, dma_conf, queue);
 		if (ret)
 			goto err_dma;
 	}
@@ -2161,27 +2220,29 @@ static int alloc_dma_tx_desc_resources(s
 	return 0;
 
 err_dma:
-	free_dma_tx_desc_resources(priv);
+	free_dma_tx_desc_resources(priv, dma_conf);
 	return ret;
 }
 
 /**
  * alloc_dma_desc_resources - alloc TX/RX resources.
  * @priv: private structure
+ * @dma_conf: structure to take the dma data
  * Description: according to which descriptor can be used (extend or basic)
  * this function allocates the resources for TX and RX paths. In case of
  * reception, for example, it pre-allocated the RX socket buffer in order to
  * allow zero-copy mechanism.
  */
-static int alloc_dma_desc_resources(struct stmmac_priv *priv)
+static int alloc_dma_desc_resources(struct stmmac_priv *priv,
+				    struct stmmac_dma_conf *dma_conf)
 {
 	/* RX Allocation */
-	int ret = alloc_dma_rx_desc_resources(priv);
+	int ret = alloc_dma_rx_desc_resources(priv, dma_conf);
 
 	if (ret)
 		return ret;
 
-	ret = alloc_dma_tx_desc_resources(priv);
+	ret = alloc_dma_tx_desc_resources(priv, dma_conf);
 
 	return ret;
 }
@@ -2189,16 +2250,18 @@ static int alloc_dma_desc_resources(stru
 /**
  * free_dma_desc_resources - free dma desc resources
  * @priv: private structure
+ * @dma_conf: structure to take the dma data
  */
-static void free_dma_desc_resources(struct stmmac_priv *priv)
+static void free_dma_desc_resources(struct stmmac_priv *priv,
+				    struct stmmac_dma_conf *dma_conf)
 {
 	/* Release the DMA TX socket buffers */
-	free_dma_tx_desc_resources(priv);
+	free_dma_tx_desc_resources(priv, dma_conf);
 
 	/* Release the DMA RX socket buffers later
 	 * to ensure all pending XDP_TX buffers are returned.
 	 */
-	free_dma_rx_desc_resources(priv);
+	free_dma_rx_desc_resources(priv, dma_conf);
 }
 
 /**
@@ -2687,8 +2750,8 @@ static void stmmac_tx_err(struct stmmac_
 	netif_tx_stop_queue(netdev_get_tx_queue(priv->dev, chan));
 
 	stmmac_stop_tx_dma(priv, chan);
-	dma_free_tx_skbufs(priv, chan);
-	stmmac_clear_tx_descriptors(priv, chan);
+	dma_free_tx_skbufs(priv, &priv->dma_conf, chan);
+	stmmac_clear_tx_descriptors(priv, &priv->dma_conf, chan);
 	stmmac_reset_tx_queue(priv, chan);
 	stmmac_init_tx_chan(priv, priv->ioaddr, priv->plat->dma_cfg,
 			    tx_q->dma_tx_phy, chan);
@@ -3686,19 +3749,93 @@ static int stmmac_request_irq(struct net
 }
 
 /**
- *  stmmac_open - open entry point of the driver
+ *  stmmac_setup_dma_desc - Generate a dma_conf and allocate DMA queue
+ *  @priv: driver private structure
+ *  @mtu: MTU to setup the dma queue and buf with
+ *  Description: Allocate and generate a dma_conf based on the provided MTU.
+ *  Allocate the Tx/Rx DMA queue and init them.
+ *  Return value:
+ *  the dma_conf allocated struct on success and an appropriate ERR_PTR on failure.
+ */
+static struct stmmac_dma_conf *
+stmmac_setup_dma_desc(struct stmmac_priv *priv, unsigned int mtu)
+{
+	struct stmmac_dma_conf *dma_conf;
+	int chan, bfsize, ret;
+
+	dma_conf = kzalloc(sizeof(*dma_conf), GFP_KERNEL);
+	if (!dma_conf) {
+		netdev_err(priv->dev, "%s: DMA conf allocation failed\n",
+			   __func__);
+		return ERR_PTR(-ENOMEM);
+	}
+
+	bfsize = stmmac_set_16kib_bfsize(priv, mtu);
+	if (bfsize < 0)
+		bfsize = 0;
+
+	if (bfsize < BUF_SIZE_16KiB)
+		bfsize = stmmac_set_bfsize(mtu, 0);
+
+	dma_conf->dma_buf_sz = bfsize;
+	/* Chose the tx/rx size from the already defined one in the
+	 * priv struct. (if defined)
+	 */
+	dma_conf->dma_tx_size = priv->dma_conf.dma_tx_size;
+	dma_conf->dma_rx_size = priv->dma_conf.dma_rx_size;
+
+	if (!dma_conf->dma_tx_size)
+		dma_conf->dma_tx_size = DMA_DEFAULT_TX_SIZE;
+	if (!dma_conf->dma_rx_size)
+		dma_conf->dma_rx_size = DMA_DEFAULT_RX_SIZE;
+
+	/* Earlier check for TBS */
+	for (chan = 0; chan < priv->plat->tx_queues_to_use; chan++) {
+		struct stmmac_tx_queue *tx_q = &dma_conf->tx_queue[chan];
+		int tbs_en = priv->plat->tx_queues_cfg[chan].tbs_en;
+
+		/* Setup per-TXQ tbs flag before TX descriptor alloc */
+		tx_q->tbs |= tbs_en ? STMMAC_TBS_AVAIL : 0;
+	}
+
+	ret = alloc_dma_desc_resources(priv, dma_conf);
+	if (ret < 0) {
+		netdev_err(priv->dev, "%s: DMA descriptors allocation failed\n",
+			   __func__);
+		goto alloc_error;
+	}
+
+	ret = init_dma_desc_rings(priv->dev, dma_conf, GFP_KERNEL);
+	if (ret < 0) {
+		netdev_err(priv->dev, "%s: DMA descriptors initialization failed\n",
+			   __func__);
+		goto init_error;
+	}
+
+	return dma_conf;
+
+init_error:
+	free_dma_desc_resources(priv, dma_conf);
+alloc_error:
+	kfree(dma_conf);
+	return ERR_PTR(ret);
+}
+
+/**
+ *  __stmmac_open - open entry point of the driver
  *  @dev : pointer to the device structure.
+ *  @dma_conf :  structure to take the dma data
  *  Description:
  *  This function is the open entry point of the driver.
  *  Return value:
  *  0 on success and an appropriate (-)ve integer as defined in errno.h
  *  file on failure.
  */
-static int stmmac_open(struct net_device *dev)
+static int __stmmac_open(struct net_device *dev,
+			 struct stmmac_dma_conf *dma_conf)
 {
 	struct stmmac_priv *priv = netdev_priv(dev);
 	int mode = priv->plat->phy_interface;
-	int bfsize = 0;
 	u32 chan;
 	int ret;
 
@@ -3725,45 +3862,10 @@ static int stmmac_open(struct net_device
 	memset(&priv->xstats, 0, sizeof(struct stmmac_extra_stats));
 	priv->xstats.threshold = tc;
 
-	bfsize = stmmac_set_16kib_bfsize(priv, dev->mtu);
-	if (bfsize < 0)
-		bfsize = 0;
-
-	if (bfsize < BUF_SIZE_16KiB)
-		bfsize = stmmac_set_bfsize(dev->mtu, priv->dma_conf.dma_buf_sz);
-
-	priv->dma_conf.dma_buf_sz = bfsize;
-	buf_sz = bfsize;
-
 	priv->rx_copybreak = STMMAC_RX_COPYBREAK;
 
-	if (!priv->dma_conf.dma_tx_size)
-		priv->dma_conf.dma_tx_size = DMA_DEFAULT_TX_SIZE;
-	if (!priv->dma_conf.dma_rx_size)
-		priv->dma_conf.dma_rx_size = DMA_DEFAULT_RX_SIZE;
-
-	/* Earlier check for TBS */
-	for (chan = 0; chan < priv->plat->tx_queues_to_use; chan++) {
-		struct stmmac_tx_queue *tx_q = &priv->dma_conf.tx_queue[chan];
-		int tbs_en = priv->plat->tx_queues_cfg[chan].tbs_en;
-
-		/* Setup per-TXQ tbs flag before TX descriptor alloc */
-		tx_q->tbs |= tbs_en ? STMMAC_TBS_AVAIL : 0;
-	}
-
-	ret = alloc_dma_desc_resources(priv);
-	if (ret < 0) {
-		netdev_err(priv->dev, "%s: DMA descriptors allocation failed\n",
-			   __func__);
-		goto dma_desc_error;
-	}
-
-	ret = init_dma_desc_rings(dev, GFP_KERNEL);
-	if (ret < 0) {
-		netdev_err(priv->dev, "%s: DMA descriptors initialization failed\n",
-			   __func__);
-		goto init_error;
-	}
+	buf_sz = dma_conf->dma_buf_sz;
+	memcpy(&priv->dma_conf, dma_conf, sizeof(*dma_conf));
 
 	if (priv->plat->serdes_powerup) {
 		ret = priv->plat->serdes_powerup(dev, priv->plat->bsp_priv);
@@ -3806,14 +3908,28 @@ irq_error:
 
 	stmmac_hw_teardown(dev);
 init_error:
-	free_dma_desc_resources(priv);
-dma_desc_error:
+	free_dma_desc_resources(priv, &priv->dma_conf);
 	phylink_disconnect_phy(priv->phylink);
 init_phy_error:
 	pm_runtime_put(priv->device);
 	return ret;
 }
 
+static int stmmac_open(struct net_device *dev)
+{
+	struct stmmac_priv *priv = netdev_priv(dev);
+	struct stmmac_dma_conf *dma_conf;
+	int ret;
+
+	dma_conf = stmmac_setup_dma_desc(priv, dev->mtu);
+	if (IS_ERR(dma_conf))
+		return PTR_ERR(dma_conf);
+
+	ret = __stmmac_open(dev, dma_conf);
+	kfree(dma_conf);
+	return ret;
+}
+
 static void stmmac_fpe_stop_wq(struct stmmac_priv *priv)
 {
 	set_bit(__FPE_REMOVING, &priv->fpe_task_state);
@@ -3860,7 +3976,7 @@ static int stmmac_release(struct net_dev
 	stmmac_stop_all_dma(priv);
 
 	/* Release and free the Rx/Tx resources */
-	free_dma_desc_resources(priv);
+	free_dma_desc_resources(priv, &priv->dma_conf);
 
 	/* Disable the MAC Rx/Tx */
 	stmmac_mac_set(priv, priv->ioaddr, false);
@@ -6383,7 +6499,7 @@ void stmmac_disable_rx_queue(struct stmm
 	spin_unlock_irqrestore(&ch->lock, flags);
 
 	stmmac_stop_rx_dma(priv, queue);
-	__free_dma_rx_desc_resources(priv, queue);
+	__free_dma_rx_desc_resources(priv, &priv->dma_conf, queue);
 }
 
 void stmmac_enable_rx_queue(struct stmmac_priv *priv, u32 queue)
@@ -6394,21 +6510,21 @@ void stmmac_enable_rx_queue(struct stmma
 	u32 buf_size;
 	int ret;
 
-	ret = __alloc_dma_rx_desc_resources(priv, queue);
+	ret = __alloc_dma_rx_desc_resources(priv, &priv->dma_conf, queue);
 	if (ret) {
 		netdev_err(priv->dev, "Failed to alloc RX desc.\n");
 		return;
 	}
 
-	ret = __init_dma_rx_desc_rings(priv, queue, GFP_KERNEL);
+	ret = __init_dma_rx_desc_rings(priv, &priv->dma_conf, queue, GFP_KERNEL);
 	if (ret) {
-		__free_dma_rx_desc_resources(priv, queue);
+		__free_dma_rx_desc_resources(priv, &priv->dma_conf, queue);
 		netdev_err(priv->dev, "Failed to init RX desc.\n");
 		return;
 	}
 
 	stmmac_reset_rx_queue(priv, queue);
-	stmmac_clear_rx_descriptors(priv, queue);
+	stmmac_clear_rx_descriptors(priv, &priv->dma_conf, queue);
 
 	stmmac_init_rx_chan(priv, priv->ioaddr, priv->plat->dma_cfg,
 			    rx_q->dma_rx_phy, rx_q->queue_index);
@@ -6446,7 +6562,7 @@ void stmmac_disable_tx_queue(struct stmm
 	spin_unlock_irqrestore(&ch->lock, flags);
 
 	stmmac_stop_tx_dma(priv, queue);
-	__free_dma_tx_desc_resources(priv, queue);
+	__free_dma_tx_desc_resources(priv, &priv->dma_conf, queue);
 }
 
 void stmmac_enable_tx_queue(struct stmmac_priv *priv, u32 queue)
@@ -6456,21 +6572,21 @@ void stmmac_enable_tx_queue(struct stmma
 	unsigned long flags;
 	int ret;
 
-	ret = __alloc_dma_tx_desc_resources(priv, queue);
+	ret = __alloc_dma_tx_desc_resources(priv, &priv->dma_conf, queue);
 	if (ret) {
 		netdev_err(priv->dev, "Failed to alloc TX desc.\n");
 		return;
 	}
 
-	ret = __init_dma_tx_desc_rings(priv, queue);
+	ret = __init_dma_tx_desc_rings(priv,  &priv->dma_conf, queue);
 	if (ret) {
-		__free_dma_tx_desc_resources(priv, queue);
+		__free_dma_tx_desc_resources(priv, &priv->dma_conf, queue);
 		netdev_err(priv->dev, "Failed to init TX desc.\n");
 		return;
 	}
 
 	stmmac_reset_tx_queue(priv, queue);
-	stmmac_clear_tx_descriptors(priv, queue);
+	stmmac_clear_tx_descriptors(priv, &priv->dma_conf, queue);
 
 	stmmac_init_tx_chan(priv, priv->ioaddr, priv->plat->dma_cfg,
 			    tx_q->dma_tx_phy, tx_q->queue_index);
@@ -6510,7 +6626,7 @@ void stmmac_xdp_release(struct net_devic
 	stmmac_stop_all_dma(priv);
 
 	/* Release and free the Rx/Tx resources */
-	free_dma_desc_resources(priv);
+	free_dma_desc_resources(priv, &priv->dma_conf);
 
 	/* Disable the MAC Rx/Tx */
 	stmmac_mac_set(priv, priv->ioaddr, false);
@@ -6535,14 +6651,14 @@ int stmmac_xdp_open(struct net_device *d
 	u32 chan;
 	int ret;
 
-	ret = alloc_dma_desc_resources(priv);
+	ret = alloc_dma_desc_resources(priv, &priv->dma_conf);
 	if (ret < 0) {
 		netdev_err(dev, "%s: DMA descriptors allocation failed\n",
 			   __func__);
 		goto dma_desc_error;
 	}
 
-	ret = init_dma_desc_rings(dev, GFP_KERNEL);
+	ret = init_dma_desc_rings(dev, &priv->dma_conf, GFP_KERNEL);
 	if (ret < 0) {
 		netdev_err(dev, "%s: DMA descriptors initialization failed\n",
 			   __func__);
@@ -6624,7 +6740,7 @@ irq_error:
 
 	stmmac_hw_teardown(dev);
 init_error:
-	free_dma_desc_resources(priv);
+	free_dma_desc_resources(priv, &priv->dma_conf);
 dma_desc_error:
 	return ret;
 }
@@ -7490,7 +7606,7 @@ int stmmac_resume(struct device *dev)
 	stmmac_reset_queues_param(priv);
 
 	stmmac_free_tx_skbufs(priv);
-	stmmac_clear_descriptors(priv);
+	stmmac_clear_descriptors(priv, &priv->dma_conf);
 
 	stmmac_hw_setup(ndev, false);
 	stmmac_init_coalesce(priv);
