--- /dev/null
+++ b/configs/mt7986a_jdcloud_re-cp-03_defconfig
@@ -0,0 +1,112 @@
+CONFIG_ARM=y
+CONFIG_SYS_HAS_NONCACHED_MEMORY=y
+CONFIG_POSITION_INDEPENDENT=y
+CONFIG_ARCH_MEDIATEK=y
+CONFIG_TEXT_BASE=0x41e00000
+CONFIG_SYS_MALLOC_F_LEN=0x4000
+CONFIG_NR_DRAM_BANKS=1
+CONFIG_ENV_SIZE=0x40000
+CONFIG_ENV_OFFSET=0x400000
+CONFIG_DEFAULT_DEVICE_TREE="mt7986a-jdcloud_re-cp-03"
+CONFIG_SYS_PROMPT="MT7986> "
+CONFIG_OF_LIBFDT_OVERLAY=y
+CONFIG_TARGET_MT7986=y
+CONFIG_PRE_CON_BUF_ADDR=0x4007EF00
+CONFIG_DEBUG_UART_BASE=0x11002000
+CONFIG_DEBUG_UART_CLOCK=40000000
+CONFIG_ENV_OFFSET_REDUND=0x440000
+CONFIG_SYS_LOAD_ADDR=0x46000000
+CONFIG_DEBUG_UART=y
+CONFIG_FIT=y
+CONFIG_BOOTDELAY=30
+CONFIG_AUTOBOOT_KEYED=y
+CONFIG_AUTOBOOT_MENU_SHOW=y
+CONFIG_DEFAULT_FDT_FILE="mediatek/mt7986a-jdcloud_re-cp-03.dtb"
+CONFIG_LOGLEVEL=7
+CONFIG_PRE_CONSOLE_BUFFER=y
+CONFIG_LOG=y
+CONFIG_BOARD_LATE_INIT=y
+CONFIG_HUSH_PARSER=y
+CONFIG_CMD_CPU=y
+CONFIG_CMD_LICENSE=y
+CONFIG_CMD_BOOTMENU=y
+CONFIG_CMD_ASKENV=y
+CONFIG_CMD_ERASEENV=y
+CONFIG_CMD_ENV_FLAGS=y
+CONFIG_CMD_STRINGS=y
+CONFIG_CMD_DM=y
+CONFIG_CMD_GPIO=y
+CONFIG_CMD_PWM=y
+CONFIG_CMD_GPT=y
+CONFIG_CMD_MMC=y
+CONFIG_CMD_PART=y
+CONFIG_CMD_DHCP=y
+CONFIG_CMD_TFTPSRV=y
+CONFIG_CMD_RARP=y
+CONFIG_CMD_PING=y
+CONFIG_CMD_CDP=y
+CONFIG_CMD_SNTP=y
+CONFIG_CMD_DNS=y
+CONFIG_CMD_LINK_LOCAL=y
+CONFIG_CMD_PXE=y
+CONFIG_CMD_CACHE=y
+CONFIG_CMD_PSTORE=y
+CONFIG_CMD_PSTORE_MEM_ADDR=0x42ff0000
+CONFIG_CMD_UUID=y
+CONFIG_CMD_HASH=y
+CONFIG_CMD_SMC=y
+CONFIG_CMD_EXT4=y
+CONFIG_CMD_FAT=y
+CONFIG_CMD_FS_GENERIC=y
+CONFIG_CMD_FS_UUID=y
+CONFIG_OF_EMBED=y
+CONFIG_ENV_OVERWRITE=y
+CONFIG_ENV_IS_IN_MMC=y
+CONFIG_SYS_REDUNDAND_ENVIRONMENT=y
+CONFIG_SYS_RELOC_GD_ENV_ADDR=y
+CONFIG_USE_DEFAULT_ENV_FILE=y
+CONFIG_DEFAULT_ENV_FILE="jdcloud_re-cp-03_env"
+CONFIG_ENV_VARS_UBOOT_RUNTIME_CONFIG=y
+CONFIG_VERSION_VARIABLE=y
+CONFIG_NET_RANDOM_ETHADDR=y
+CONFIG_NETCONSOLE=y
+CONFIG_USE_IPADDR=y
+CONFIG_IPADDR="192.168.1.1"
+CONFIG_USE_SERVERIP=y
+CONFIG_SERVERIP="192.168.1.254"
+CONFIG_REGMAP=y
+CONFIG_SYSCON=y
+CONFIG_BUTTON=y
+CONFIG_BUTTON_GPIO=y
+CONFIG_CLK=y
+CONFIG_GPIO_HOG=y
+CONFIG_LED=y
+CONFIG_LED_BLINK=y
+CONFIG_LED_GPIO=y
+CONFIG_SUPPORT_EMMC_BOOT=y
+CONFIG_MMC_HS200_SUPPORT=y
+CONFIG_MMC_MTK=y
+CONFIG_PHY_FIXED=y
+CONFIG_DM_MDIO=y
+CONFIG_MEDIATEK_ETH=y
+CONFIG_PHY=y
+CONFIG_PHY_MTK_TPHY=y
+CONFIG_PINCTRL=y
+CONFIG_PINCONF=y
+CONFIG_PINCTRL_MT7622=y
+CONFIG_PINCTRL_MT7986=y
+CONFIG_POWER_DOMAIN=y
+CONFIG_MTK_POWER_DOMAIN=y
+CONFIG_DM_REGULATOR=y
+CONFIG_DM_REGULATOR_FIXED=y
+CONFIG_DM_REGULATOR_GPIO=y
+CONFIG_DM_PWM=y
+CONFIG_PWM_MTK=y
+CONFIG_RAM=y
+CONFIG_SCSI=y
+CONFIG_DM_SCSI=y
+CONFIG_DM_SERIAL=y
+CONFIG_MTK_SERIAL=y
+CONFIG_ZSTD=y
+CONFIG_HEXDUMP=y
+CONFIG_LMB_MAX_REGIONS=64
--- /dev/null
+++ b/arch/arm/dts/mt7986a-jdcloud_re-cp-03.dts
@@ -0,0 +1,145 @@
+// SPDX-License-Identifier: GPL-2.0-or-later
+
+/dts-v1/;
+#include <dt-bindings/input/linux-event-codes.h>
+#include "mt7986.dtsi"
+#include <dt-bindings/gpio/gpio.h>
+
+/ {
+	#address-cells = <1>;
+	#size-cells = <1>;
+	model = "JDCloud RE-CP-03";
+	compatible = "mediatek,mt7986", "mediatek,mt7986-rfb";
+
+	chosen {
+		stdout-path = &uart0;
+		tick-timer = &timer0;
+	};
+
+	memory@40000000 {
+		device_type = "memory";
+		reg = <0x40000000 0x40000000>;
+	};
+
+	gpio-keys {
+		compatible = "gpio-keys";
+
+		button-joylink {
+			label = "joylink";
+			linux,code = <BTN_0>;
+			gpios = <&gpio 10 GPIO_ACTIVE_LOW>;
+		};
+
+		button-reset {
+			label = "reset";
+			linux,code = <KEY_RESTART>;
+			gpios = <&gpio 9 GPIO_ACTIVE_LOW>;
+		};
+	};
+
+	gpio-leds {
+		compatible = "gpio-leds";
+
+		led-0 {
+			label = "blue:status";
+			gpios = <&gpio 7 GPIO_ACTIVE_HIGH>;
+		};
+
+		red_led: led-1 {
+			label = "red:status";
+			gpios = <&gpio 11 GPIO_ACTIVE_HIGH>;
+		};
+
+		green_led: led-2 {
+			label = "green:status";
+			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
+		};
+	};
+
+	reg_1p8v: regulator-1p8v {
+		compatible = "regulator-fixed";
+		regulator-name = "fixed-1.8V";
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <1800000>;
+		regulator-boot-on;
+		regulator-always-on;
+	};
+
+	reg_3p3v: regulator-3p3v {
+		compatible = "regulator-fixed";
+		regulator-name = "fixed-3.3V";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-boot-on;
+		regulator-always-on;
+	};
+};
+
+&eth {
+	status = "okay";
+	mediatek,gmac-id = <0>;
+	phy-mode = "2500base-x";
+	mediatek,switch = "mt7531";
+	reset-gpios = <&gpio 5 GPIO_ACTIVE_HIGH>;
+
+	fixed-link {
+		speed = <2500>;
+		full-duplex;
+	};
+};
+
+&mmc0 {
+	bus-width = <8>;
+	cap-mmc-highspeed;
+	cap-mmc-hw-reset;
+	max-frequency = <200000000>;
+	non-removable;
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc0_pins_default>;
+	vmmc-supply = <&reg_3p3v>;
+	vqmmc-supply = <&reg_1p8v>;
+	status = "okay";
+};
+
+&pinctrl {
+	mmc0_pins_default: mmc0default {
+		mux {
+			function = "flash";
+			groups =  "emmc_51";
+		};
+
+		conf-cmd-dat {
+			pins = "EMMC_DATA_0", "EMMC_DATA_1", "EMMC_DATA_2",
+			       "EMMC_DATA_3", "EMMC_DATA_4", "EMMC_DATA_5",
+			       "EMMC_DATA_6", "EMMC_DATA_7", "EMMC_CMD";
+			input-enable;
+			drive-strength = <MTK_DRIVE_4mA>;
+			bias-pull-up = <MTK_PUPD_SET_R1R0_01>;
+		};
+
+		conf-clk {
+			pins = "EMMC_CK";
+			drive-strength = <MTK_DRIVE_6mA>;
+			bias-pull-down = <MTK_PUPD_SET_R1R0_10>;
+		};
+
+		conf-dsl {
+			pins = "EMMC_DSL";
+			bias-pull-down = <MTK_PUPD_SET_R1R0_10>;
+		};
+
+		conf-rst {
+			pins = "EMMC_RSTB";
+			drive-strength = <MTK_DRIVE_4mA>;
+			bias-pull-up = <MTK_PUPD_SET_R1R0_01>;
+		};
+	};
+};
+
+&uart0 {
+	status = "okay";
+};
+
+&watchdog {
+	status = "disabled";
+};
--- /dev/null
+++ b/jdcloud_re-cp-03_env
@@ -0,0 +1,55 @@
+ipaddr=192.168.1.1
+serverip=192.168.1.254
+loadaddr=0x46000000
+console=earlycon=uart8250,mmio32,0x11002000 console=ttyS0
+bootargs=root=/dev/mmcblk0p65
+bootcmd=if pstore check ; then run boot_recovery ; else run boot_emmc ; fi
+bootconf=config-1
+bootdelay=0
+bootfile=immortalwrt-mediatek-filogic-jdcloud_re-cp-03-initramfs-recovery.itb
+bootfile_bl2=immortalwrt-mediatek-filogic-jdcloud_re-cp-03-preloader.bin
+bootfile_fip=immortalwrt-mediatek-filogic-jdcloud_re-cp-03-bl31-uboot.fip
+bootfile_upg=immortalwrt-mediatek-filogic-jdcloud_re-cp-03-squashfs-sysupgrade.itb
+bootled_pwr=red:status
+bootled_rec=blue:status
+bootmenu_confirm_return=askenv - Press ENTER to return to menu ; bootmenu 60
+bootmenu_default=0
+bootmenu_delay=0
+bootmenu_title=      [0;34m( ( ( [1;39mOpenWrt[0;34m ) ) )
+bootmenu_0=Initialize environment.=run _firstboot
+bootmenu_0d=Run default boot command.=run boot_default
+bootmenu_1=Boot system via TFTP.=run boot_tftp ; run bootmenu_confirm_return
+bootmenu_2=Boot production system from eMMC.=run boot_production ; run bootmenu_confirm_return
+bootmenu_3=Boot recovery system from eMMC.=run boot_recovery ; run bootmenu_confirm_return
+bootmenu_4=Load production system via TFTP then write to eMMC.=setenv noboot 1 ; setenv replacevol 1 ; run boot_tftp_production ; setenv noboot ; setenv replacevol ; run bootmenu_confirm_return
+bootmenu_5=Load recovery system via TFTP then write to eMMC.=setenv noboot 1 ; setenv replacevol 1 ; run boot_tftp_recovery ; setenv noboot ; setenv replacevol ; run bootmenu_confirm_return
+bootmenu_6=[31mLoad BL31+U-Boot FIP via TFTP then write to eMMC.[0m=run boot_tftp_write_fip ; run bootmenu_confirm_return
+bootmenu_7=[31mLoad BL2 preloader via TFTP then write to eMMC.[0m=run boot_tftp_write_bl2 ; run bootmenu_confirm_return
+bootmenu_8=Reboot.=reset
+bootmenu_9=Reset all settings to factory defaults.=run reset_factory ; reset
+boot_first=if button reset ; then led $bootled_rec on ; run boot_tftp_recovery ; setenv flag_recover 1 ; run boot_default ; fi ; bootmenu
+boot_default=if env exists flag_recover ; then else run bootcmd ; fi ; run boot_recovery ; setenv replacevol 1 ; run boot_tftp_forever
+boot_production=led $bootled_pwr on ; run emmc_read_production && bootm $loadaddr#$bootconf ; led $bootled_pwr off
+boot_recovery=led $bootled_rec on ; run emmc_read_recovery && bootm $loadaddr#$bootconf ; led $bootled_rec off
+boot_emmc=run boot_production ; run boot_recovery
+boot_tftp_forever=led $bootled_rec on ; while true ; do run boot_tftp_recovery ; sleep 1 ; done
+boot_tftp_production=tftpboot $loadaddr $bootfile_upg && env exists replacevol && iminfo $loadaddr && run emmc_write_production ; if env exists noboot ; then else bootm $loadaddr#$bootconf ; fi
+boot_tftp_recovery=tftpboot $loadaddr $bootfile && env exists replacevol && iminfo $loadaddr && run emmc_write_recovery ; if env exists noboot ; then else bootm $loadaddr#$bootconf ; fi
+boot_tftp_write_fip=tftpboot $loadaddr $bootfile_fip && run emmc_write_fip
+boot_tftp_write_bl2=tftpboot $loadaddr $bootfile_bl2 && run emmc_write_bl2
+boot_tftp=tftpboot $loadaddr $bootfile && bootm $loadaddr#$bootconf
+mmc_write_vol=imszb $loadaddr image_size && test 0x$image_size -le 0x$part_size && mmc erase 0x$part_addr 0x$image_size && mmc write $loadaddr 0x$part_addr 0x$image_size
+mmc_read_vol=mmc read $loadaddr $part_addr 0x100 && imszb $loadaddr image_size && test 0x$image_size -le 0x$part_size && mmc read $loadaddr 0x$part_addr 0x$image_size && setexpr filesize $image_size * 0x200
+part_default=production
+part_recovery=recovery
+reset_factory=eraseenv && reset
+emmc_read_production=part start mmc 0 $part_default part_addr && part size mmc 0 $part_default part_size && run mmc_read_vol
+emmc_read_recovery=part start mmc 0 $part_recovery part_addr && part size mmc 0 $part_recovery part_size && run mmc_read_vol
+emmc_write_bl2=mmc partconf 0 1 1 1 && mmc erase 0x0 0x400 && mmc write $fileaddr 0x0 0x400 ; mmc partconf 0 1 1 0
+emmc_write_fip=mmc erase 0x3400 0x2000 && mmc write $fileaddr 0x3400 0x2000 && mmc erase 0x2000 0x800
+emmc_write_production=part start mmc 0 $part_default part_addr && part size mmc 0 $part_default part_size && run mmc_write_vol
+emmc_write_recovery=part start mmc 0 $part_recovery part_addr && part size mmc 0 $part_recovery part_size && run mmc_write_vol
+_init_env=setenv _init_env ; setenv _create_env ; saveenv ; saveenv
+_firstboot=setenv _firstboot ; run _switch_to_menu ; run _init_env ; run boot_first
+_switch_to_menu=setenv _switch_to_menu ; setenv bootdelay 3 ; setenv bootmenu_delay 3 ; setenv bootmenu_0 $bootmenu_0d ; setenv bootmenu_0d ; run _bootmenu_update_title
+_bootmenu_update_title=setenv _bootmenu_update_title ; setenv bootmenu_title "$bootmenu_title       [33m$ver[0m"
