From ba5dfa2fd8d0aed4e4b6f650ba9e8ea7cdd6ead1 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Tue, 15 Feb 2022 07:36:39 +0100
Subject: [PATCH] arm64: dts: broadcom: bcm4908: add I2C block
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

BCM4908 uses the same I2C hw as BCM63xx / BCM67xx / BCM68xx SoCs.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Signed-off-by: Florian Fainelli <f.fainelli@gmail.com>
---
 arch/arm64/boot/dts/broadcom/bcmbca/bcm4908.dtsi | 9 +++++++++
 1 file changed, 9 insertions(+)

--- a/arch/arm64/boot/dts/broadcom/bcmbca/bcm4908.dtsi
+++ b/arch/arm64/boot/dts/broadcom/bcmbca/bcm4908.dtsi
@@ -458,6 +458,15 @@
 			};
 		};
 
+		i2c@2100 {
+			compatible = "brcm,brcmper-i2c";
+			reg = <0x2100 0x58>;
+			clock-frequency = <97500>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&pins_i2c_a>;
+			status = "disabled";
+		};
+
 		misc@2600 {
 			compatible = "brcm,misc", "simple-mfd";
 			reg = <0x2600 0xe4>;
