From 15a84d1c44ae8c1451c265ee60500588a24e8cd6 Mon Sep 17 00:00:00 2001
From: Daniel Golle <daniel@makrotopia.org>
Date: Tue, 22 Aug 2023 17:32:03 +0100
Subject: [PATCH 111/250] net: ethernet: mtk_eth_soc: add reset bits for MT7988

Add bits needed to reset the frame engine on MT7988.

Fixes: 445eb6448ed3 ("net: ethernet: mtk_eth_soc: add basic support for MT7988 SoC")
Signed-off-by: Daniel Golle <daniel@makrotopia.org>
Link: https://lore.kernel.org/r/89b6c38380e7a3800c1362aa7575600717bc7543.1692721443.git.daniel@makrotopia.org
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/ethernet/mediatek/mtk_eth_soc.c | 76 +++++++++++++++------
 drivers/net/ethernet/mediatek/mtk_eth_soc.h | 16 +++--
 2 files changed, 68 insertions(+), 24 deletions(-)

--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.c
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.c
@@ -3541,19 +3541,34 @@ static void mtk_hw_reset(struct mtk_eth
 {
 	u32 val;
 
-	if (mtk_is_netsys_v2_or_greater(eth)) {
+	if (mtk_is_netsys_v2_or_greater(eth))
 		regmap_write(eth->ethsys, ETHSYS_FE_RST_CHK_IDLE_EN, 0);
+
+	if (mtk_is_netsys_v3_or_greater(eth)) {
+		val = RSTCTRL_PPE0_V3;
+
+		if (MTK_HAS_CAPS(eth->soc->caps, MTK_RSTCTRL_PPE1))
+			val |= RSTCTRL_PPE1_V3;
+
+		if (MTK_HAS_CAPS(eth->soc->caps, MTK_RSTCTRL_PPE2))
+			val |= RSTCTRL_PPE2;
+
+		val |= RSTCTRL_WDMA0 | RSTCTRL_WDMA1 | RSTCTRL_WDMA2;
+	} else if (mtk_is_netsys_v2_or_greater(eth)) {
 		val = RSTCTRL_PPE0_V2;
+
+		if (MTK_HAS_CAPS(eth->soc->caps, MTK_RSTCTRL_PPE1))
+			val |= RSTCTRL_PPE1;
 	} else {
 		val = RSTCTRL_PPE0;
 	}
 
-	if (MTK_HAS_CAPS(eth->soc->caps, MTK_RSTCTRL_PPE1))
-		val |= RSTCTRL_PPE1;
-
 	ethsys_reset(eth, RSTCTRL_ETH | RSTCTRL_FE | val);
 
-	if (mtk_is_netsys_v2_or_greater(eth))
+	if (mtk_is_netsys_v3_or_greater(eth))
+		regmap_write(eth->ethsys, ETHSYS_FE_RST_CHK_IDLE_EN,
+			     0x6f8ff);
+	else if (mtk_is_netsys_v2_or_greater(eth))
 		regmap_write(eth->ethsys, ETHSYS_FE_RST_CHK_IDLE_EN,
 			     0x3ffffff);
 }
@@ -3579,13 +3594,21 @@ static void mtk_hw_warm_reset(struct mtk
 		return;
 	}
 
-	if (mtk_is_netsys_v2_or_greater(eth))
+	if (mtk_is_netsys_v3_or_greater(eth)) {
+		rst_mask = RSTCTRL_ETH | RSTCTRL_PPE0_V3;
+		if (MTK_HAS_CAPS(eth->soc->caps, MTK_RSTCTRL_PPE1))
+			rst_mask |= RSTCTRL_PPE1_V3;
+		if (MTK_HAS_CAPS(eth->soc->caps, MTK_RSTCTRL_PPE2))
+			rst_mask |= RSTCTRL_PPE2;
+
+		rst_mask |= RSTCTRL_WDMA0 | RSTCTRL_WDMA1 | RSTCTRL_WDMA2;
+	} else if (mtk_is_netsys_v2_or_greater(eth)) {
 		rst_mask = RSTCTRL_ETH | RSTCTRL_PPE0_V2;
-	else
+		if (MTK_HAS_CAPS(eth->soc->caps, MTK_RSTCTRL_PPE1))
+			rst_mask |= RSTCTRL_PPE1;
+	} else {
 		rst_mask = RSTCTRL_ETH | RSTCTRL_PPE0;
-
-	if (MTK_HAS_CAPS(eth->soc->caps, MTK_RSTCTRL_PPE1))
-		rst_mask |= RSTCTRL_PPE1;
+	}
 
 	regmap_update_bits(eth->ethsys, ETHSYS_RSTCTRL, rst_mask, rst_mask);
 
@@ -3937,11 +3960,17 @@ static void mtk_prepare_for_reset(struct
 	u32 val;
 	int i;
 
-	/* disabe FE P3 and P4 */
-	val = mtk_r32(eth, MTK_FE_GLO_CFG) | MTK_FE_LINK_DOWN_P3;
-	if (MTK_HAS_CAPS(eth->soc->caps, MTK_RSTCTRL_PPE1))
-		val |= MTK_FE_LINK_DOWN_P4;
-	mtk_w32(eth, val, MTK_FE_GLO_CFG);
+	/* set FE PPE ports link down */
+	for (i = MTK_GMAC1_ID;
+	     i <= (mtk_is_netsys_v3_or_greater(eth) ? MTK_GMAC3_ID : MTK_GMAC2_ID);
+	     i += 2) {
+		val = mtk_r32(eth, MTK_FE_GLO_CFG(i)) | MTK_FE_LINK_DOWN_P(PSE_PPE0_PORT);
+		if (MTK_HAS_CAPS(eth->soc->caps, MTK_RSTCTRL_PPE1))
+			val |= MTK_FE_LINK_DOWN_P(PSE_PPE1_PORT);
+		if (MTK_HAS_CAPS(eth->soc->caps, MTK_RSTCTRL_PPE2))
+			val |= MTK_FE_LINK_DOWN_P(PSE_PPE2_PORT);
+		mtk_w32(eth, val, MTK_FE_GLO_CFG(i));
+	}
 
 	/* adjust PPE configurations to prepare for reset */
 	for (i = 0; i < ARRAY_SIZE(eth->ppe); i++)
@@ -4002,11 +4031,18 @@ static void mtk_pending_work(struct work
 		}
 	}
 
-	/* enabe FE P3 and P4 */
-	val = mtk_r32(eth, MTK_FE_GLO_CFG) & ~MTK_FE_LINK_DOWN_P3;
-	if (MTK_HAS_CAPS(eth->soc->caps, MTK_RSTCTRL_PPE1))
-		val &= ~MTK_FE_LINK_DOWN_P4;
-	mtk_w32(eth, val, MTK_FE_GLO_CFG);
+	/* set FE PPE ports link up */
+	for (i = MTK_GMAC1_ID;
+	     i <= (mtk_is_netsys_v3_or_greater(eth) ? MTK_GMAC3_ID : MTK_GMAC2_ID);
+	     i += 2) {
+		val = mtk_r32(eth, MTK_FE_GLO_CFG(i)) & ~MTK_FE_LINK_DOWN_P(PSE_PPE0_PORT);
+		if (MTK_HAS_CAPS(eth->soc->caps, MTK_RSTCTRL_PPE1))
+			val &= ~MTK_FE_LINK_DOWN_P(PSE_PPE1_PORT);
+		if (MTK_HAS_CAPS(eth->soc->caps, MTK_RSTCTRL_PPE2))
+			val &= ~MTK_FE_LINK_DOWN_P(PSE_PPE2_PORT);
+
+		mtk_w32(eth, val, MTK_FE_GLO_CFG(i));
+	}
 
 	clear_bit(MTK_RESETTING, &eth->state);
 
--- a/drivers/net/ethernet/mediatek/mtk_eth_soc.h
+++ b/drivers/net/ethernet/mediatek/mtk_eth_soc.h
@@ -76,9 +76,8 @@
 #define	MTK_HW_LRO_SDL_REMAIN_ROOM	1522
 
 /* Frame Engine Global Configuration */
-#define MTK_FE_GLO_CFG		0x00
-#define MTK_FE_LINK_DOWN_P3	BIT(11)
-#define MTK_FE_LINK_DOWN_P4	BIT(12)
+#define MTK_FE_GLO_CFG(x)	(((x) == MTK_GMAC3_ID) ? 0x24 : 0x00)
+#define MTK_FE_LINK_DOWN_P(x)	BIT(((x) + 8) % 16)
 
 /* Frame Engine Global Reset Register */
 #define MTK_RST_GL		0x04
@@ -519,9 +518,15 @@
 /* ethernet reset control register */
 #define ETHSYS_RSTCTRL			0x34
 #define RSTCTRL_FE			BIT(6)
+#define RSTCTRL_WDMA0			BIT(24)
+#define RSTCTRL_WDMA1			BIT(25)
+#define RSTCTRL_WDMA2			BIT(26)
 #define RSTCTRL_PPE0			BIT(31)
 #define RSTCTRL_PPE0_V2			BIT(30)
 #define RSTCTRL_PPE1			BIT(31)
+#define RSTCTRL_PPE0_V3			BIT(29)
+#define RSTCTRL_PPE1_V3			BIT(30)
+#define RSTCTRL_PPE2			BIT(31)
 #define RSTCTRL_ETH			BIT(23)
 
 /* ethernet reset check idle register */
@@ -928,6 +933,7 @@ enum mkt_eth_capabilities {
 	MTK_QDMA_BIT,
 	MTK_SOC_MT7628_BIT,
 	MTK_RSTCTRL_PPE1_BIT,
+	MTK_RSTCTRL_PPE2_BIT,
 	MTK_U3_COPHY_V2_BIT,
 
 	/* MUX BITS*/
@@ -962,6 +968,7 @@ enum mkt_eth_capabilities {
 #define MTK_QDMA		BIT_ULL(MTK_QDMA_BIT)
 #define MTK_SOC_MT7628		BIT_ULL(MTK_SOC_MT7628_BIT)
 #define MTK_RSTCTRL_PPE1	BIT_ULL(MTK_RSTCTRL_PPE1_BIT)
+#define MTK_RSTCTRL_PPE2	BIT_ULL(MTK_RSTCTRL_PPE2_BIT)
 #define MTK_U3_COPHY_V2		BIT_ULL(MTK_U3_COPHY_V2_BIT)
 
 #define MTK_ETH_MUX_GDM1_TO_GMAC1_ESW		\
@@ -1044,7 +1051,8 @@ enum mkt_eth_capabilities {
 		      MTK_MUX_GMAC12_TO_GEPHY_SGMII | MTK_QDMA | \
 		      MTK_RSTCTRL_PPE1)
 
-#define MT7988_CAPS  (MTK_GDM1_ESW | MTK_QDMA | MTK_RSTCTRL_PPE1)
+#define MT7988_CAPS  (MTK_GDM1_ESW | MTK_QDMA | MTK_RSTCTRL_PPE1 | \
+		      MTK_RSTCTRL_PPE2)
 
 struct mtk_tx_dma_desc_info {
 	dma_addr_t	addr;
