From f63ea127643a605da97090ce585fdd7c2d17fa42 Mon Sep 17 00:00:00 2001
From: Robert Marko <robert.marko@sartura.hr>
Date: Mon, 14 Dec 2020 13:35:35 +0100
Subject: [PATCH] mmc: sdhci-msm: use sdhci_set_clock

When using sdhci_msm_set_clock clock setting will fail, so lets
use the generic sdhci_set_clock.

Signed-off-by: Robert Marko <robert.marko@sartura.hr>
---
 drivers/mmc/host/sdhci-msm.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/mmc/host/sdhci-msm.c
+++ b/drivers/mmc/host/sdhci-msm.c
@@ -2447,7 +2447,7 @@ MODULE_DEVICE_TABLE(of, sdhci_msm_dt_mat
 
 static const struct sdhci_ops sdhci_msm_ops = {
 	.reset = sdhci_msm_reset,
-	.set_clock = sdhci_msm_set_clock,
+	.set_clock = sdhci_set_clock,
 	.get_min_clock = sdhci_msm_get_min_clock,
 	.get_max_clock = sdhci_msm_get_max_clock,
 	.set_bus_width = sdhci_set_bus_width,
