From 083e5464b828cfbcb8c2a38a776267ce575d157d Mon Sep 17 00:00:00 2001
From: David Plowman <david.plowman@raspberrypi.com>
Date: Thu, 21 Oct 2021 14:45:07 +0100
Subject: [PATCH] media: i2c: imx519: Sensor should report RAW color
 space

Tested on Raspberry Pi running libcamera.

Signed-off-by: David Plowman <david.plowman@raspberrypi.com>
---
 drivers/media/i2c/imx519.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/media/i2c/imx519.c
+++ b/drivers/media/i2c/imx519.c
@@ -1317,7 +1317,7 @@ static int imx519_enum_frame_size(struct
 
 static void imx519_reset_colorspace(struct v4l2_mbus_framefmt *fmt)
 {
-	fmt->colorspace = V4L2_COLORSPACE_SRGB;
+	fmt->colorspace = V4L2_COLORSPACE_RAW;
 	fmt->ycbcr_enc = V4L2_MAP_YCBCR_ENC_DEFAULT(fmt->colorspace);
 	fmt->quantization = V4L2_MAP_QUANTIZATION_DEFAULT(true,
 							  fmt->colorspace,
