[ "$ACTION" == "add" ] || exit 0

PHYNBR=${DEVPATH##*/phy}

[ -n $PHYNBR ] || exit 0

. /lib/functions.sh
. /lib/functions/system.sh

board=$(board_name)

case "$board" in
	bananapi,bpi-r64)
		[ "$PHYNBR" = "0" ] && macaddr_add $(cat /sys/class/net/eth0/address) 2 > /sys${DEVPATH}/macaddress
		;;
	buffalo,wsr-3200ax4s)
		basemac=$(mtd_get_mac_ascii board_data "mac")
		[ "$PHYNBR" = "0" ] && macaddr_add $basemac 1 > /sys${DEVPATH}/macaddress
		[ "$PHYNBR" = "1" ] && macaddr_add $basemac 8 > /sys${DEVPATH}/macaddress
		;;
	dlink,eagle-pro-ai-m32-a1)
		[ "$PHYNBR" = "0" ] && macaddr_add $(cat /sys/class/net/eth0/address) 2 > /sys${DEVPATH}/macaddress
		[ "$PHYNBR" = "1" ] && macaddr_add $(cat /sys/class/net/eth0/address) 3 > /sys${DEVPATH}/macaddress
		;;
	reyee,ax3200-e5|\
	ruijie,rg-ew3200gx-pro)
		[ "$PHYNBR" = "0" ] && macaddr_add $(get_mac_label) 3 > /sys${DEVPATH}/macaddress
		[ "$PHYNBR" = "1" ] && macaddr_add $(get_mac_label) 2 > /sys${DEVPATH}/macaddress
		;;
esac
