From 859df5cf6ff07a9c930be4681284346aa73dd1fb Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Ar=C4=B1n=C3=A7=20=C3=9CNAL?= <arinc.unal@arinc9.com>
Date: Fri, 1 Mar 2024 12:43:01 +0200
Subject: [PATCH 23/30] net: dsa: mt7530: get rid of
 priv->info->cpu_port_config()
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

priv->info->cpu_port_config() is used for MT7531 and the switch on the
MT7988 SoC. It sets up the ports described as a CPU port earlier than the
phylink code path would do.

This function is useless as:
- Configuring the MACs can be done from the phylink_mac_config code path
  instead.
- All the link configuration it does on the CPU ports are later undone with
  the port_enable, phylink_mac_config, and then phylink_mac_link_up code
  path [1].

priv->p5_interface and priv->p6_interface were being used to prevent
configuring the MACs from the phylink_mac_config code path. Remove them now
that they hold no purpose.

Remove priv->info->cpu_port_config(). On mt753x_phylink_mac_config, switch
to if statements to simplify the code.

Remove the overwriting of the speed and duplex interfaces for certain
interface modes. Phylink already provides the speed and duplex variables
with proper values. Phylink already sets the max speed of TRGMII to
SPEED_1000. Add SPEED_2500 for PHY_INTERFACE_MODE_2500BASEX to where the
speed and EEE bits are set instead.

On the switch on the MT7988 SoC, PHY_INTERFACE_MODE_INTERNAL is being used
to describe the interface mode of the 10G MAC, which is of port 6. On
mt7988_cpu_port_config() PMCR_FORCE_SPEED_1000 was set via the
PMCR_CPU_PORT_SETTING() mask. Add SPEED_10000 case to where the speed bits
are set to cover this. No need to add it to where the EEE bits are set as
the "MT7988A Wi-Fi 7 Generation Router Platform: Datasheet (Open Version)
v0.1" document shows that these bits don't exist on the MT7530_PMCR_P(6)
register.

Remove the definition of PMCR_CPU_PORT_SETTING() now that it holds no
purpose.

Change mt753x_cpu_port_enable() to void now that there're no error cases
left.

Link: https://lore.kernel.org/netdev/ZHy2jQLesdYFMQtO@shell.armlinux.org.uk/ [1]
Suggested-by: Russell King (Oracle) <linux@armlinux.org.uk>
Signed-off-by: Arınç ÜNAL <arinc.unal@arinc9.com>
Signed-off-by: Paolo Abeni <pabeni@redhat.com>
---
 drivers/net/dsa/mt7530.c | 114 +++------------------------------------
 drivers/net/dsa/mt7530.h |  11 ----
 2 files changed, 7 insertions(+), 118 deletions(-)

--- a/drivers/net/dsa/mt7530.c
+++ b/drivers/net/dsa/mt7530.c
@@ -1002,18 +1002,10 @@ mt753x_trap_frames(struct mt7530_priv *p
 		   MT753X_BPDU_CPU_ONLY);
 }
 
-static int
+static void
 mt753x_cpu_port_enable(struct dsa_switch *ds, int port)
 {
 	struct mt7530_priv *priv = ds->priv;
-	int ret;
-
-	/* Setup max capability of CPU port at first */
-	if (priv->info->cpu_port_config) {
-		ret = priv->info->cpu_port_config(ds, port);
-		if (ret)
-			return ret;
-	}
 
 	/* Enable Mediatek header mode on the cpu port */
 	mt7530_write(priv, MT7530_PVC_P(port),
@@ -1039,8 +1031,6 @@ mt753x_cpu_port_enable(struct dsa_switch
 	/* Set to fallback mode for independent VLAN learning */
 	mt7530_rmw(priv, MT7530_PCR_P(port), PCR_PORT_VLAN_MASK,
 		   MT7530_PORT_FALLBACK_MODE);
-
-	return 0;
 }
 
 static int
@@ -2297,8 +2287,6 @@ mt7530_setup(struct dsa_switch *ds)
 	val |= MHWTRAP_MANUAL;
 	mt7530_write(priv, MT7530_MHWTRAP, val);
 
-	priv->p6_interface = PHY_INTERFACE_MODE_NA;
-
 	mt753x_trap_frames(priv);
 
 	/* Enable and reset MIB counters */
@@ -2313,9 +2301,7 @@ mt7530_setup(struct dsa_switch *ds)
 		mt7530_set(priv, MT7530_PSC_P(i), SA_DIS);
 
 		if (dsa_is_cpu_port(ds, i)) {
-			ret = mt753x_cpu_port_enable(ds, i);
-			if (ret)
-				return ret;
+			mt753x_cpu_port_enable(ds, i);
 		} else {
 			mt7530_port_disable(ds, i);
 
@@ -2419,9 +2405,7 @@ mt7531_setup_common(struct dsa_switch *d
 		mt7530_set(priv, MT7531_DBG_CNT(i), MT7531_DIS_CLR);
 
 		if (dsa_is_cpu_port(ds, i)) {
-			ret = mt753x_cpu_port_enable(ds, i);
-			if (ret)
-				return ret;
+			mt753x_cpu_port_enable(ds, i);
 		} else {
 			mt7530_port_disable(ds, i);
 
@@ -2510,10 +2494,6 @@ mt7531_setup(struct dsa_switch *ds)
 	mt7530_rmw(priv, MT7531_GPIO_MODE0, MT7531_GPIO0_MASK,
 		   MT7531_GPIO0_INTERRUPT);
 
-	/* Let phylink decide the interface later. */
-	priv->p5_interface = PHY_INTERFACE_MODE_NA;
-	priv->p6_interface = PHY_INTERFACE_MODE_NA;
-
 	/* Enable PHY core PLL, since phy_device has not yet been created
 	 * provided for phy_[read,write]_mmd_indirect is called, we provide
 	 * our own mt7531_ind_mmd_phy_[read,write] to complete this
@@ -2725,26 +2705,9 @@ mt753x_phylink_mac_config(struct dsa_swi
 	struct mt7530_priv *priv = ds->priv;
 	u32 mcr_cur, mcr_new;
 
-	switch (port) {
-	case 5:
-		if (priv->p5_interface == state->interface)
-			break;
-
+	if (port == 5 || port == 6)
 		mt753x_mac_config(ds, port, mode, state);
 
-		if (priv->p5_intf_sel != P5_DISABLED)
-			priv->p5_interface = state->interface;
-		break;
-	case 6:
-		if (priv->p6_interface == state->interface)
-			break;
-
-		mt753x_mac_config(ds, port, mode, state);
-
-		priv->p6_interface = state->interface;
-		break;
-	}
-
 	mcr_cur = mt7530_read(priv, MT7530_PMCR_P(port));
 	mcr_new = mcr_cur;
 	mcr_new &= ~PMCR_LINK_SETTINGS_MASK;
@@ -2780,17 +2743,10 @@ static void mt753x_phylink_mac_link_up(s
 
 	mcr = PMCR_RX_EN | PMCR_TX_EN | PMCR_FORCE_LNK;
 
-	/* MT753x MAC works in 1G full duplex mode for all up-clocked
-	 * variants.
-	 */
-	if (interface == PHY_INTERFACE_MODE_TRGMII ||
-	    (phy_interface_mode_is_8023z(interface))) {
-		speed = SPEED_1000;
-		duplex = DUPLEX_FULL;
-	}
-
 	switch (speed) {
 	case SPEED_1000:
+	case SPEED_2500:
+	case SPEED_10000:
 		mcr |= PMCR_FORCE_SPEED_1000;
 		break;
 	case SPEED_100:
@@ -2808,6 +2764,7 @@ static void mt753x_phylink_mac_link_up(s
 	if (mode == MLO_AN_PHY && phydev && phy_init_eee(phydev, false) >= 0) {
 		switch (speed) {
 		case SPEED_1000:
+		case SPEED_2500:
 			mcr |= PMCR_FORCE_EEE1G;
 			break;
 		case SPEED_100:
@@ -2819,61 +2776,6 @@ static void mt753x_phylink_mac_link_up(s
 	mt7530_set(priv, MT7530_PMCR_P(port), mcr);
 }
 
-static int
-mt7531_cpu_port_config(struct dsa_switch *ds, int port)
-{
-	struct mt7530_priv *priv = ds->priv;
-	phy_interface_t interface;
-	int speed;
-
-	switch (port) {
-	case 5:
-		if (!priv->p5_sgmii)
-			interface = PHY_INTERFACE_MODE_RGMII;
-		else
-			interface = PHY_INTERFACE_MODE_2500BASEX;
-
-		priv->p5_interface = interface;
-		break;
-	case 6:
-		interface = PHY_INTERFACE_MODE_2500BASEX;
-
-		priv->p6_interface = interface;
-		break;
-	default:
-		return -EINVAL;
-	}
-
-	if (interface == PHY_INTERFACE_MODE_2500BASEX)
-		speed = SPEED_2500;
-	else
-		speed = SPEED_1000;
-
-	mt7531_mac_config(ds, port, MLO_AN_FIXED, interface);
-
-	mt7530_write(priv, MT7530_PMCR_P(port),
-		     PMCR_CPU_PORT_SETTING(priv->id));
-	mt753x_phylink_mac_link_up(ds, port, MLO_AN_FIXED, interface, NULL,
-				   speed, DUPLEX_FULL, true, true);
-
-	return 0;
-}
-
-static int
-mt7988_cpu_port_config(struct dsa_switch *ds, int port)
-{
-	struct mt7530_priv *priv = ds->priv;
-
-	mt7530_write(priv, MT7530_PMCR_P(port),
-		     PMCR_CPU_PORT_SETTING(priv->id));
-
-	mt753x_phylink_mac_link_up(ds, port, MLO_AN_FIXED,
-				   PHY_INTERFACE_MODE_INTERNAL, NULL,
-				   SPEED_10000, DUPLEX_FULL, true, true);
-
-	return 0;
-}
-
 static void mt753x_phylink_get_caps(struct dsa_switch *ds, int port,
 				    struct phylink_config *config)
 {
@@ -3132,7 +3034,6 @@ const struct mt753x_info mt753x_table[]
 		.phy_write_c22 = mt7531_ind_c22_phy_write,
 		.phy_read_c45 = mt7531_ind_c45_phy_read,
 		.phy_write_c45 = mt7531_ind_c45_phy_write,
-		.cpu_port_config = mt7531_cpu_port_config,
 		.mac_port_get_caps = mt7531_mac_port_get_caps,
 		.mac_port_config = mt7531_mac_config,
 	},
@@ -3144,7 +3045,6 @@ const struct mt753x_info mt753x_table[]
 		.phy_write_c22 = mt7531_ind_c22_phy_write,
 		.phy_read_c45 = mt7531_ind_c45_phy_read,
 		.phy_write_c45 = mt7531_ind_c45_phy_write,
-		.cpu_port_config = mt7988_cpu_port_config,
 		.mac_port_get_caps = mt7988_mac_port_get_caps,
 	},
 };
--- a/drivers/net/dsa/mt7530.h
+++ b/drivers/net/dsa/mt7530.h
@@ -331,13 +331,6 @@ enum mt7530_vlan_port_acc_frm {
 					 PMCR_TX_FC_EN | PMCR_RX_FC_EN | \
 					 PMCR_FORCE_FDX | PMCR_FORCE_LNK | \
 					 PMCR_FORCE_EEE1G | PMCR_FORCE_EEE100)
-#define  PMCR_CPU_PORT_SETTING(id)	(PMCR_FORCE_MODE_ID((id)) | \
-					 PMCR_IFG_XMIT(1) | PMCR_MAC_MODE | \
-					 PMCR_BACKOFF_EN | PMCR_BACKPR_EN | \
-					 PMCR_TX_EN | PMCR_RX_EN | \
-					 PMCR_TX_FC_EN | PMCR_RX_FC_EN | \
-					 PMCR_FORCE_SPEED_1000 | \
-					 PMCR_FORCE_FDX | PMCR_FORCE_LNK)
 
 #define MT7530_PMEEECR_P(x)		(0x3004 + (x) * 0x100)
 #define  WAKEUP_TIME_1000(x)		(((x) & 0xFF) << 24)
@@ -744,7 +737,6 @@ struct mt753x_info {
 			    int regnum);
 	int (*phy_write_c45)(struct mt7530_priv *priv, int port, int devad,
 			     int regnum, u16 val);
-	int (*cpu_port_config)(struct dsa_switch *ds, int port);
 	void (*mac_port_get_caps)(struct dsa_switch *ds, int port,
 				  struct phylink_config *config);
 	void (*mac_port_validate)(struct dsa_switch *ds, int port,
@@ -770,7 +762,6 @@ struct mt753x_info {
  * @ports:		Holding the state among ports
  * @reg_mutex:		The lock for protecting among process accessing
  *			registers
- * @p6_interface	Holding the current port 6 interface
  * @p5_intf_sel:	Holding the current port 5 interface select
  * @p5_sgmii:		Flag for distinguishing if port 5 of the MT7531 switch
  *			has got SGMII
@@ -792,8 +783,6 @@ struct mt7530_priv {
 	const struct mt753x_info *info;
 	unsigned int		id;
 	bool			mcm;
-	phy_interface_t		p6_interface;
-	phy_interface_t		p5_interface;
 	enum p5_interface_select p5_intf_sel;
 	bool			p5_sgmii;
 	u8			mirror_rx;
