From f4cf4e5db331a5ce69e3f0b21d322cac0f4e4b5d Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Rafa=C5=82=20Mi=C5=82ecki?= <rafal@milecki.pl>
Date: Mon, 23 Oct 2023 12:27:59 +0200
Subject: [PATCH] Revert "nvmem: add new config option"
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This reverts commit 517f14d9cf3533d5ab4fded195ab6f80a92e378f.

Config option "no_of_node" is no longer needed since adding a more
explicit and targeted option "add_legacy_fixed_of_cells".

That "no_of_node" config option was needed *earlier* to help mtd's case.

DT nodes of MTD partitions (that are also NVMEM devices) may contain
subnodes. Those SHOULD NOT be treated as NVMEM fixed cells.

To prevent NVMEM core code from parsing subnodes a "no_of_node" option
was added (and set to true in mtd) to make for_each_child_of_node() in
NVMEM a no-op. That was a bit hacky because it was messing with
"of_node" pointer to achieve some side-effect.

With the introduction of "add_legacy_fixed_of_cells" config option
things got more explicit. MTD subsystem simply tells NVMEM when to look
for fixed cells and there is no need to hack "of_node" pointer anymore.

Signed-off-by: Rafał Miłecki <rafal@milecki.pl>
Reviewed-by: Miquel Raynal <miquel.raynal@bootlin.com>
Signed-off-by: Srinivas Kandagatla <srinivas.kandagatla@linaro.org>
Link: https://lore.kernel.org/r/20231023102759.31529-1-zajec5@gmail.com
Signed-off-by: Greg Kroah-Hartman <gregkh@linuxfoundation.org>
---
 drivers/mtd/mtdcore.c          | 1 -
 drivers/nvmem/core.c           | 2 +-
 include/linux/nvmem-provider.h | 2 --
 3 files changed, 1 insertion(+), 4 deletions(-)

--- a/drivers/mtd/mtdcore.c
+++ b/drivers/mtd/mtdcore.c
@@ -549,7 +549,6 @@ static int mtd_nvmem_add(struct mtd_info
 	config.read_only = true;
 	config.root_only = true;
 	config.ignore_wp = true;
-	config.no_of_node = !of_device_is_compatible(node, "nvmem-cells");
 	config.priv = mtd;
 
 	mtd->nvmem = nvmem_register(&config);
--- a/drivers/nvmem/core.c
+++ b/drivers/nvmem/core.c
@@ -936,7 +936,7 @@ struct nvmem_device *nvmem_register(cons
 	nvmem->nkeepout = config->nkeepout;
 	if (config->of_node)
 		nvmem->dev.of_node = config->of_node;
-	else if (!config->no_of_node)
+	else
 		nvmem->dev.of_node = config->dev->of_node;
 
 	switch (config->id) {
--- a/include/linux/nvmem-provider.h
+++ b/include/linux/nvmem-provider.h
@@ -89,7 +89,6 @@ struct nvmem_cell_info {
  * @read_only:	Device is read-only.
  * @root_only:	Device is accessibly to root only.
  * @of_node:	If given, this will be used instead of the parent's of_node.
- * @no_of_node:	Device should not use the parent's of_node even if it's !NULL.
  * @reg_read:	Callback to read data.
  * @reg_write:	Callback to write data.
  * @size:	Device size.
@@ -122,7 +121,6 @@ struct nvmem_config {
 	bool			ignore_wp;
 	struct nvmem_layout	*layout;
 	struct device_node	*of_node;
-	bool			no_of_node;
 	nvmem_reg_read_t	reg_read;
 	nvmem_reg_write_t	reg_write;
 	int	size;
