// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "qcom-ipq4019.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/soc/qcom,tcsr.h>
#include <dt-bindings/leds/common.h>

/ {
	model = "ASUS Lyra MAP-AC2200";
	compatible = "asus,map-ac2200";

	aliases {
		led-boot = &led_blue0;
		led-failsafe = &led_red0;
		led-running = &led_blue0;
		led-upgrade = &led_red0;
		ethernet1 = &swport4;
	};

	soc {
		rng@22000 {
			status = "okay";
		};

		mdio@90000 {
			status = "okay";
		};

		tcsr@1949000 {
			compatible = "qcom,tcsr";
			reg = <0x1949000 0x100>;
			qcom,wifi_glb_cfg = <TCSR_WIFI_GLB_CFG>;
		};

		ess_tcsr@1953000 {
			compatible = "qcom,tcsr";
			reg = <0x1953000 0x1000>;
			qcom,ess-interface-select = <TCSR_ESS_PSGMII>;
		};

		tcsr@1957000 {
			compatible = "qcom,tcsr";
			reg = <0x1957000 0x100>;
			qcom,wifi_noc_memtype_m0_m2 = <TCSR_WIFI_NOC_MEMTYPE_M0_M2>;
		};

		usb2@60f8800 {
			status = "okay";
		};

		crypto@8e3a000 {
			status = "okay";
		};

		watchdog@b017000 {
			status = "okay";
		};
	};

	keys {
		compatible = "gpio-keys";

		reset {
			label = "reset";
			gpios = <&tlmm 34 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&tlmm 18 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};
	};
};

&nand {
	pinctrl-0 = <&nand_pins>;
	pinctrl-names = "default";
	status = "okay";

	nand@0 {
		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "SBL1";
				reg = <0x0 0x80000>;
				read-only;
			};

			partition@80000 {
				label = "MIBIB";
				reg = <0x80000 0x80000>;
				read-only;
			};

			partition@100000 {
				label = "QSEE";
				reg = <0x100000 0x100000>;
				read-only;
			};

			partition@200000 {
				label = "CDT";
				reg = <0x200000 0x80000>;
				read-only;
			};

			partition@280000 {
				label = "APPSBL";
				reg = <0x280000 0x140000>;
				read-only;
			};

			partition@3c0000 {
				label = "APPSBLENV";
				reg = <0x3c0000 0x40000>;
				read-only;
			};

			partition@400000 {
				label = "ubi";
				reg = <0x400000 0x7c00000>;
			};
		};
	};
};

&tlmm {
	i2c_0_pins: i2c_0_pinmux {
		pinmux {
			function = "blsp_i2c0";
			pins = "gpio20", "gpio21";
			drive-strength = <16>;
			bias-disable;
		};
	};

	serial_pins: serial_pinmux {
		mux {
			pins = "gpio16", "gpio17";
			function = "blsp_uart0";
			bias-disable;
		};
	};

	nand_pins: nand_pins {
		pullups {
			pins =	"gpio52", "gpio53", "gpio58",
				"gpio59";
			function = "qpic";
			bias-pull-up;
		};

		pulldowns {
			pins =	"gpio54", "gpio55", "gpio56",
				"gpio57", "gpio60", "gpio61",
				"gpio62", "gpio63", "gpio64",
				"gpio65", "gpio66", "gpio67",
				"gpio68", "gpio69";
			function = "qpic";
			bias-pull-down;
		};
	};
	enable_ext_pa_high {
		gpio-hog;
		gpios = <44 GPIO_ACTIVE_HIGH>,
			<46 GPIO_ACTIVE_HIGH>;
		output-high;
		bias-pull-down;
		line-name = "enable external PA output-high";
	};
	enable_ext_pa_low {
		gpio-hog;
		gpios = <45 GPIO_ACTIVE_HIGH>,
			<47 GPIO_ACTIVE_HIGH>;
		output-low;
		bias-pull-down;
		line-name = "enable external PA output-low";
	};
};

&cryptobam {
	status = "okay";
};

&blsp_dma {
	status = "okay";
};

&qpic_bam {
	status = "okay";
};

&wifi0 {
	status = "okay";
	qcom,ath10k-calibration-variant = "ASUS-MAP-AC2200";
};

&wifi1 {
	status = "okay";
	qcom,ath10k-calibration-variant = "ASUS-MAP-AC2200";
	ieee80211-freq-limit = <5470000 5875000>;
};

&pcie0 {
	status = "okay";
	perst-gpio = <&tlmm 38 GPIO_ACTIVE_LOW>;
	wake-gpio = <&tlmm 50 GPIO_ACTIVE_LOW>;

	bridge@0,0 {
		reg = <0x00000000 0 0 0 0>;
		#address-cells = <3>;
		#size-cells = <2>;
		ranges;

		wifi2: wifi@1,0 {
			compatible = "qcom,ath10k";
			status = "okay";
			reg = <0x00010000 0 0 0 0>;
			qcom,ath10k-calibration-variant = "ASUS-MAP-AC2200";
			ieee80211-freq-limit = <5170000 5350000>;
		};
	};
};

&usb2_hs_phy {
	/* Bluetooth module attached via USB */
	status = "okay";
};

&blsp1_i2c3 {
	pinctrl-0 = <&i2c_0_pins>;
	pinctrl-names = "default";
	status = "okay";

	led-controller@32 {
		/* 9-channel RGB LED controller */
		compatible = "national,lp5523";
		reg = <0x32>;
		clock-mode = /bits/ 8 <1>;
		#address-cells = <1>;
		#size-cells = <0>;

		/*
		 * There is only one single extremely bright RGB-LED.
		 * The RGB-color channels are running in parallel to
		 * increase the current delivery capabilities beyond
		 * what a single PWM-output of the controller can do.
		 */

		led_blue0: led@0 {
			chan-name = "blue-0";
			led-cur = /bits/ 8 <0xfa>;
			max-cur = /bits/ 8 <0xff>;
			reg = <0>;
			color = <LED_COLOR_ID_BLUE>;
			function-enumerator = <0>;
		};

		led@1 {
			chan-name = "blue-1";
			led-cur = /bits/ 8 <0xfa>;
			max-cur = /bits/ 8 <0xff>;
			reg = <1>;
			color = <LED_COLOR_ID_BLUE>;
			function-enumerator = <1>;
		};

		led@2 {
			chan-name = "blue-2";
			led-cur = /bits/ 8 <0xfa>;
			max-cur = /bits/ 8 <0xff>;
			reg = <2>;
			color = <LED_COLOR_ID_BLUE>;
			function-enumerator = <2>;
		};

		led_green0: led@3 {
			chan-name = "green-0";
			led-cur = /bits/ 8 <0xfa>;
			max-cur = /bits/ 8 <0xff>;
			reg = <3>;
			color = <LED_COLOR_ID_GREEN>;
			function-enumerator = <0>;
		};

		led@4 {
			chan-name = "green-1";
			led-cur = /bits/ 8 <0xfa>;
			max-cur = /bits/ 8 <0xff>;
			reg = <4>;
			color = <LED_COLOR_ID_GREEN>;
			function-enumerator = <1>;
		};

		led@5 {
			chan-name = "green-2";
			led-cur = /bits/ 8 <0xfa>;
			max-cur = /bits/ 8 <0xff>;
			reg = <5>;
			color = <LED_COLOR_ID_GREEN>;
			function-enumerator = <2>;
		};

		led_red0: led@6 {
			chan-name = "red-0";
			led-cur = /bits/ 8 <0xfa>;
			max-cur = /bits/ 8 <0xff>;
			reg = <6>;
			color = <LED_COLOR_ID_RED>;
			function-enumerator = <0>;
		};

		led@7 {
			chan-name = "red-1";
			led-cur = /bits/ 8 <0xfa>;
			max-cur = /bits/ 8 <0xff>;
			reg = <7>;
			color = <LED_COLOR_ID_RED>;
			function-enumerator = <1>;
		};

		led@8 {
			chan-name = "red-2";
			led-cur = /bits/ 8 <0xfa>;
			max-cur = /bits/ 8 <0xff>;
			reg = <8>;
			color = <LED_COLOR_ID_RED>;
			function-enumerator = <2>;
		};
	};
};

&blsp1_uart1 {
	pinctrl-0 = <&serial_pins>;
	pinctrl-names = "default";
	status = "okay";
};

&gmac {
	status = "okay";
};

&switch {
	status = "okay";
};

&swport4 {
	status = "okay";

	label = "wan";
};

&swport5 {
	status = "okay";

	label = "lan";
};
