// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "mt7621.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	aliases {
		led-boot = &led_status_red;
		led-failsafe = &led_status_red;
		led-running = &led_status_green;
		led-upgrade = &led_status_red;
	};

	leds {
		compatible = "gpio-leds";

		led_status_green: led-0 {
			color = <LED_COLOR_ID_GREEN>;
			function = LED_FUNCTION_STATUS;
			gpios = <&gpio 15 GPIO_ACTIVE_LOW>;
		};

		led_status_red: led-1 {
			color = <LED_COLOR_ID_RED>;
			function = LED_FUNCTION_STATUS;
			gpios = <&gpio 16 GPIO_ACTIVE_LOW>;
		};
	};

	keys {
		compatible = "gpio-keys";

		button-0 {
			label = "reset";
			gpios = <&gpio 3 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	ubi-concat {
		compatible = "mtd-concat";
		devices = <&ubiconcat0 &ubiconcat1>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "ubi";
				reg = <0x0 0x5240000>;
			};
		};
	};
};

&nand {
	status = "okay";

	partitions {
		compatible = "fixed-partitions";
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "u-boot";
			reg = <0x0 0x100000>;
			read-only;
		};

		partition@100000 {
			label = "u-boot-env";
			reg = <0x100000 0x100000>;
		};

		partition@200000 {
			label = "Factory";
			reg = <0x200000 0x100000>;
			read-only;

			nvmem-layout {
				compatible = "fixed-layout";
				#address-cells = <1>;
				#size-cells = <1>;

				eeprom_factory_0: eeprom@0 {
					reg = <0x0 0x4da8>;
				};

				/* We keep the block below to prevent eth0 MAC
				 * from randomization. Unique WAN, LAN, WLAN MACs
				 * are stored in u-boot-env.
				 */

				/* Default Ralink MAC (00:0c:43:28:80:xx) */
				macaddr_factory_fff0: macaddr@fff0 {
					reg = <0xfff0 0x6>;
				};
			};
		};

		partition@300000 {
			label = "firmware";
			reg = <0x300000 0x2000000>;

			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "kernel";
				reg = <0x0 0x440000>;
			};

			ubiconcat0: partition@400000 {
				label = "ubiconcat0";
				reg = <0x440000 0x1bc0000>;
			};
		};

		partition@2300000 {
			label = "Firmware2";
			reg = <0x2300000 0x2000000>;
			read-only;
		};

		partition@4300000 {
			label = "glbcfg";
			reg = <0x4300000 0x200000>;
			read-only;
		};

		partition@4500000 {
			label = "board_data";
			reg = <0x4500000 0x100000>;
			read-only;
		};

		partition@4600000 {
			label = "glbcfg2";
			reg = <0x4600000 0x200000>;
			read-only;
		};

		partition@4800000 {
			label = "board_data2";
			reg = <0x4800000 0x100000>;
			read-only;
		};

		ubiconcat1: partition@4900000 {
			label = "ubiconcat1";
			reg = <0x4900000 0x3680000>;
		};
	};
};

&pcie {
	status = "okay";
};

&pcie1 {
	wifi@0,0 {
		compatible = "mediatek,mt76";
		reg = <0x0000 0 0 0 0>;
		nvmem-cells = <&eeprom_factory_0>;
		nvmem-cell-names = "eeprom";
	};
};

&gmac0 {
	nvmem-cells = <&macaddr_factory_fff0>;
	nvmem-cell-names = "mac-address";
};

&gmac1 {
	status = "okay";
	label = "wan";
	phy-handle = <&ethphy4>;

	nvmem-cells = <&macaddr_factory_fff0>;
	nvmem-cell-names = "mac-address";
};

&mdio {
	ethphy4: ethernet-phy@4 {
		reg = <4>;
	};
};

&switch0 {
	ports {
		port@2 {
			status = "okay";
			label = "lan2";
		};

		port@3 {
			status = "okay";
			label = "lan1";
		};
	};
};

&state_default {
	gpio {
		groups = "i2c", "jtag";
		function = "gpio";
	};
};
