From 767d43808d7fdf21896de50b38216d8884ca9f35 Mon Sep 17 00:00:00 2001
From: Dave Stevenson <dave.stevenson@raspberrypi.org>
Date: Mon, 18 Feb 2019 15:52:29 +0000
Subject: [PATCH] staging: mmal-vchiq: Update mmal_parameters.h with
 recently defined params

mmal_parameters.h hasn't been updated to reflect additions made
over the last few years. Update it to reflect the currently
supported parameters.

Signed-off-by: Dave Stevenson <dave.stevenson@raspberrypi.org>
---
 .../vchiq-mmal/mmal-parameters.h              | 32 ++++++++++++++++++-
 1 file changed, 31 insertions(+), 1 deletion(-)

--- a/drivers/staging/vc04_services/vchiq-mmal/mmal-parameters.h
+++ b/drivers/staging/vc04_services/vchiq-mmal/mmal-parameters.h
@@ -577,7 +577,37 @@ enum mmal_parameter_video_type {
 	MMAL_PARAMETER_VIDEO_ENCODE_H264_LOW_DELAY_HRD_FLAG,
 
 	/**< @ref MMAL_PARAMETER_BOOLEAN_T */
-	MMAL_PARAMETER_VIDEO_ENCODE_INLINE_HEADER
+	MMAL_PARAMETER_VIDEO_ENCODE_INLINE_HEADER,
+
+	/**< Take a @ref MMAL_PARAMETER_BOOLEAN_T. */
+	MMAL_PARAMETER_VIDEO_ENCODE_SEI_ENABLE,
+
+	/**< Take a @ref MMAL_PARAMETER_BOOLEAN_T. */
+	MMAL_PARAMETER_VIDEO_ENCODE_INLINE_VECTORS,
+
+	/**< Take a @ref MMAL_PARAMETER_VIDEO_RENDER_STATS_T. */
+	MMAL_PARAMETER_VIDEO_RENDER_STATS,
+
+	/**< Take a @ref MMAL_PARAMETER_VIDEO_INTERLACE_TYPE_T. */
+	MMAL_PARAMETER_VIDEO_INTERLACE_TYPE,
+
+	/**< Takes a @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_VIDEO_INTERPOLATE_TIMESTAMPS,
+
+	/**< Takes a @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_VIDEO_ENCODE_SPS_TIMING,
+
+	/**< Takes a @ref MMAL_PARAMETER_UINT32_T */
+	MMAL_PARAMETER_VIDEO_MAX_NUM_CALLBACKS,
+
+	/**< Takes a @ref MMAL_PARAMETER_SOURCE_PATTERN_T */
+	MMAL_PARAMETER_VIDEO_SOURCE_PATTERN,
+
+	/**< Takes a @ref MMAL_PARAMETER_BOOLEAN_T */
+	MMAL_PARAMETER_VIDEO_ENCODE_SEPARATE_NAL_BUFS,
+
+	/**< Takes a @ref MMAL_PARAMETER_UINT32_T */
+	MMAL_PARAMETER_VIDEO_DROPPABLE_PFRAME_LENGTH,
 };
 
 /** Valid mirror modes */
