# SPDX-License-Identifier: GPL-2.0-only
. /lib/functions/uci-defaults.sh

board_config_update

case "$(board_name)" in
gateworks,gw2348|\
gateworks,gw2358)
	ucidef_set_interfaces_lan_wan "eth0" "eth1"
	;;
linksys,nslu2)
	ucidef_set_interface_lan "eth0" "dhcp"
	;;
usr,usr8200)
	# LAN ports connected to eth1 thru the MV88E6060 DSA switch
	ucidef_set_interface "eth" device "eth1" protocol "none"
	ucidef_set_interfaces_lan_wan "lan1 lan2 lan3 lan4" "eth0"
	;;
*)
	ucidef_set_interface_lan "eth0" "dhcp"
	;;
esac

board_config_flush

exit 0
