From afd5f659b0453e4c710ce5cf74c577563ff16239 Mon Sep 17 00:00:00 2001
From: Andrew Scheller <andrew.scheller@raspberrypi.com>
Date: Tue, 20 Feb 2024 17:53:03 +0000
Subject: [PATCH 1281/1295] Add IQaudio CodecZero to hat_map.dts

Fixes https://github.com/raspberrypi/Pi-Codec/issues/9
---
 arch/arm/boot/dts/overlays/hat_map.dts | 5 +++++
 1 file changed, 5 insertions(+)

--- a/arch/arm/boot/dts/overlays/hat_map.dts
+++ b/arch/arm/boot/dts/overlays/hat_map.dts
@@ -6,6 +6,11 @@
 		overlay = "iqaudio-codec";
 	};
 
+	iqaudio-pi-codeczero {
+		uuid = [ e15c739c 877d 4e29 ab36 4dc73c21127c ];
+		overlay = "iqaudio-codec";
+	};
+
 	pisound {
 		uuid = [ a7ee5d28 da03 41f5 bbd7 20438a4bec5d ];
 		overlay = "pisound";
