From e5c266a61186b462c388c53a3564c375e72f2244 Mon Sep 17 00:00:00 2001
From: Hayes Wang <hayeswang@realtek.com>
Date: Wed, 26 Jul 2023 11:08:08 +0800
Subject: [PATCH] r8152: set bp in bulk

PLA_BP_0 ~ PLA_BP_15 (0xfc28 ~ 0xfc46) are continuous registers, so we
could combine the control transfers into one control transfer.

Signed-off-by: Hayes Wang <hayeswang@realtek.com>
Link: https://lore.kernel.org/r/20230726030808.9093-419-nic_swsd@realtek.com
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/usb/r8152.c | 75 ++++++++++++++---------------------------
 1 file changed, 25 insertions(+), 50 deletions(-)

--- a/drivers/net/usb/r8152.c
+++ b/drivers/net/usb/r8152.c
@@ -3983,29 +3983,10 @@ static void rtl_reset_bmu(struct r8152 *
 /* Clear the bp to stop the firmware before loading a new one */
 static void rtl_clear_bp(struct r8152 *tp, u16 type)
 {
-	switch (tp->version) {
-	case RTL_VER_01:
-	case RTL_VER_02:
-	case RTL_VER_07:
-		break;
-	case RTL_VER_03:
-	case RTL_VER_04:
-	case RTL_VER_05:
-	case RTL_VER_06:
-		ocp_write_byte(tp, type, PLA_BP_EN, 0);
-		break;
-	case RTL_VER_14:
-		ocp_write_word(tp, type, USB_BP2_EN, 0);
+	u16 bp[16] = {0};
+	u16 bp_num;
 
-		ocp_write_word(tp, type, USB_BP_8, 0);
-		ocp_write_word(tp, type, USB_BP_9, 0);
-		ocp_write_word(tp, type, USB_BP_10, 0);
-		ocp_write_word(tp, type, USB_BP_11, 0);
-		ocp_write_word(tp, type, USB_BP_12, 0);
-		ocp_write_word(tp, type, USB_BP_13, 0);
-		ocp_write_word(tp, type, USB_BP_14, 0);
-		ocp_write_word(tp, type, USB_BP_15, 0);
-		break;
+	switch (tp->version) {
 	case RTL_VER_08:
 	case RTL_VER_09:
 	case RTL_VER_10:
@@ -4013,32 +3994,31 @@ static void rtl_clear_bp(struct r8152 *t
 	case RTL_VER_12:
 	case RTL_VER_13:
 	case RTL_VER_15:
-	default:
 		if (type == MCU_TYPE_USB) {
 			ocp_write_word(tp, MCU_TYPE_USB, USB_BP2_EN, 0);
-
-			ocp_write_word(tp, MCU_TYPE_USB, USB_BP_8, 0);
-			ocp_write_word(tp, MCU_TYPE_USB, USB_BP_9, 0);
-			ocp_write_word(tp, MCU_TYPE_USB, USB_BP_10, 0);
-			ocp_write_word(tp, MCU_TYPE_USB, USB_BP_11, 0);
-			ocp_write_word(tp, MCU_TYPE_USB, USB_BP_12, 0);
-			ocp_write_word(tp, MCU_TYPE_USB, USB_BP_13, 0);
-			ocp_write_word(tp, MCU_TYPE_USB, USB_BP_14, 0);
-			ocp_write_word(tp, MCU_TYPE_USB, USB_BP_15, 0);
-		} else {
-			ocp_write_byte(tp, MCU_TYPE_PLA, PLA_BP_EN, 0);
+			bp_num = 16;
+			break;
 		}
+		fallthrough;
+	case RTL_VER_03:
+	case RTL_VER_04:
+	case RTL_VER_05:
+	case RTL_VER_06:
+		ocp_write_byte(tp, type, PLA_BP_EN, 0);
+		fallthrough;
+	case RTL_VER_01:
+	case RTL_VER_02:
+	case RTL_VER_07:
+		bp_num = 8;
+		break;
+	case RTL_VER_14:
+	default:
+		ocp_write_word(tp, type, USB_BP2_EN, 0);
+		bp_num = 16;
 		break;
 	}
 
-	ocp_write_word(tp, type, PLA_BP_0, 0);
-	ocp_write_word(tp, type, PLA_BP_1, 0);
-	ocp_write_word(tp, type, PLA_BP_2, 0);
-	ocp_write_word(tp, type, PLA_BP_3, 0);
-	ocp_write_word(tp, type, PLA_BP_4, 0);
-	ocp_write_word(tp, type, PLA_BP_5, 0);
-	ocp_write_word(tp, type, PLA_BP_6, 0);
-	ocp_write_word(tp, type, PLA_BP_7, 0);
+	generic_ocp_write(tp, PLA_BP_0, BYTE_EN_DWORD, bp_num << 1, bp, type);
 
 	/* wait 3 ms to make sure the firmware is stopped */
 	usleep_range(3000, 6000);
@@ -5015,10 +4995,9 @@ static void rtl8152_fw_phy_nc_apply(stru
 
 static void rtl8152_fw_mac_apply(struct r8152 *tp, struct fw_mac *mac)
 {
-	u16 bp_en_addr, bp_index, type, bp_num, fw_ver_reg;
+	u16 bp_en_addr, type, fw_ver_reg;
 	u32 length;
 	u8 *data;
-	int i;
 
 	switch (__le32_to_cpu(mac->blk_hdr.type)) {
 	case RTL_FW_PLA:
@@ -5060,12 +5039,8 @@ static void rtl8152_fw_mac_apply(struct
 	ocp_write_word(tp, type, __le16_to_cpu(mac->bp_ba_addr),
 		       __le16_to_cpu(mac->bp_ba_value));
 
-	bp_index = __le16_to_cpu(mac->bp_start);
-	bp_num = __le16_to_cpu(mac->bp_num);
-	for (i = 0; i < bp_num; i++) {
-		ocp_write_word(tp, type, bp_index, __le16_to_cpu(mac->bp[i]));
-		bp_index += 2;
-	}
+	generic_ocp_write(tp, __le16_to_cpu(mac->bp_start), BYTE_EN_DWORD,
+			  __le16_to_cpu(mac->bp_num) << 1, mac->bp, type);
 
 	bp_en_addr = __le16_to_cpu(mac->bp_en_addr);
 	if (bp_en_addr)
