From 8400889a0f241a12353673c35087bf6c38ea09e9 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime@cerno.tech>
Date: Mon, 15 Aug 2022 13:34:02 +0200
Subject: [PATCH] media: uapi: Add some RGB bus formats for VC4 DPI
 output

The VC4 DPI controller can output more RGB formats that aren't described
through a media bus format yet, so let's add them.

Signed-off-by: Maxime Ripard <maxime@cerno.tech>
---
 include/uapi/linux/media-bus-format.h | 5 ++++-
 1 file changed, 4 insertions(+), 1 deletion(-)

--- a/include/uapi/linux/media-bus-format.h
+++ b/include/uapi/linux/media-bus-format.h
@@ -34,19 +34,22 @@
 
 #define MEDIA_BUS_FMT_FIXED			0x0001
 
-/* RGB - next is	0x1022 */
+/* RGB - next is	0x1025 */
 #define MEDIA_BUS_FMT_RGB444_1X12		0x1016
 #define MEDIA_BUS_FMT_RGB444_2X8_PADHI_BE	0x1001
 #define MEDIA_BUS_FMT_RGB444_2X8_PADHI_LE	0x1002
 #define MEDIA_BUS_FMT_RGB555_2X8_PADHI_BE	0x1003
 #define MEDIA_BUS_FMT_RGB555_2X8_PADHI_LE	0x1004
 #define MEDIA_BUS_FMT_RGB565_1X16		0x1017
+#define MEDIA_BUS_FMT_RGB565_1X24_CPADHI	0x1022
 #define MEDIA_BUS_FMT_BGR565_2X8_BE		0x1005
 #define MEDIA_BUS_FMT_BGR565_2X8_LE		0x1006
 #define MEDIA_BUS_FMT_RGB565_2X8_BE		0x1007
 #define MEDIA_BUS_FMT_RGB565_2X8_LE		0x1008
+#define MEDIA_BUS_FMT_BGR666_1X18		0x1023
 #define MEDIA_BUS_FMT_RGB666_1X18		0x1009
 #define MEDIA_BUS_FMT_RBG888_1X24		0x100e
+#define MEDIA_BUS_FMT_BGR666_1X24_CPADHI	0x1024
 #define MEDIA_BUS_FMT_RGB666_1X24_CPADHI	0x1015
 #define MEDIA_BUS_FMT_RGB666_1X7X3_SPWG		0x1010
 #define MEDIA_BUS_FMT_BGR888_1X24		0x1013
