From 92c8b9d558160d94b981dd8a2b9c47657627ffdc Mon Sep 17 00:00:00 2001
From: Daniel Golle <daniel@makrotopia.org>
Date: Sat, 22 Apr 2023 01:23:08 +0100
Subject: [PATCH 2/3] net: phy: realtek: use inline functions for 10GbE
 advertisement

Use existing generic inline functions to encode local advertisement
of 10GbE link modes as well as to decode link-partner advertisement.

Signed-off-by: Daniel Golle <daniel@makrotopia.org>
---
 drivers/net/phy/realtek.c | 22 +++++-----------------
 1 file changed, 5 insertions(+), 17 deletions(-)

--- a/drivers/net/phy/realtek.c
+++ b/drivers/net/phy/realtek.c
@@ -69,10 +69,6 @@
 #define RTL_SUPPORTS_5000FULL			BIT(14)
 #define RTL_SUPPORTS_2500FULL			BIT(13)
 #define RTL_SUPPORTS_10000FULL			BIT(0)
-#define RTL_ADV_2500FULL			BIT(7)
-#define RTL_LPADV_10000FULL			BIT(11)
-#define RTL_LPADV_5000FULL			BIT(6)
-#define RTL_LPADV_2500FULL			BIT(5)
 
 #define RTL9000A_GINMR				0x14
 #define RTL9000A_GINMR_LINK_STATUS		BIT(4)
@@ -699,14 +695,11 @@ static int rtl822x_config_aneg(struct ph
 	int ret = 0;
 
 	if (phydev->autoneg == AUTONEG_ENABLE) {
-		u16 adv2500 = 0;
-
-		if (linkmode_test_bit(ETHTOOL_LINK_MODE_2500baseT_Full_BIT,
-				      phydev->advertising))
-			adv2500 = RTL_ADV_2500FULL;
-
 		ret = phy_modify_paged_changed(phydev, 0xa5d, 0x12,
-					       RTL_ADV_2500FULL, adv2500);
+					       MDIO_AN_10GBT_CTRL_ADV10G |
+					       MDIO_AN_10GBT_CTRL_ADV5G |
+					       MDIO_AN_10GBT_CTRL_ADV2_5G,
+			linkmode_adv_to_mii_10gbt_adv_t(phydev->advertising));
 		if (ret < 0)
 			return ret;
 	}
@@ -743,12 +736,7 @@ static int rtl822x_read_status(struct ph
 		if (lpadv < 0)
 			return lpadv;
 
-		linkmode_mod_bit(ETHTOOL_LINK_MODE_10000baseT_Full_BIT,
-			phydev->lp_advertising, lpadv & RTL_LPADV_10000FULL);
-		linkmode_mod_bit(ETHTOOL_LINK_MODE_5000baseT_Full_BIT,
-			phydev->lp_advertising, lpadv & RTL_LPADV_5000FULL);
-		linkmode_mod_bit(ETHTOOL_LINK_MODE_2500baseT_Full_BIT,
-			phydev->lp_advertising, lpadv & RTL_LPADV_2500FULL);
+		mii_10gbt_stat_mod_linkmode_lpa_t(phydev->lp_advertising, lpadv);
 	}
 
 	ret = rtlgen_read_status(phydev);
