From 6decd1aad15f56b169217789630a0098b496de0e Mon Sep 17 00:00:00 2001
From: Ilya Lipnitskiy <ilya.lipnitskiy@gmail.com>
Date: Wed, 7 Apr 2021 13:07:38 -0700
Subject: [PATCH] MIPS: add support for buggy MT7621S core detection

Most MT7621 SoCs have 2 cores, which is detected and supported properly
by CPS.

Unfortunately, MT7621 SoC has a less common S variant with only one core.
On MT7621S, GCR_CONFIG still reports 2 cores, which leads to hangs when
starting SMP. CPULAUNCH registers can be used in that case to detect the
absence of the second core and override the GCR_CONFIG PCORES field.

Rework a long-standing OpenWrt patch to override the value of
mips_cps_numcores on single-core MT7621 systems.

Tested on a dual-core MT7621 device (Ubiquiti ER-X) and a single-core
MT7621 device (Netgear R6220).

Original 4.14 OpenWrt patch:
Link: https://git.openwrt.org/?p=openwrt/openwrt.git;a=commitdiff;h=4cdbc90a376dd0555201c1434a2081e055e9ceb7
Current 5.10 OpenWrt patch:
Link: https://git.openwrt.org/?p=openwrt/openwrt.git;a=blob;f=target/linux/ramips/patches-5.10/320-mt7621-core-detect-hack.patch;h=c63f0f4c1ec742e24d8480e80553863744b58f6a;hb=10267e17299806f9885d086147878f6c492cb904

Suggested-by: Felix Fietkau <nbd@nbd.name>
Signed-off-by: Ilya Lipnitskiy <ilya.lipnitskiy@gmail.com>
Signed-off-by: Thomas Bogendoerfer <tsbogend@alpha.franken.de>
---
 arch/mips/include/asm/mips-cps.h | 23 ++++++++++++++++++++++-
 1 file changed, 22 insertions(+), 1 deletion(-)

--- a/arch/mips/include/asm/mips-cps.h
+++ b/arch/mips/include/asm/mips-cps.h
@@ -11,6 +11,8 @@
 #include <linux/io.h>
 #include <linux/types.h>
 
+#include <asm/mips-boards/launch.h>
+
 extern unsigned long __cps_access_bad_size(void)
 	__compiletime_error("Bad size for CPS accessor");
 
@@ -162,12 +164,31 @@ static inline uint64_t mips_cps_cluster_
  */
 static inline unsigned int mips_cps_numcores(unsigned int cluster)
 {
+	unsigned int ncores;
+
 	if (!mips_cm_present())
 		return 0;
 
 	/* Add one before masking to handle 0xff indicating no cores */
-	return FIELD_GET(CM_GCR_CONFIG_PCORES,
+	ncores = FIELD_GET(CM_GCR_CONFIG_PCORES,
 			 mips_cps_cluster_config(cluster) + 1);
+
+	if (IS_ENABLED(CONFIG_SOC_MT7621)) {
+		struct cpulaunch *launch;
+
+		/*
+		 * Ralink MT7621S SoC is single core, but the GCR_CONFIG method
+		 * always reports 2 cores. Check the second core's LAUNCH_FREADY
+		 * flag to detect if the second core is missing. This method
+		 * only works before the core has been started.
+		 */
+		launch = (struct cpulaunch *)CKSEG0ADDR(CPULAUNCH);
+		launch += 2; /* MT7621 has 2 VPEs per core */
+		if (!(launch->flags & LAUNCH_FREADY))
+			ncores = 1;
+	}
+
+	return ncores;
 }
 
 /**
