From 19f291d8a65cd19e7595006c7872cd95aa6f9e93 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Alexis=20Lothor=C3=A9?= <alexis.lothore@bootlin.com>
Date: Fri, 4 Aug 2023 19:13:10 +0200
Subject: [PATCH 893/898] net: dsa: mv88e6xxx: pass directly chip structure to
 mv88e6xxx_phy_is_internal
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Since this function is a simple helper, we do not need to pass a full
dsa_switch structure, we can directly pass the mv88e6xxx_chip structure.
Doing so will allow to share this function with any other function
not manipulating dsa_switch structure but needing info about number of
internal phys

Signed-off-by: Alexis Lothoré <alexis.lothore@bootlin.com>
Reviewed-by: Russell King (Oracle) <rmk+kernel@armlinux.org.uk>
Reviewed-by: Florian Fainelli <f.fainelli@gmail.com>
Signed-off-by: Jakub Kicinski <kuba@kernel.org>
---
 drivers/net/dsa/mv88e6xxx/chip.c | 6 ++----
 1 file changed, 2 insertions(+), 4 deletions(-)

--- a/drivers/net/dsa/mv88e6xxx/chip.c
+++ b/drivers/net/dsa/mv88e6xxx/chip.c
@@ -459,10 +459,8 @@ restore_link:
 	return err;
 }
 
-static int mv88e6xxx_phy_is_internal(struct dsa_switch *ds, int port)
+static int mv88e6xxx_phy_is_internal(struct mv88e6xxx_chip *chip, int port)
 {
-	struct mv88e6xxx_chip *chip = ds->priv;
-
 	return port < chip->info->num_internal_phys;
 }
 
@@ -704,7 +702,7 @@ static void mv88e6xxx_mac_config(struct
 
 	mv88e6xxx_reg_lock(chip);
 
-	if (mode != MLO_AN_PHY || !mv88e6xxx_phy_is_internal(ds, port)) {
+	if (mode != MLO_AN_PHY || !mv88e6xxx_phy_is_internal(chip, port)) {
 		/* In inband mode, the link may come up at any time while the
 		 * link is not forced down. Force the link down while we
 		 * reconfigure the interface mode.
