From a22e1110a6ffcc2cf4b3b598f037879cbd0915d3 Mon Sep 17 00:00:00 2001
From: Emil Renner Berthing <kernel@esmil.dk>
Date: Wed, 31 Aug 2022 22:54:07 +0200
Subject: [PATCH 1005/1024] RISC-V: Mark StarFive JH7100 as having non-coherent
 DMAs

Signed-off-by: Emil Renner Berthing <kernel@esmil.dk>
---
 arch/riscv/boot/dts/starfive/jh7100.dtsi | 1 +
 1 file changed, 1 insertion(+)

--- a/arch/riscv/boot/dts/starfive/jh7100.dtsi
+++ b/arch/riscv/boot/dts/starfive/jh7100.dtsi
@@ -111,6 +111,7 @@
 	soc {
 		compatible = "simple-bus";
 		interrupt-parent = <&plic>;
+		dma-noncoherent;
 		#address-cells = <2>;
 		#size-cells = <2>;
 		ranges;
