// SPDX-License-Identifier: GPL-2.0-or-later OR MIT

#include "ar7241.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/leds/common.h>

/ {
	compatible = "tplink,tl-wr842n-v1", "qca,ar7241";
	model = "TP-Link TL-WR842N/ND v1";

	aliases {
		led-boot = &led_system;
		led-failsafe = &led_system;
		led-running = &led_system;
		led-upgrade = &led_system;
		label-mac-device = &ath9k;
	};

	keys {
		compatible = "gpio-keys";

		rfkill {
			label = "rfkill";
			linux,code = <KEY_RFKILL>;
			gpios = <&gpio 11 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};

		reset {
			label = "reset";
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led_system: system {
			label = "green:system";
			gpios = <&gpio 1 GPIO_ACTIVE_LOW>;
		};

		qss {
			label = "green:qss";
			gpios = <&gpio 0 GPIO_ACTIVE_LOW>;
		};

		led3g {
			label = "green:3g";
			gpios = <&gpio 8 GPIO_ACTIVE_LOW>;
			trigger-sources = <&hub_port>;
			linux,default-trigger = "usbport";
		};
	};

	ath9k-leds {
		compatible = "gpio-leds";

		wlan {
			function = LED_FUNCTION_WLAN;
			color = <LED_COLOR_ID_GREEN>;
			gpios = <&ath9k 0 GPIO_ACTIVE_LOW>;
			linux,default-trigger = "phy0tpt";
		};
	};

	gpio-export {
		compatible = "gpio-export";

		gpio_usb_power {
			gpio-export,name = "tp-link:power:usb";
			gpio-export,output = <1>;
			gpios = <&gpio 6 GPIO_ACTIVE_HIGH>;
		};
	};
};

&usb {
	status = "okay";
};

&usb_phy {
	status = "okay";
};

&spi {
	status = "okay";

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			uboot: partition@0 {
				reg = <0x0 0x20000>;
				label = "u-boot";
				read-only;

				nvmem-layout {
					compatible = "fixed-layout";
					#address-cells = <1>;
					#size-cells = <1>;

					macaddr_uboot_1fc00: macaddr@1fc00 {
						compatible = "mac-base";
						reg = <0x1fc00 0x6>;
						#nvmem-cell-cells = <1>;
					};
				};
			};

			partition@20000 {
				compatible = "tplink,firmware";
				reg = <0x20000 0x7d0000>;
				label = "firmware";
			};

			partition@7f0000 {
				reg = <0x7f0000 0x10000>;
				label = "art";
				read-only;
			};
		};
	};
};

&pcie {
	status = "okay";

	ath9k: wifi@0,0 {
		compatible = "pci168c,002e";
		reg = <0x0000 0 0 0 0>;
		#gpio-cells = <2>;
		gpio-controller;
		qca,no-eeprom;
		nvmem-cells = <&macaddr_uboot_1fc00 0>;
		nvmem-cell-names = "mac-address";
	};
};

&eth0 {
	status = "okay";

	nvmem-cells = <&macaddr_uboot_1fc00 (-1)>;
	nvmem-cell-names = "mac-address";
};

&eth1 {
	nvmem-cells = <&macaddr_uboot_1fc00 1>;
	nvmem-cell-names = "mac-address";
};
